|  |  |
| --- | --- |
| 3GPP TS 24.175 V18.0.0 (2024-04) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  Management Object (MO) for multi-device and multi-identity in the IP Multimedia Subsystem (IMS)  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  https://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 6

2 References 6

3 Definitions of terms, symbols and abbreviations 6

3.1 Terms 6

3.2 Symbols 6

3.3 Abbreviations 6

4 Multi-Device and Multi-Identity management object 7

5 Management object parameters 7

5.1 General 7

5.2 Node: /<X> 7

5.3 /<X>/MultiIdentity 8

5.4 /<X>/MultiIdentity/SharedIdentity 8

5.5 /<X>/MultiIdentity/SharedIdentity/<X> 8

5.6 /<X>/MultiIdentity/SharedIdentity/<X>/SharedId 8

5.7 /<X>/MultiIdentity/DelegatedIdentity 9

5.8 /<X>/MultiIdentity/DelegatedIdentity/<X> 9

5.9 /<X>/MultiIdentity/DelegatedIdentity/<X>/DelegatedId 9

5.10 /<X>/MultiDevice 9

5.11 /<X>/MultiDevice/CallLogUri 10

5.12 /*<X>*/SNPN\_Configuration 10

5.13 /*<X>*/SNPN\_Configuration/<X> 10

5.14 /*<X>*/SNPN\_Configuration/<X>/SNPN\_identifier 10

5.15 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/SharedIdentity 11

5.16 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ SharedIdentity/<X> 11

5.17 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ SharedIdentity/<X>/SharedId 11

5.18 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity 12

5.19 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity/<X> 12

5.20 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity/<X>/DelegatedId 12

5.21 /*<X>*/SNPN\_Configuration/<X>/MultiDevice 12

5.22 /*<X>*/SNPN\_Configuration/<X>/MultiDevice/CallLogUri 13

Annex A (informative) : DDF of MO for Multi-Device and Multi-Identity in IMS 14

Annex B (informative): Change history 24

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document defines the management object (MO) for Multi-Device and Multi-Identity in IMS.

The MO for Multi-Device (MuD) and Multi-Identity (MiD) in IMS is compatible with OMA device management protocol specifications, version 1.2 and upwards, and is defined using the OMA DM device description framework as described in the enabler release definition OMA-ERELD\_DM-V1\_2 [2].

The MO for Multi-Device and Multi-Identity in IMS consists of relevant configuration parameters that can be managed for a UE supporting the UE role specified in 3GPP TS 24.174 [3].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] OMA OMA-ERELD-DM-V1\_2-20070209-A: "Enabler Release Definition for OMA Device Management, Version 1.2".

[3] 3GPP TS 24.174: "Support of Multi-Device and Multi-Identity in IMS; Stage 3".

[4] OMA-TS-DM\_TND-V1\_3-20160524-A: "OMA Device Management Tree and Description".

[5] 3GPP TS 23.003: "Numbering, addressing and identification".

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

MiD Multi-iDentity

MO Management Object

MuD Multi-Device

SNPN Stand-alone Non-Public Network

# 4 Multi-Device and Multi-Identity management object

The MO for Multi-Device and Multi-Identity in IMS is used to manage settings of the UE for Multi-Device and Multi-Identity in IMS. Figure 4-1 gives an overview of the configuration parameters of this MO. The conventions used in this specification are as defined in OMA-TS-DM\_TND [4] with the following modifications:

- interior nodes are drawn as rectangles, not rectangles with rounded corners; and

- leaf nodes are plain text, not rectangles.

The MO for Multi-Device and Multi-Identity in IMS covers configuration parameters for a UE supporting Multi-Device and Multi-Identity in IMS specified in TS 24.174 [3].

The MO identifier is: urn:oma:mo:ext-3gpp-mudmid:1.0.

Figure 4-1: MO for Multi-Device and Multi-Identity in IMS

# 5 Management object parameters

## 5.1 General

This clause describes the configuration parameters for the MO for Multi-Device and Multi-Identity in IMS.

## 5.2 Node: /<X>

Table 5.2.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| /<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node acts as a placeholder for the MO for Multi-Device and Multi-Identity in IMS. | | | | |

The interior node is mandatory for a UE supporting the UE role specified in TS 24.174 [3].

NOTE: One node is normally used. More nodes are only used in case the terminal supports multiple UICCs.

Child nodes of this interior node which are not defined in this version of the present document are ignored.

- Values: N/A

## 5.3 /<X>/MultiIdentity

Table 5.3.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the multi-identity parameters. | | | | |

- Values: N/A

## 5.4 /<X>/MultiIdentity/SharedIdentity

Table 5.4.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/SharedIdentity | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the parameters of shared identities. | | | | |

- Values: N/A

## 5.5 /<X>/MultiIdentity/SharedIdentity/<X>

Table 5.5.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/SharedIdentity/<X> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the settings of shared identities. | | | | |

- Values: N/A

## 5.6 /<X>/MultiIdentity/SharedIdentity/<X>/SharedId

Table 5.6.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/SharedIdentity/<X>/SharedId | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node contains a shared identity the UE can use. | | | | |

- Values: N/A

## 5.7 /<X>/MultiIdentity/DelegatedIdentity

Table 5.7.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/DelegatedIdentity | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the multi-device parameters of delegated identities. | | | | |

- Values: N/A

## 5.8 /<X>/MultiIdentity/DelegatedIdentity/<X>

Table 5.8.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/DelegatedIdentity/<X> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the settings of delegated identities. | | | | |

- Values: N/A

## 5.9 /<X>/MultiIdentity/DelegatedIdentity/<X>/DelegatedId

Table 5.9.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiIdentity/DelegatedIdentity/<X>/DelegatedId | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node contains a delegated identity that is allowed to use the native identity. | | | | |

This leaf node contains a delegated identity that is allowed to use the native identity.

- Values: N/A

## 5.10 /<X>/MultiDevice

Table 5.10.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiDevice | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the multi-device parameters. | | | | |

- Values: N/A

## 5.11 /<X>/MultiDevice/CallLogUri

Table 5.11.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MultiDevice/CallLogUri | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get, Replace |  |
|  | This leaf node contains a URI the UE can use to access the call log. | | | | |

- Values: N/A

## 5.12 /*<X>*/SNPN\_Configuration

Table 5.12.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains configuration parameters regarding a UE operating in SNPN access operation mode. | | | | |

- Values: N/A

## 5.13 /*<X>*/SNPN\_Configuration/<X>

Table 5.13.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node contains per SNPN configurations. | | | | |

This interior node acts as a placeholder for a list of:

a) SNPN identity; and

b) configuration parameters.

NOTE: For each of the elements in the list, a) must be present and at least one parameter of b) needs to appear.

A configuration parameter in an /<X>/SNPN\_Configuration/<X> node other than the SNPN\_identifier, is applicable when the UE selects an entry of "list of subscriber data" with the SNPN identity of the subscribed SNPN which is the same as the SNPN identity in the SNPN\_identifier leaf.

- Values: N/A

## 5.14 /*<X>*/SNPN\_Configuration/<X>/SNPN\_identifier

Table 5.14.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/SNPN\_identifier | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf indicates the SNPN identity of the subscribed SNPN for which the list of configuration parameters are applicable. | | | | |

- Values: <PLMN><NID>

The PLMN and NID are in the format defined by 3GPP TS 23.003 [5], with each digit of the MCC and MNC of the PLMN and each digit of the assignment mode and NID value of the NID encoded as an ASCII character.

## 5.15 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/SharedIdentity

Table 5.15.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/SharedIdentity | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the parameters of shared identities. | | | | |

- Values: N/A

## 5.16 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ SharedIdentity/<X>

Table 5.16.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/SharedIdentity/<X> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the settings of shared identities. | | | | |

- Values: N/A

## 5.17 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ SharedIdentity/<X>/SharedId

Table 5.17.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/SharedIdentity/<X>/SharedId | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node contains a shared identity the UE can use. | | | | |

- Values: N/A

## 5.18 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity

Table 5.18.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/DelegatedIdentity | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the multi-device parameters of delegated identities. | | | | |

- Values: N/A

## 5.19 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity/<X>

Table 5.19.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/DelegatedIdentity/<X> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the settings of delegated identities. | | | | |

- Values: N/A

## 5.20 /*<X>*/SNPN\_Configuration/<X>/MultiIdentity/ DelegatedIdentity/<X>/DelegatedId

Table 5.20.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiIdentity/DelegatedIdentity/<X>/DelegatedId | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node contains a delegated identity that is allowed to use the native identity. | | | | |

This leaf node contains a delegated identity that is allowed to use the native identity.

- Values: N/A

## 5.21 /*<X>*/SNPN\_Configuration/<X>/MultiDevice

Table 5.21.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiDevice | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the multi-device parameters. | | | | |

- Values: N/A

## 5.22 /*<X>*/SNPN\_Configuration/<X>/MultiDevice/CallLogUri

Table 5.22.1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SNPN\_Configuration/<X>/MultiDevice/CallLogUri | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get, Replace |  |
|  | This leaf node contains a URI the UE can use to access the call log. | | | | |

- Values: N/A

Annex A (informative) :  
DDF of MO for Multi-Device and Multi-Identity in IMS

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version.

<?xml version="1.0" encoding="UTF-8"?>

<!DOCTYPE MgmtTree PUBLIC "-//OMA//DTD-DM-DDF 1.2//EN"

"http://www.openmobilealliance.org/tech/DTD/DM\_DDF-V1\_2.dtd">

<MgmtTree>

<VerDTD>1.2</VerDTD>

<Man>--The device manufacturer--</Man>

<Mod>--The device model--</Mod>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>The Management Object (MO) for Multi-Device and Multi-Identity in IMS.</DFTitle>

<DFType>

<DDFName>urn:oma:mo:ext-3gpp-mudmid:1.0</DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>MultiIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-identity parameters</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>SharedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of shared identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of shared identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>SharedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a shared identity the UE can use</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>DelegatedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of delegated identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of delegated identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>DelegatedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains the delegated identity allowed to use the native identity</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>MultiDevice</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-device parameters</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>CallLogUri</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a URI the UE can use to access the call log</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

<Node>

<NodeName>SNPN\_Configuration</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>SNPN Configuration.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>SNPN configuration parameters.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

<Node>

<NodeName>SNPN\_identifier</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Identifier of the SNPN.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>MultiIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-identity parameters</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>SharedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of shared identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of shared identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>SharedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a shared identity the UE can use</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>DelegatedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of delegated identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of delegated identities</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>DelegatedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains the delegated identity allowed to use the native identity</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>MultiDevice</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-device parameters</DFTitle>

<DFType><DDFName/></DFType>

</DFProperties>

<Node>

<NodeName>CallLogUri</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a URI the UE can use to access the call log</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>SNPN\_Configuration</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>SNPN Configuration.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>SNPN configuration parameters.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

<Node>

<NodeName>SNPN\_identifier</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Identifier of the SNPN.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>MultiIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-identity parameters</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName>SharedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of shared identities</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of shared identities</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName>SharedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a shared identity the UE can use</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>DelegatedIdentity</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing parameters of delegated identities</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrMore/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This interior node contains the settings of delegated identities</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName>DelegatedId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains the delegated identity allowed to use the native identity</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>MultiDevice</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>Interior node containing multi-device parameters</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName>CallLogUri</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Dynamic/>

</Scope>

<DFTitle>This leaf node contains a URI the UE can use to access the call log</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

</Node>

</MgmtTree>

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2019-11 | CT1#121 | C1-198315, C1-198317, C1-198318, C1-198833, C1-198834 |  |  |  | First version of this specification | 0.0.0 |
| 2019-12 | CT#86 | CP-193163 |  |  |  | Presentation for information to TSG CT | 1.0.0 |
| 2019-12 | CT#86 | CP-193293 |  |  |  | A TS number added | 1.0.1 |
| 2020-03 | CT1#122E | C1-201030 |  |  |  | Sent for approval to TSG CT | 1.1.0 |
| 2020-03 | CT-87e | CP-200164 |  |  |  | Presentation for approval to TSG CT | 2.0.0 |
| 2020-03 | CT-87e |  |  |  |  | Version 16.0.0 created after approval | 16.0.0 |
| 2022-03 | CT-95e | CP-220275 | 0002 | - | D | Reformatting 24.175 to align with OMA template | 17.0.0 |
| 2022-06 | CT-95e | CP-221249 | 0003 | 1 | B | SNPN configuration for multi-device | 17.1.0 |
| 2024-04 | - | - | - | - | - | Update to Rel-18 version (MCC) | **18.0.0** |