|  |  |
| --- | --- |
| 3GPP TS 26.191 V18.0.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Services and System Aspects;  Speech codec speech processing functions;  Adaptive Multi-Rate - Wideband (AMR-WB) speech codec; Error concealment of erroneous or lost frames  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 5

2 Normative references 5

3 Definitions and abbreviations 5

3.1 Definitions 5

3.2 Abbreviations 5

4 General 6

5 Requirements 6

5.1 Error detection 6

5.2 Erroneous or lost speech frames 6

5.3 First lost SID frame 6

5.4 Subsequent lost SID frames 6

6 Example ECU/BFH Solution 6

6.1 State Machine 6

6.2 Substitution and muting of erroneous/lost speech frames 8

6.2.1 BFI = 0, prevBFI = 0, State = 0 or 1 8

6.2.2 BFI = 0, prevBFI = 1, State = 0 to3 9

6.2.3 BFI = 1, prevBFI = 0 or 1, State = 1...6 9

6.2.3.1 LTP gain & fixed codebook gain concealment when RX\_FRAMETYPE = SPEECH\_BAD 9

6.2.3.2 LTP gain & fixed codebook gain concealment when RX\_FRAMETYPE = SPEECH\_LOST 10

6.2.3.3 ISF concealment 10

6.2.3.4 LTP-lag concealment 11

6.2.3.4.1 LTP-lag concealment when RX\_FRAMETYPE = SPEECH\_BAD 11

6.2.3.4.2 LTP-lag concealment when RX\_FRAMETYPE = SPEECH\_LOST 12

6.2.4 Innovation sequence 12

6.2.5 High-band gain (for 23.85 kbit/s mode) 12

6.3 Substitution and muting of lost SID frames 13

Annex A (informative): Change history 14

# Foreword

This Technical Specification has been produced by the 3GPP.

The present document defines an error concealment procedure, also termed frame substitution and muting procedure, of the wideband telephony speech service employing the Adaptive Multi-Rate – Wideband (AMR-WB) speech coder within the 3GPP system.

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of this TS, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 Indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the specification;

# 1 Scope

This specification defines an error concealment procedure, also termed frame substitution and muting procedure, which shall be used by the AMR-WB speech codec receiving end when one or more erroneous/lost speech or lost Silence Descriptor (SID) frames are received.

The requirements of this document are mandatory for implementation in all networks and User Equipment (UE)s capable of supporting the AMR-WB speech codec. It is not mandatory to follow the bit exact implementation outlined in this document and the corresponding C source code.

# 2 Normative references

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 26.202"AMR Wideband Speech Codec; Interface to RAN".

[2] 3GPP TS 26.190"AMR Wideband Speech Codec; Transcoding functions".

[3] 3GPP TS 26.193"AMR Wideband Speech Codec; Source Controlled Rate operation".

[4] 3GPP TS 26.201"AMR Wideband Speech Codec; Frame structure".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of this document, the following definition applies:

**N-point median operation:** Consists of sorting the N elements belonging to the set for which the median operation is to be performed in an ascending order according to their values, and selecting the (int (N/2) + 1) -th largest value of the sorted set as the median value.

Further definitions of terms used in this document can be found in the references.

## 3.2 Abbreviations

For the purposes of this document, the following abbreviations apply:

AMR-WB Adaptive Multi Rate - WideBand

AN Access Network

BFI Bad Frame Indication from AN

BSI\_netw Bad Sub-block Indication obtained from AN interface CRC checks

prevBFI Bad Frame Indication of previous frame

RX Receive

SCR Source Controlled Rate (operation)

SID Silence Descriptor frame (Background noise)

CRC Cyclic Redundancy Check

ECU Error Concealment Unit

BFH Bad Frame Handling

medianN N-point median operation

# 4 General

The purpose of the error concealment procedure is to conceal the effect of erroneous/lost AMR-WB speech frames. The purpose of muting the output in the case of several erroneous/lost frames is to indicate the breakdown of the channel to the user and to avoid generating possible annoying sounds as a result from the error concealment procedure.

The network shall indicate erroneous/lost speech or lost SID frames by setting the RX\_TYPE values [3] to SPEECH\_BAD, SID\_BAD or SPEECH\_LOST. If these flags are set, the speech decoder shall perform parameter substitution to conceal errors.

The example solution provided in paragraph 6 apply only to bad frame handling on a complete speech frame basis. Sub-frame based error concealment may be derived using similar methods.

# 5 Requirements

## 5.1 Error detection

If the most sensitive bits of the AMR-WB speech data (class A in [4]) are received in error, the network shall indicate RX\_TYPE = SPEECH\_BAD in which case the BFI flag is set. When the frame is not received, the network shall indicate RX\_TYPE = RX\_SPEECH\_LOST in which case the BFI flag is set as well. If a SID frame is received in error, the network shall indicate RX\_TYPE = SID\_BAD..

## 5.2 Erroneous or lost speech frames

Normal decoding of erroneous/lost speech frames would result in very unpleasant noise effects. In order to improve the subjective quality, erroneous/lost speech frames shall be substituted with either a repetition or an extrapolation of the previous good speech frame(s). This substitution is done so that it gradually will decrease the output level, resulting in silence at the output. Subclause 6 provides example solution.

## 5.3 First lost SID frame

A lost SID frame shall be substituted by using the SID information from earlier received valid SID frames and the procedure for valid SID frames be applied as described in [3].

## 5.4 Subsequent lost SID frames

For many subsequent lost SID frames, a muting technique shall be applied to the comfort noise that will gradually decrease the output level. For subsequent lost SID frames, the muting of the output shall be maintained. Subclause 6 provides example solutions.

# 6 Example ECU/BFH Solution

## 6.1 State Machine

This example solution for substitution and muting is based on a state machine with seven states (Figure 1).

The system starts in state 0. Each time a bad frame is detected, the state counter is incremented by one and is saturated when it reaches 6. Each time a good speech frame is detected, the state counter is right-shifted by one. The state indicates the quality of the channel: the larger the value of the state counter, the worse the channel quality is. The control flow of the state machine can be described by the following C code (**BFI** = bad frame indicator, **State** = state variable):

**if(BFI != 0 )**

**State = State + 1;**

**if(State > 6)**

**State = 6;**

**else**

**State = State >> 1;**

In addition to this state machine, the **Bad Frame Flag** from the previous frame is checked (**prevBFI**). The processing depends on the value of the **State**-variable. In states 0 and 6, the processing depends on the **BFI** flag.

The procedure can be described as follows:



Figure 1: State machine for controlling the bad frame substitution

## 6.2 Substitution and muting of erroneous/lost speech frames

### 6.2.1 BFI = 0, prevBFI = 0, State = 0 or 1

No error is detected in the received or in the previous received speech frame. The received speech parameters are used normally in the speech synthesis. The current frame of speech parameters is saved.

### 6.2.2 BFI = 0, prevBFI = 1, State = 0 to3

No error is detected in the received speech frame but the previous received speech frame was bad. The LTP gain is used normally in the speech synthesis and fixed codebook gain are limited below the values used for the last received good subframe:

 (1)

where

 = current decoded fixed codebook-gain  
  = fixed codebook gain used for the last good subframe (BFI = 0)  
  = fixed codebook gain to be used for the current frame.

The rest of the received speech parameters are used normally in the speech synthesis. The current frame of speech parameters is saved.

### 6.2.3 BFI = 1, prevBFI = 0 or 1, State = 1...6

An error is detected in the received speech frame and the substitution and muting procedure is started.

#### 6.2.3.1 LTP gain & fixed codebook gain concealment when RX\_FRAMETYPE = SPEECH\_BAD

The LTP gain  and fixed codebook gain  are replaced by attenuated values from the previous subframes:

 (2)

 (3)

where:

= current decoded LTP gain,   
 = current decoded fixed codebook gain,   
 = LTP gains used for the last 5 subframes,   
 = fixed codebook gains used for the last 5 subframes,  
 *median5()* = 5-point median operation,   
 = attenuation factor (*Pp(1)* = 0.98, *Pp (2)* = 0.96, *Pp (3)* = 0.75, *Pp (4)* = 0.23, *Pp (5)* = 0.05,  
 *Pp(6)* = 0.01),  
 = attenuation factor (*Pc (1)* = 0.98, *Pc (2)* = 0.98, *Pc (3)* = 0.98, *Pc (4)* = 0.98, *Pc (5)* = 0.98,  
 *Pc (6)* = 0.70),  
 *state* = state number {0..6},  
 VAD\_HIST is number of consecutive VAD=0 decisions.

The higher the state value is, the more the gains are attenuated. Also the memory of the predictive fixed codebook gain is updated by using the average value of the past four values in the memory:

 (4)

#### 6.2.3.2 LTP gain & fixed codebook gain concealment when RX\_FRAMETYPE = SPEECH\_LOST

The LTP gain  and fixed codebook gain  are replaced by attenuated values from the previous subframes:

 (5)

 (6)

where:

= current decoded LTP gain,   
 = current decoded fixed codebook gain,   
 = LTP gains used for the last 5 subframes,   
 = fixed codebook gains used for the last 5 subframes,  
 *median5()* = 5-point median operation,   
  = attenuation factor (*Pp(1)* = 0.95, *Pp (2)* = 0.90, *Pp (3 )* = 0.75, *Pp (4)* = 0.23, *Pp (5)* = 0.05,  
 *Pp (6)* = 0.01),   
  = attenuation factor (*Pc (1)* = 0.50, *Pc (2) =* 0.25, *Pc (3)* = 0.25, *Pc (4)* = 0.25, *Pc (5)* = 0.15,  
 *Pc (6)* = 0.01),   
 *state* = state number {0..6},  
 VAD\_HIST is number of consecutive VAD=0 decisions.

The higher the state value is, the more the gains are attenuated. Also the memory of the predictive fixed codebook gain is updated by using the average value of the past four values in the memory:

 (7)

#### 6.2.3.3 ISF concealment

The past ISFs are shifted towards their partly adaptive mean:

 *i = 0..16* (8)

where

 = 0.9,   
  is ISF-vector for a current frame,   
  is ISF-vector from the previous frame,   
  vector is combination of adaptive mean and constant mean ISF-vectors in the following manner:

*, i = 0..16* (9)

*where*

 = 0.75,  
  and is updated whenever BFI =0.   
  is a vector containing long time average of ISF-vectors.

#### 6.2.3.4 LTP-lag concealment

The histories of five last good LTP-lags and LTP-gains are used for finding the best method to update.

##### 6.2.3.4.1 LTP-lag concealment when RX\_FRAMETYPE = SPEECH\_BAD

The usability of the received LTP lag () is defined as follows: (Predicts if the received lag is most probably very close to one that was sent and therefore its usage should not introduce any bad artifacts)

 (10)

where:

 is LTP lag from the previous good frame,   
 ,   
 ,  
 ,   
 is received lag,   
 ,  
 is LTP gain of the current frame,  
 (-1) is LTP gain of the previous good frame,   
 (-2) is LTP gain of the frame before previous good frame,   
 

LPT lag value for the current frame is defined as follows:

 (11)

where:  
 ,   
 is second largest value in ,   
 is second largest value in ,   
 is random value generated to range 

##### 6.2.3.4.2 LTP-lag concealment when RX\_FRAMETYPE = SPEECH\_LOST

The usability of the LTP lag from last good frame () is defined as follows: (Predicts if the received lag is most probably very close to one that was sent and therefore its usage should not introduce any bad artifacts)

 (12)

where:

,  
 (n-1) is LTP gain of the previous good frame,   
 (n-2) is LTP gain of the frame before previous good frame

LPT lag value for the current frame is defined as follows:

 (13)

where:

 is LTP lag from the previous good frame,   
 ,   
 is second largest value in ,   
 is second largest value in ,   
 is random value generated to range 

### 6.2.4 Innovation sequence

When RX\_FRAMETYPE = SPEECH\_BAD, the received fixed codebook innovation pulses from the erroneous frame are used as they are received.

When RX\_FRAMETYPE = SPEECH\_LOST, the received fixed codebook innovation pulses from the erroneous frame are not used and the fixed codebook innovation vector is filled with random signal (values limited to   
range [-1, +1]).

### 6.2.5 High-band gain (for 23.85 kbit/s mode)

When RX\_FRAMETYPE = SPEECH\_BAD or RX\_FRAMETYPE = SPEECH\_LOST the received high-band energy parameter of the frame is not used and the estimation for the high-band gain is used instead. This means that in case of bad/lost speech frames, the high-band reconstruction operates in the same way for all the modes.

## 6.3 Substitution and muting of lost SID frames

In the speech decoder a single frame classified as SID\_BAD shall be substituted by the last valid SID frame information and the procedure for valid SID frames be applied. If the time between SID information updates (updates are specified by SID\_UPDATE arrivals and occasionally by SID\_FIRST arrivals) is greater than one second this shall lead to attenuation.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | |
| **Date** | **TSG SA#** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 03-2001 | 11 | SP-010086 |  |  | Version 2.0.0 produced for approval |  | 5.0.0 |
| 03-2002 | 15 | SP-020083 | 001 |  | Error concealment of high band gain in 23.85 kbit/s mode | 5.0.0 | 5.1.0 |
| 12-2004 | 26 |  |  |  | Version for Release 6 | 5.1.0 | 6.0.0 |
| 06-2007 | 36 |  |  |  | Version for Release 7 | 6.0.0 | 7.0.0 |
| 12-2008 | 42 |  |  |  | Version for Release 8 | 7.0.0 | 8.0.0 |
| 12-2009 | 46 |  |  |  | Version for Release 9 | 8.0.0 | 9.0.0 |
| 03-2011 | 51 |  |  |  | Version for Release 10 | 9.0.0 | 10.0.0 |
| 09-2012 | 57 |  |  |  | Version for Release 11 | 10.0.0 | 11.0.0 |
| 09-2014 | 65 |  |  |  | Version for Release 12 | 11.0.0 | 12.0.0 |
| 12-2015 | 70 |  |  |  | Version for Release 13 | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | 75 |  |  |  |  | Version for Release 14 | 14.0.0 |
| 2018-06 | 80 |  |  |  |  | Version for Release 15 | 15.0.0 |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | 16.0.0 |
| 2022-04 | - | - | - | - | - | Update to Rel-17 version (MCC) | 17.0.0 |
| 2024-03 | - | - | - | - | - | Update to Rel-18 version (MCC) | 18.0.0 |