|  |  |
| --- | --- |
| 3GPP TS 26.453 V18.0.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Services and System Aspects; Speech codec speech processing functions; Codec for Enhanced Voice Services (EVS); Speech codec frame structure  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 5

2 References 5

3 Abbreviations 6

4 EVS Codec generic frame format in CS Networks 6

4.1 General 6

4.2 EVS payload sizes in CS Networks 6

4.3 EVS generic frame header 7

4.4 EVS frame quality classification 7

4.5 EVS codec mode request in CS Networks 7

Annex A (informative): Change history 8

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The Enhanced Voice Services (EVS) Codec is specified in the series of Technical Specifications TS 26.441 [3], TS 26.442 [4], TS 26.443 [5], TS 26.444 [6], TS 26.445 [7], TS 26.446 [8], TS 26.447 [9], TS 26.448 [10], TS 26.449 [11], TS 26.450 [12], TS 26.451 [13] and TS 26.452 [15]. The EVS Codec is characterized in TR 26.952 [14].

The present document describes the "generic frame format" for the EVS Codec for the application in 3G Circuit-Switched Networks. This format is based on the RTP framing, as specified in TS 26.445 [7]. This generic frame format will be used as a common reference point, when interfacing speech frames between different elements of the 3G system. Appropriate mappings to and from this generic frame format will be used within and between each system element.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TR 41.001: "GSM Specification set".

[3] 3GPP TS 26.441: "Codec for Enhanced Voice Services (EVS); General overview".

[4] 3GPP TS 26.442: "Codec for Enhanced Voice Services (EVS); ANSI C code (fixed-point)".

[5] 3GPP TS 26.443: "Codec for Enhanced Voice Services (EVS); ANSI C code (floating-point)".

[6] 3GPP TS 26.444: "Codec for Enhanced Voice Services (EVS); Test Sequences".

[7] 3GPP TS 26.445: "Codec for Enhanced Voice Services (EVS); Detailed algorithmic description".

[8] 3GPP TS 26.446: "Codec for Enhanced Voice Services (EVS); Adaptive Multi-Rate - Wideband (AMR-WB) backward compatible functions".

[9] 3GPP TS 26.447: "Codec for Enhanced Voice Services (EVS); Error concealment of lost packets".

[10] 3GPP TS 26.448: "Codec for Enhanced Voice Services (EVS); Jitter buffer management".

[11] 3GPP TS 26.449: "Codec for Enhanced Voice Services (EVS); Comfort Noise Generation (CNG) aspects".

[12] 3GPP TS 26.450: "Codec for Enhanced Voice Services (EVS); Discontinuous Transmission (DTX)".

[13] 3GPP TS 26.451: "Codec for Enhanced Voice Services (EVS); Voice Activity Detection (VAD)".

[14] 3GPP TR 26.952: "Codec for Enhanced Voice Services (EVS); Performance Characterization".

[15] 3GPP TS 26.452: "Codec for Enhanced Voice Services (EVS); ANSI C code; Alternative fixed-point using updated basic operators".

# 3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

AMR-WB Adaptive Multi-Rate - WideBand

CMR Codec Mode Request (for AMR and AMR-WB and EVS)

CS Circuit Switched

EVS Enhanced Voice Services

EVS-CMR CMR for EVS

EVS-SID SID for EVS

FQC Frame quality Classification

EVS AMR-WB IO EVS AMR-WB Inter Operable (mode of operation)

MSB Most Significant Bit

RTP Real Time Protocol

SID Silence Insertion Descriptor (for AMR and AMR-WB)

ToC Table of Contents

WB-CMR CMR for AMR-WB

WB-SID SID for AMR-WB (and for EVS AMR-WB IO)

# 4 EVS Codec generic frame format in CS Networks

## 4.1 General

This clause describes the "generic frame format" of the EVS Codec in 3G CS networks for the Speech and SID frames of the primary modes of operation and the Speech and SID frames of the EVS AMR-WB IO mode of operation.

This generic frame format is illustrated in Figure 4.1-1 and it is based on the RTP format specified in TS 26.445 [7], Annex A, Figure A.3 (c), "Payload structure of Header-Full format with CMR + ToC single frame" and in TS 26.445 [7], Annex A, Figure A.6, "Payload structure for EVS AMR-WB IO SID (56 bit) payload" with the following modifications:

- The leading "1" bit, d(0), in the CMR octet (MSB) is omitted in CS networks;  
bits d(1) ... d(7) are copied bit by bit in the same order. EVS-CMR has therefore 7 bits.

- The ToC octet is omitted (Table of Contents in RTP).

- The Speech data or SID of the EVS primary and the EVS AMR-WB IO modes are copied bit by bit.  
Each rate has its own, unique number of bits (n+1).

- The 40 bits of the AMR-WB SID, d(0) ... d(39), are copied bit by bit into the generic frame format.

Note that the order of Speech data or SID bits is the same as in in TS 26.445 [7].




Figure 4.1-1: EVS Generic Frame Format in CS Networks

## 4.2 EVS payload sizes in CS Networks

Table 4.2-1 lists all EVS Primary rates for the application in CS Networks, including No\_Data. These payload sizes are always integer multiples of 8 bits (excluding the 7-bit EVS-CMR).

Table 4.2-1: Payload sizes for EVS Primary Rates in CS Networks

|  |  |  |
| --- | --- | --- |
| Rate | Payload Size (bits) | Net bit rate for active speech (kbps) |
| No\_Data | 0 | - |
| EVS Primary SID | 48 | - |
| EVS Primary 2.8 | 56 | 2,8 |
| EVS Primary 7.2 | 144 | 7,2 |
| EVS Primary 8.0 | 160 | 8,0 |
| EVS Primary 9.6 | 192 | 9,6 |
| EVS Primary 13.2 | 264 | 13,2 |
| EVS Primary 16.4 | 328 | 16,4 |
| EVS Primary 24.4 | 488 | 24,4 |

Table 4.2-2 lists all EVS AMR-WB IO rates for the application in CS Networks. In contrast to the payload sizes used in RTP, these payloads do not include any CMR overhead. These payload sizes are not always integer multiples of 8 bits (excluding the 7-bit EVS-CMR).

Table 4.2-2: Payload sizes for EVS AMR-WB IO modes in CS Networks

|  |  |  |
| --- | --- | --- |
| Rate | Payload Size (bits) | Net bit rate for active speech (kbps) |
| EVS-AMR-WB IO SID | 40 | - |
| EVS AMR-WB IO 6.6 | 132 | 6,6 |
| EVS AMR-WB IO 8.85 | 177 | 8,85 |
| EVS AMR-WB IO 12.65 | 253 | 12,65 |

## 4.3 EVS generic frame header

The EVS Codec generic frame format in CS networks has no header. The payload size defines the used Codec rate. Parameters inside this EVS payload differentiate the EVS audio bandwidth and the EVS mode of operation. For details, see TS 26.445 [7].

## 4.4 EVS frame quality classification

The EVS Codec generic frame format has no own Frame Quality Indicator. If transported on Iu and Nb the "Frame Quality Classification" (FQC) of the Iu and Nb framing protocol is used.

## 4.5 EVS codec mode request in CS Networks

The EVS Codec Mode Request (EVS-CMR) is specified in TS 26.445 [7], Annex A, Table A.3: Structure of CMR. The EVS-CMR has a size of 7 bits. The Header bit (MSB), specified in TS 26.445 [7], is omitted in CS networks.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG SA#** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 2016-03 | 70 | SP-160071 |  |  | Presented to TSG SA#71 Plenary (for approval) | - | 1.0.0 |
| 2016-03 |  |  |  |  | Approved at TSG SA#71 | 1.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | 75 |  |  |  |  | Version for Release 14 | 14.0.0 |
| 2018-06 | 80 |  |  |  |  | Version for Release 15 | 15.0.0 |
| 2019-03 | 83 | SP-190036 | 0001 | - | B | Addition of reference to Alt\_FX\_EVS implementation | 16.0.0 |
| 2022-04 | - | - | - | - | - | Update to Rel-17 version (MCC) | **17.0.0** |
| 2024-03 | - | - | - | - | - | Update to Rel-18 version (MCC) | **18.0.0** |