|  |  |
| --- | --- |
| 3GPP TS 38.101-5 V18.2.0 (2023-06) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 5: Satellite access Radio Frequency (RF) and performance requirements  (Release 18) | |
|  | |
|  | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 6

1 Scope 8

2 References 8

3 Definitions of terms, symbols and abbreviations 8

3.1 Terms 8

3.2 Symbols 9

3.3 Abbreviations 9

4 General 10

4.1 Relationship between minimum requirements and test requirements 10

4.2 Applicability of minimum requirements 10

4.3 Specification suffix information 11

4.4 Relationship with other core specifications 11

5 Operating bands and channel arrangement 11

5.1 General 11

5.2 Operating bands 11

5.2.1 General 11

5.2.2 Operating bands with conducted requirements 11

5.2.3 reserved (for radiated requirements) 12

5.3 UE channel bandwidth 12

5.3.1 General 12

5.3.2 Maximum transmission bandwidth configuration 12

5.3.3 Minimum guardband and transmission bandwidth configuration 13

5.3.4 RB alignment 14

5.3.5 UE channel bandwidth per operating band 14

5.4 Channel arrangement 14

5.4.1 Channel spacing 14

5.4.1.1 Channel spacing for adjacent NTN satellite carriers 14

5.4.2 Channel raster 14

5.4.2.1 NR-ARFCN and channel raster 14

5.4.2.2 Channel raster to resource element mapping 15

5.4.2.3 Channel raster entries for each operating band 15

5.4.3 Synchronization raster 15

5.4.3.1 Synchronization raster and numbering 15

5.4.3.2 Synchronization raster to synchronization block resource element mapping 16

5.4.3.3 Synchronization raster entries for each operating band 16

5.4.4 TX–RX frequency separation 16

6 Conducted transmitter characteristics 16

6.1 General 16

6.2 Transmitter power 17

6.2.1 UE maximum output power 17

6.2.2 UE maximum output power reduction 17

6.2.3 UE additional maximum output power reduction 17

6.2.3.1 General 17

6.2.4 Configured transmitted power 18

6.3 Output power dynamics. 18

6.3.1 Minimum output power 18

6.3.2 Transmit OFF power 19

6.3.3 Transmit ON/OFF time mask 19

6.3.4 Power control 19

6.4 Transmit signal quality 19

6.4.1 Frequency error 19

6.4.2 Transmit modulation quality 19

6.5 Output RF spectrum emissions 19

6.5.1 Occupied bandwidth 19

6.5.2 Out of band emission 20

6.5.2.1 General 20

6.5.2.2 Spectrum emission mask 20

6.5.2.3 “Reserved” 20

6.5.2.4 Adjacent channel leakage ratio 20

6.5.2.4.1 NR ACLR 21

6.5.2.4.2 UTRA ACLR 21

6.5.3 Spurious emission 21

6.5.3.1 General spurious emissions 21

6.5.3.2 Spurious emissions for UE co-existence 22

6.5.3.3 Additional spurious emissions 23

6.5.3.3.1 General 23

6.5.3.3.2 Requirement for network signalling value "NS\_02N" 23

6.5.4 Transmit intermodulation 23

7 Conducted receiver characteristics 24

7.1 General 24

7.2 Diversity characteristics 24

7.3 Reference sensitivity 24

7.3.1 General 24

7.3.2 Reference sensitivity power level 25

7.4 Maximum input level 25

7.5 Adjacent channel selectivity 26

7.6 Blocking characteristics 27

7.6.1 General 27

7.6.2 In-band blocking 27

7.6.3 Out-of-band blocking 28

7.6.4 Narrow band blocking 29

7.7 Spurious response 29

7.8 Intermodulation characteristics 30

7.9 Spurious emissions 30

8 Conducted performance requirements 30

8.1 General 30

8.1.1 Relationship between minimum requirements and test requirements 30

8.1.2 Applicability of minimum requirements 30

8.1.3 Conducted requirements 31

8.1.3.1 Introduction 31

8.1.3.2 Reference point 31

8.1.3.3 SNR definition 31

8.1.3.4 Noc 31

8.1.3.4.1 Introduction 31

8.1.3.4.2 Noc for NR operating bands in FR1 31

8.2 Demodulation performance requirements 32

8.2.1 General 32

8.2.1.1 Applicability of requirements 32

8.2.1.1.1 General 32

8.2.1.1.2 Applicability of requirements for optional UE features 32

8.2.1.2 PDSCH demodulation requirements 33

8.2.1.2.1 1RX requirements 36

8.2.1.2.2 2RX requirements 36

8.2.1.2.2.1.1 Minimum requirements for PDSCH Mapping Type A 36

8.3 CSI reporting requirements 38

Annex A (normative): Measurement channels 39

A.1 General 39

A.1.1 Throughput definition 39

A.2 UL reference measurement channels 39

A.3 DL reference measurement channels 39

A.3.1 General 39

A.3.2 Reference measurement channels for PDSCH performance requirements 39

A.3.2.1 FDD 40

A.3.2.1.1 Reference measurement channels for SCS 15 kHz FR1 40

Annex B (normative): Propagation conditions 42

B.1 Static propagation condition 42

B.1.1 UE Receiver with 1Rx 42

B.1.2 UE Receiver with 2Rx 42

B.2.1 Delay profiles 42

B.2.2 Combinations of channel model parameters 43

B.2.3 MIMO Channel Correlation Matrices 43

B.2.3.1 MIMO Correlation Matrices using Uniform Linear Array (ULA) 43

B.2.3.1.1 Definition of MIMO Correlation Matrices 43

B.2.3.1.2 MIMO Correlation Matrices at High, Medium and Low Level 44

Annex C (normative): Downlink physical channels 45

C.1 General 45

C.2 Setup (Conducted) 45

C.3 Connection (Conducted) 45

C.3.1 Measurement of Performance requirements 45

Annex D (informative): Void 46

Annex E (normative): Environmental conditions 46

E.1 General 46

E.2 Environmental (Conducted) 46

E.2.1 Temperature 46

E.2.2 Voltage 47

E.2.3 Vibration 47

Annex F (informative): Change history 48

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document establishes the minimum RF and performance requirements for NR User Equipment (UE) supporting satellite access operation.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.521-5: "NR; User Equipment (UE) conformance specification; Radio transmission and reception; Part 5: Satellite access Radio Frequency (RF) and performance requirements ".

[3] Recommendation ITU-R M.1545: "Measurement uncertainty as it applies to test limits for the terrestrial component of International Mobile Telecommunications-2000".

[4] 3GPP TS 38.108: "NR; Satellite Node radio transmission and reception"

[5] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[6] 3GPP TS 38.101-4: "NR; User Equipment (UE) radio transmission and reception; Part 4: Performance requirements".

[7] 3GPP TS 38.213: "NR; Physical layer procedures for control"

[8] 3GPP TS 38.331: " Radio Resource Control (RRC) protocol specification".

[9] 3GPP TS 38.300: "NR; NR and NG-RAN Overall description; Stage-2".

[10] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception".

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Geosynchronous Earth Orbit:** Earth-centered orbit at approximately 35786 kilometres above Earth's surface and synchronised with Earth's rotation. A geostationary orbit is a non-inclined geosynchronous orbit, i.e. in the Earth’s equator plane.

**Low Earth Orbit:** Orbit around the Earth with an altitude between 300 km, and 1500 km.

**Non-terrestrial networks:** Networks, or segments of networks, using an airborne or space-borne vehicle to embark a transmission equipment relay node or base station.

**Satellite:** A space-borne vehicle embarking a bent pipe payload or a regenerative payload telecommunication transmitter, placed into Low-Earth Orbit (LEO), Medium-Earth Orbit (MEO), or Geostationary Earth Orbit (GEO).

**Satellite Access Node:** see definition in TS 38.108[4].

**UE transmission bandwidth configuration**: Set of resource blocks located within the UE channel bandwidth which may be used for transmitting or receiving by the UE.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

ΔFGlobal Granularity of the global frequency raster

ΔFRaster Band dependent channel raster granularity

BWChannel Channel bandwidth

BWinterferer Bandwidth of the interferer

FDL\_low The lowest frequency of the downlink *operating band*

FDL\_high The highest frequency of the downlink *operating band*

FUL\_low The lowest frequency of the uplink *operating band*

FUL\_high The highest frequency of the uplink *operating band*

FInterferer Frequency of the interferer

FInterferer (offset) Frequency offset of the interferer (between the center frequency of the interferer and the carrier frequency of the carrier measured)

FIoffset Frequency offset of the interferer (between the center frequency of the interferer and the closest edge of the carrier measured)

FOOB The boundary between the NR out of band emission and spurious emission domains

FREF RF reference frequency

FREF-Offs Offset used for calculating FREF

Fuw (offset) The frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer

NRB Transmission bandwidth configuration, expressed in units of resource blocks

NREF NR Absolute Radio Frequency Channel Number (NR-ARFCN)

NREF-Offs Offset used for calculating NREF

PInterferer Modulated mean power of the interferer

Puw Power of an unwanted DL signal

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ACLR Adjacent Channel Leakage Ratio

ACS Adjacent Channel Selectivity

A-MPR Additional Maximum Power Reduction

BW Bandwidth

BWP Bandwidth Part

CP-OFDM Cyclic Prefix-OFDM

CW Continuous Wave

DFT-s-OFDM Discrete Fourier Transform-spread-OFDM

DM-RS Demodulation Reference Signal

DTX Discontinuous Transmission

EIRP Equivalent Isotropically Radiated Power

EVM Error Vector Magnitude

FR Frequency Range

FRC Fixed Reference Channel

GEO Geosynchronous Earth Orbit

GSCN Global Synchronization Channel Number

IBB In-band Blocking

ITU-R Radiocommunication Sector of the International Telecommunication Union

LEO Low Earth Orbiting

MBW Measurement bandwidth defined for the protected band

MEO Medium Earth Orbiting

MOP Maximum Output Power

MPR Allowed maximum power reduction

MSD Maximum Sensitivity Degradation

NGEO Non-Geostationary Earth Orbiting

NR New Radio

NR-ARFCN NR Absolute Radio Frequency Channel Number

NS Network Signalling

NTN Non-Terrestrial Network

OCNG OFDMA Channel Noise Generator

OOB Out-of-band

PRB Physical Resource Block

QAM Quadrature Amplitude Modulation

RAN Radio Access Network

RE Resource Element

REFSENS REFerence SENSitivity

RF Radio Frequency

RMS Root Mean Square (value)

RSRP Reference Signal Receive Power

RSRQ Reference Signal Receive Quality

RX Receiver

SAN Satellite Access Node

SC Single Carrier

SCS Subcarrier spacing

SEM Spectrum Emission Mask

SNR Signal-to-Noise Ratio

SRS Sounding Reference Symbol

SS Synchronization Symbol

TN Terrestrial Network

TX Transmitter

TxD Tx Diversity

UE User Equipment

# 4 General

## 4.1 Relationship between minimum requirements and test requirements

The present document is a Single-RAT specification for satellite NR UE, covering RF characteristics and minimum performance requirements. Conformance to the present specification is demonstrated by fulfilling the test requirements specified in the conformance specification 3GPP TS 38.521-5 [2].

The Minimum Requirements given in this specification make no allowance for measurement uncertainty. The test specification 3GPP TS 38.521-5 [2] defines test tolerances. These test tolerances are individually calculated for each test. The test tolerances are used to relax the minimum requirements in this specification to create test requirements. For some requirements, including regulatory requirements, the test tolerance is set to zero.

The measurement results returned by the test system are compared - without any modification - against the test requirements as defined by the shared risk principle.

The shared risk principle is defined in Recommendation ITU‑R M.1545 [3].

## 4.2 Applicability of minimum requirements

a) In this specification the Minimum Requirements are specified as general requirements and additional requirements. Where the Requirement is specified as a general requirement, the requirement is mandated to be met in all scenarios

b) For specific scenarios for which an additional requirement is specified, in addition to meeting the general requirement, the UE is mandated to meet the additional requirements.

c) The spurious emissions power requirements are for the long-term average of the power. For the purpose of reducing measurement uncertainty, it is acceptable to average the measured power over a period of time sufficient to reduce the uncertainty due to the statistical nature of the signal.

## 4.3 Specification suffix information

Specification suffix information is not defined for the time being in Release 17.

## 4.4 Relationship with other core specifications

The present document establishes the minimum RF and performance requirements for NR User Equipment (UE) operating in a Non-Terrestrial Network. The present document for the single-RAT specification of a satellite NR UE side is used together with the technical specification 3GPP TS 38.108 [4] specifying the Satellite Access Node (SAN).

# 5 Operating bands and channel arrangement

## 5.1 General

The channel arrangements presented in this clause are based on the operating bands and channel bandwidths defined in the present Release of specifications.

NOTE: Other operating bands and channel bandwidths may be considered in future Releases.

Requirements throughout the RF specifications are in many cases defined separately for different frequency ranges (FR). The frequency ranges in which NTN satellite can operate according to this version of the specification are identified as described in Table 5.1-1.

Table 5.1-1: Definition of frequency ranges

|  |  |
| --- | --- |
| Frequency range designation | Corresponding frequency range |
| FR1 | 410 MHz – 7125 MHz |

The present specification covers FR1 operating bands.

## 5.2 Operating bands

### 5.2.1 General

NTN satellite covers FR1 operating bands in the present specification.

### 5.2.2 Operating bands with conducted requirements

NTN satellite is designed to operate in the operating bands defined in Table 5.2.2-1.

Table 5.2.2-1: NTN satellite bands in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NTN satellite operating band | Uplink (UL) operating band Satellite Access Node receive / UE transmit  FUL,low – FUL,high | Downlink (DL) operating band Satellite Access Node transmit / UE receive  FDL,low – FDL,high | Duplex mode |
| n256 | 1980MHz – 2010 MHz | 2170 MHz – 2200 MHz | FDD |
| n255 | 1626.5 MHz – 1660.5 MHz | 1525 MHz – 1559 MHz | FDD |
| NOTE: NTN satellite bands are numbered in descending order from n256. | | | |

### 5.2.3 reserved (for radiated requirements)

[To be updated]

## 5.3 UE channel bandwidth

### 5.3.1 General

The UE channel bandwidth supports a single RF carrier in the uplink or downlink at the UE. From a SAN perspective, different UE channel bandwidths may be supported within the same spectrum for transmitting to and receiving from UEs connected to the SAN.

From a UE perspective, the UE is configured with one or more BWP / carriers, each with its own UE channel bandwidth. The UE does not need to be aware of the SAN channel bandwidth or how the SAN allocates bandwidth to different UEs.

The placement of the UE channel bandwidth for each UE carrier is flexible but can only be completely within the SAN channel bandwidth.

The relationship between the channel bandwidth, the guardband and the maximum transmission bandwidth configuration is shown in Figure 5.3.1-1.



Figure 5.3.1-1: Definition of the channel bandwidth and the maximum transmission bandwidth configuration for one channel

### 5.3.2 Maximum transmission bandwidth configuration

The maximum transmission bandwidth configuration NRB for each UE channel bandwidth and subcarrier spacing is specified in Table 5.3.2-1.

**Table 5.3.2-1: Maximum transmission bandwidth configuration NRB**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SCS (kHz) | 5  MHz | 10  MHz | 15  MHz | 20  MHz |
| NRB | NRB | NRB | NRB |
| 15 | 25 | 52 | 79 | 106 |
| 30 | 11 | 24 | 38 | 51 |
| 60 | N/A | 11 | 18 | 24 |

### 5.3.3 Minimum guardband and transmission bandwidth configuration

The minimum guardband for each UE channel bandwidth and SCS is specified in Table 5.3.3-1,

Table 5.3.3-1: Minimum guardband for each UE channel bandwidth and SCS (kHz)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SCS (kHz) | 5  MHz | 10  MHz | 15  MHz | 20  MHz |
| 15 | 242.5 | 312.5 | 382.5 | 452.5 |
| 30 | 505 | 665 | 645 | 805 |
| 60 | N/A | 1010 | 990 | 1330 |

NOTE: The minimum guardbands have been calculated using the following equation: (BWChannel x 1000 (kHz) - NRB x SCS x 12) / 2 - SCS/2, where NRB are from Table 5.3.2-1.

Figure 5.3.3-1: Void

The number of RBs configured in any channel bandwidth shall ensure that the minimum guardband specified in this clause is met.




Figure 5.3.3-2: UE PRB utilization

In the case that multiple numerologies are multiplexed in the same symbol, the minimum guard band on each side of the carrier is the guard band applied at the configured UE channel bandwidth for the numerology that is transmitted/received immediately adjacent to the guard band.




Figure 5.3.3-3: Guard band definition when transmitting multiple numerologies

NOTE: Figure 5.3.3-2 is not intended to imply the size of any guard between the two numerologies. Inter-numerology guard band within the carrier is implementation dependent.

### 5.3.4 RB alignment

The RB alignment refers to NR RB alignments as specified in 3GPP TS 38.101-1 [5] clause 5.3.4.

### 5.3.5 UE channel bandwidth per operating band

The requirements in this specification apply to the combination of channel bandwidths, SCS and operating bands shown in Table 5.3.5-1. The transmission bandwidth configuration in Table 5.3.2-1 shall be supported for each of the specified channel bandwidths. The channel bandwidths are specified for both the TX and RX path.

Table 5.3.5-1: Channel bandwidths for each NTN satellite band

| NTN satellite band | SCS  kHz | UE Channel bandwidth (MHz) | | | |
| --- | --- | --- | --- | --- | --- |
| 5 | 10 | 15 | 20 |
|  | 15 | 5 | 10 | 15 | 20 |
| n256 | 30 |  | 10 | 15 | 20 |
|  | 60 |  | 10 | 15 | 20 |
|  | 15 | 5 | 10 | 15 | 20 |
| n255 | 30 |  | 10 | 15 | 20 |
|  | 60 |  | 10 | 15 | 20 |

## 5.4 Channel arrangement

### 5.4.1 Channel spacing

#### 5.4.1.1 Channel spacing for adjacent NTN satellite carriers

The channel spacing for adjacent NTN satellite carriers refers to the NR channel spacing as specified in 3GPP TS 38.101-1 [5] clause 5.4.1.1.

### 5.4.2 Channel raster

#### 5.4.2.1 NR-ARFCN and channel raster

The global frequency channel raster defines a set of RF reference frequencies FREF. The RF reference frequency is used in signalling to identify the position of RF channels, SS blocks and other elements.

The global frequency raster is defined for all frequencies from 0 to 100 GHz. The granularity of the global frequency raster is ΔFGlobal.

RF reference frequencies are designated by an NR Absolute Radio Frequency Channel Number (NR-ARFCN) in the range (0…2016666) on the global frequency raster. The relation between the NR-ARFCN and the RF reference frequency FREF in MHz is given by the following equation, where FREF-Offs and NREF-Offs are given in Table 5.4.2.1-1 and NREF is the NR-ARFCN.

FREF = FREF-Offs + ΔFGlobal (NREF – NREF-Offs)

Table 5.4.2.1-1: NR-ARFCN parameters for the global frequency raster

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency range (MHz) | ΔFGlobal (kHz) | FREF-Offs (MHz) | NREF-Offs | Range of NREF |
| 0 – 3000 | 5 | 0 | 0 | 0 – 599999 |

The channel raster defines a subset of RF reference frequencies that can be used to identify the RF channel position in the uplink and downlink. The RF reference frequency for an RF channel maps to a resource element on the carrier. For each operating band, a subset of frequencies from the global frequency raster are applicable for that band and forms a channel raster with a granularity ΔFRaster, which may be equal to or larger than ΔFGlobal.

The mapping between the channel raster and corresponding resource element is given in clause 5.4.2.2. The applicable entries for each operating band are defined in clause 5.4.2.3.

#### 5.4.2.2 Channel raster to resource element mapping

The mapping between the RF reference frequency on the channel raster and the corresponding resource element refers to the NR requirements specified in 3GPP TS 38.101-1 [5] clause 5.4.2.2.

#### 5.4.2.3 Channel raster entries for each operating band

The RF channel positions on the channel raster in each NTN satellite operating band are given through the applicable NR-ARFCN in Table 5.4.2.3‑1, using the channel raster to resource element mapping in clause 5.4.2.2.

For NTN satellite operating bands with 100 kHz channel raster, ΔFRaster = 20 × ΔFGlobal. In this case every 20th NR-ARFCN within the operating band are applicable for the channel raster within the operating band and the step size for the channel raster in Table 5.4.2.3‑1 is given as <20>.

Table 5.4.2.3-1: Applicable NR-ARFCN per operating band

|  |  |  |  |
| --- | --- | --- | --- |
| NTN satellite operating band | ΔFRaster  (kHz) | Uplink  Range of NREF  (First – <Step size> – Last) | Downlink  Range of NREF  (First – <Step size> – Last) |
| n256 | 100 | 396000 – <20> – 402000 | 434000 – <20> – 440000 |
| n255 | 100 | 325300 – <20> – 332100 | 305000 – <20> – 311800 |
| NOTE : The channel numbers that designate carrier frequencies so close to the operating band edges that the carrier extends beyond the operating band edge shall not be used. | | | |

### 5.4.3 Synchronization raster

#### 5.4.3.1 Synchronization raster and numbering

The synchronization raster indicates the frequency positions of the synchronization block that can be used by the UE for system acquisition when explicit signalling of the synchronization block position is not present.

A global synchronization raster is defined for all frequencies. The frequency position of the SS block is defined as SSREF with corresponding number GSCN. The parameters defining the SSREF and GSCN for all the frequency ranges are in Table 5.4.3.1-1.

The resource element corresponding to the SS block reference frequency SSREF is given in clause 5.4.3.2. The synchronization raster and the subcarrier spacing of the synchronization block is defined separately for each band.

Table 5.4.3.1-1: GSCN parameters for the global frequency raster

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | SS Block frequency position SSREF | GSCN | Range of GSCN |
| 0 – 3000 MHz | N \* 1200kHz + M \* 50 kHz,  N=1:2499, M ϵ {1,3,5}1 | 3N + (M-3)/2 | 2 – 7498 |
| NOTE: The default value for operating bands with which only support SCS spaced channel raster(s) is M=3. | | | |

#### 5.4.3.2 Synchronization raster to synchronization block resource element mapping

The mapping between the synchronization raster and the corresponding resource element of the SS block refers to 3GPP TS 38.101-1 [5] clause 5.4.3.2.

#### 5.4.3.3 Synchronization raster entries for each operating band

The synchronization raster for each band is give in Table 5.4.3.3-1. The distance between applicable GSCN entries is given by the <Step size> indicated in Table 5.4.3.3-1.

Table 5.4.3.3-1: Applicable SS raster entries per operating band

|  |  |  |  |
| --- | --- | --- | --- |
| NTN satellite operating band | SS Block SCS | SS Block pattern1 | Range of GSCN  (First – <Step size> – Last) |
| n256 | 15 kHz | Case A | 5429 – <1> – 5494 |
| n255 | 15 kHz | Case A | 3818 – <1> – 3892 |
|  | 30 kHz | Case B | 3824 – <1> – 3886 |
| NOTE : SS Block pattern is defined in clause 4.1 in 3GPP TS 38.213 [7]. | | | |

### 5.4.4 TX–RX frequency separation

The default TX channel (carrier centre frequency) to RX channel (carrier centre frequency) separation for operating bands is specified in Table 5.4.4-1.

Table 5.4.4-1: UE TX-RX frequency separation

| NTN Satellite Operating Band | TX – RX  carrier centre frequency separation |
| --- | --- |
| n256 | 190 MHz |
| n255 | -101.5 MHz |

# 6 Conducted transmitter characteristics

## 6.1 General

Unless otherwise stated, the transmitter characteristics for satellite access UEs are specified at the antenna connector of the UE with a single or multiple transmit antenna(s). For UE with integral antenna only, a reference antenna with a gain of 0 dBi is assumed. Handheld power class 3 UE is assumed in Release 17 for satellite access.

All requriements in this section, other than frequency error in clause 6.4.1, shall be verified when Doppler conditions are set to zero.

## 6.2 Transmitter power

### 6.2.1 UE maximum output power

The following UE Power Classes define the maximum output power for any transmission bandwidth within the channel bandwidth of NR carrier unless otherwise stated. The period of measurement shall be at least one sub frame (1ms).

Table 6.2.1-1: UE Power Class

|  |  |  |
| --- | --- | --- |
| NR satellite band | Class 3 (dBm) | Tolerance (dB) |
| n256 | 23 | ±2 |
| n255 | 23 | ±2 |
| NOTE 1: PPowerClass is the maximum UE power specified without taking into account the tolerance  NOTE 2: Powerclass 3 is default power class unless otherwise stated | | |

### 6.2.2 UE maximum output power reduction

UE is allowed to reduce the maximum output power due to higher order modulations and transmit bandwidth configurations. For UE power class 3, the allowed maximum power reduction (MPR) is defined as Table 6.2.2-1 in 3GPP TS 38.101-1[5] clause 6.2.2.

### 6.2.3 UE additional maximum output power reduction

#### 6.2.3.1 General

Additional emission requirements can be signalled by the network. Each additional emission requirement is associated with a unique network signalling (NS) value indicated in RRC signalling by an NR frequency band number of the applicable operating band and an associated value in the field *additionalSpectrumEmission.* Throughout this specification, the notion of indication or signalling of an NS value refers to the corresponding indication of an NR satellite band number of the applicable operating band, the IE field *freqBandIndicatorNR* and an associated value of *additionalSpectrumEmission* in the relevant RRC information elements [6]*.*

To meet the additional requirements, additional maximum power reduction (A-MPR) is allowed for the maximum output power as specified in Table 6.2.1-1. Unless stated otherwise, the total reduction to UE maximum output power is max(MPR, A-MPR) where MPR is defined in clause 6.2.2. Outer and inner allocation notation used in clause 6.2.3 is defined in 3GPP TS 38.101-1 [5] clause 6.2.2. In absence of modulation and waveform types the A-MPR applies to all modulation and waveform types.

Table 6.2.3.1-1 specifies the additional requirements with their associated network signalling values and the allowed A-MPR and applicable operating band(s) for each NS value. The mapping of NR satellite band numbers and values of the *additionalSpectrumEmission* to network signalling labels is specified in Table 6.2.3.1-1A.

Table 6.2.3.1-1: Additional maximum power reduction (A-MPR)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Network signalling label | Requirements (clause) | NR satellite Band | Channel bandwidth (MHz) | Resources blocks (*N*RB) | A-MPR (dB) |
| NS\_01 |  | Table 5.2-1 | 5, 10, 15, 20 | Table 5.3.2-1 in 3GPP TS 38.101-1 [5] | N/A |
| NS\_24 | 6.5.3.3.13 in 3GPP TS 38.101-1 [5] | n256 | 5, 10, 15, 20 | Table 6.2.3.15-1 in 3GPP TS 38.101-1 [5] | Clause 6.2.3.7 in 3GPP TS 38.101-1 [5]2 |
| NS\_02N | 6.5.3.3.2 | n255 | 5, 10, 15, 20 |  | N/A |
| NS\_100 | 6.5.2.4.2 in 3GPP TS 38.101-1 [5] | n2561 |  |  | Table  6.2.3.1-2 in 3GPP TS 38.101-1 [5] |
| NOTE 1: This NS can be signalled for NR bands that have UTRA services deployed.  NOTE 2: A-MPR for the upper 5 MHz of the band is not specified, and therefore shall be used as a guard band. | | | | | |

[The NS\_01 label with the field *additionalPmax* [8] absent is default for all NTN satellite bands.]

Table 6.2.3.1-1A: Mapping of network signalling label

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR satellite band | Value of additionalSpectrumEmission | | | | | | | |
|  | **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** |
| n256 | NS\_01 | NS\_24 | NS\_100 |  |  |  |  |  |
| n255 | NS\_01 | NS\_02N |  |  |  |  |  |  |
| NOTE: *additionalSpectrumEmission* corresponds to an information element of the same name defined in clause 6.3.2 of 3GPP TS 38.331 [8]. | | | | | | | | |

### 6.2.4 Configured transmitted power

The requirements for configured transmitted power defined in subclause 6.2.4 of 3GPP TS 38.101-1 [5] clause 6.2.4 shall apply to NTN satellite UE.

## 6.3 Output power dynamics.

### 6.3.1 Minimum output power

The minimum controlled output power of the UE is defined as the power in the channel bandwidth for all transmit bandwidth configurations (resource blocks), when the power is set to a minimum value.

The minimum output power is defined as the mean power in at least one sub-frame (1 ms). The minimum output power shall not exceed the values specified in Table 6.3.1-1.

Table 6.3.1-1: Minimum output power

|  |  |  |
| --- | --- | --- |
| Channel bandwidth  (MHz) | Minimum output power  (dBm) | Measurement bandwidth  (MHz) |
| 5 | -40 | 4.515 |
| 10 | -40 | 9.375 |
| 15 | -40 | 14.235 |
| 20 | -40 | 19.095 |

### 6.3.2 Transmit OFF power

Transmit OFF power is defined as the mean power in the channel bandwidth when the transmitter is OFF. The transmitter is considered OFF when the UE is not allowed to transmit on any of its ports.

The transmit OFF power is defined as the mean power in a duration of at least one sub-frame (1 ms) excluding any transient periods. The transmit OFF power shall not exceed the values specified in Table 6.3.2-1.

Table 6.3.2-1: Transmit OFF power

|  |  |  |
| --- | --- | --- |
| Channel bandwidth | (MHz) | 5, 10, 15, 20 |
| REF\_SCS | (kHz) | 15 |
| Transmit OFF power | (dBm) | -50 |
| Measurement bandwidth | (MHz) | MBW=REF\_SCS\*(12\*NRB+1)/1000 |

### 6.3.3 Transmit ON/OFF time mask

The requirements for transmit ON/OFF time mask defined in 3GPP TS 38.101-1 [5] clause 6.3.3 shall apply for NTN satellite UE.

### 6.3.4 Power control

The requirements for Power control defined in 3GPP TS 38.101-1 [5] clause 6.3.4 shall apply for NTN satellite UE.

## 6.4 Transmit signal quality

### 6.4.1 Frequency error

The NTN satellite UE basic measurement interval of modulated carrier frequency is 1 UL slot. The NTN satellite UE pre-compensates the uplink modulated carrier frequency by the estimated Doppler shift according to 3GPP TS 38.300 [9] clause 16.14.2. The mean value of basic measurements of NTN UE modulated carrier frequency shall be accurate to within ± 0.1 PPM observed over a period of 1 ms of cumulated measurement intervals compared to ideally pre-compensated reference uplink carrier frequency.

[NOTE: The ideally pre-compensated reference uplink carrier frequency consists of the UL carrier frequency signalled to the UE by SAN and UL pre-compensated Doppler frequency shift. For the test case, the location of the UE is explicitly provided to the UE from the test equipment.]

Requirement will be verified for at least two cases of which one has zero Doppler conditions.

### 6.4.2 Transmit modulation quality

The requirements for transmit modulation quality defined in 3GPP TS 38.101-1 [5] clause 6.4.2 shall apply for NTN satellite UE except for the requirements for Pi/2 BPSK modulation.

## 6.5 Output RF spectrum emissions

### 6.5.1 Occupied bandwidth

Occupied bandwidth is defined as the bandwidth containing 99 % of the total integrated mean power of the transmitted spectrum on the assigned channel. The occupied bandwidth for all transmission bandwidth configurations (Resources Blocks) shall be less than the channel bandwidth specified in Table 6.5.1-1.

Table 6.5.1-1: Occupied channel bandwidth

|  |  |
| --- | --- |
|  | NR NTN satellite channel bandwidth (MHz) |
|  | 5, 10, 15, 20 |
| **Occupied channel bandwidth (MHz)** | Same as NR NTN satellite channel bandwidth |

### 6.5.2 Out of band emission

#### 6.5.2.1 General

The Out of band emissions are unwanted emissions immediately outside the assigned channel bandwidth resulting from the modulation process and non-linearity in the transmitter but excluding spurious emissions. This out of band emission limit is specified in terms of a spectrum emission mask and an adjacent channel leakage power ratio.

To improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

#### 6.5.2.2 Spectrum emission mask

The spectrum emission mask of the UE applies to frequencies (ΔfOOB) starting from the ± edge of the assigned NR channel bandwidth. For frequencies offset greater than ΔfOOB, the spurious requirements in clause 6.5.3 are applicable.

NOTE: For measurement conditions at the edge of each frequency range, the lowest frequency of the measurement position in each frequency range should be set at the lowest boundary of the frequency range plus MBW/2. The highest frequency of the measurement position in each frequency range should be set at the highest boundary of the frequency range minus MBW/2. MBW denotes the measurement bandwidth defined for the protected band.

The power of any UE emission shall not exceed the levels specified in Table 6.5.2.2-1 for the specified channel bandwidth.

Table 6.5.2.2-1: General NR spectrum emission mask

|  |  |  |  |
| --- | --- | --- | --- |
| ΔfOOB  (MHz) | Channel bandwidth (MHz) / Spectrum emission limit (dBm) | | Measurement bandwidth |
| 5 | 10, 15, 20 |
| ± 0-1 | -13 | -13 | 1 % of channel BW |
| ± 1-5 | -10 | -10 | 1 MHz |
| ± 5-6 | -13 |  |
| ± 6-10 | -25 |  |
| ± 5-BWChannel |  | -13 |
| ± BWChannel-(BWChannel+5) |  | -25 |

#### 6.5.2.3 “Reserved”

#### 6.5.2.4 Adjacent channel leakage ratio

Adjacent Channel Leakage power Ratio (ACLR) is the ratio of the filtered mean power centred on the assigned channel frequency to the filtered mean power centred on an adjacent channel frequency.

To improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

##### 6.5.2.4.1 NR ACLR

NR Adjacent Channel Leakage power Ratio (NRACLR) is the ratio of the filtered mean power centred on the assigned NR channel frequency to the filtered mean power centred on an adjacent NR channel frequency at nominal channel spacing.

The assigned NR channel power and adjacent NR channel power are measured with rectangular filters with measurement bandwidths specified in Table 6.5.2.4.1-1.

If the measured adjacent channel power is greater than –50 dBm then the NRACLR shall be higher than the value specified in Table 6.5.2.4.1-2.

Table 6.5.2.4.1-1: NR ACLR measurement bandwidth

|  |  |  |
| --- | --- | --- |
| Channel bandwidth | (MHz) | 5,10,15,20 |
| REF\_SCS | (kHz) | 15 |
| NR ACLR measurement bandwidth | (MHz) | MBW=REF\_SCS\*(12\*NRB+1)/1000 |

Table 6.5.2.4.1-2: NR ACLR requirement

|  |  |
| --- | --- |
|  | Power class 3 |
| NR ACLR | 30 dB |

##### 6.5.2.4.2 UTRA ACLR

UTRA adjacent channel leakage power ratio (UTRAACLR) is the ratio of the filtered mean power centred on the assigned NR channel frequency to the filtered mean power centred on an adjacent(s) UTRA channel frequency.

UTRAACLR is specified for the first adjacent UTRA channel (UTRAACLR1) which center frequency is ± 2.5 MHz from NR channel edge and for the 2nd adjacent UTRA channel (UTRAACLR2) which center frequency is ± 7.5 MHz from NR channel edge.

The UTRA channel power is measured with a RRC filter with roll-off factor = 0.22 and bandwidth of 3.84 MHz. The assigned NR channel power is measured with a rectangular filter with measurement bandwidth specified in Table 6.5.2.4.1-1.

If the measured adjacent channel power is greater than – 50 dBm then the UTRAACLR1 and UTRAACLR2 shall be higher than the value specified in Table 6.5.2.4.2-1.

Table 6.5.2.4.2-1: UTRA ACLR requirement

|  |  |
| --- | --- |
|  | Power class 3 |
| UTRAACLR1 | 33 dB |
| UTRAACLR2 | 36 dB |

UTRA ACLR requirement is applicable when signalled by the network with network signalling value indicated by the field *additionalSpectrumEmission*.

### 6.5.3 Spurious emission

#### 6.5.3.1 General spurious emissions

Unless otherwise stated, the spurious emission limits apply for the frequency ranges that are more than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth. The spurious emission limits in Table 6.5.3.1-2 apply for all transmitter band configurations (NRB) and channel bandwidths.

Table 6.5.3.1-1: Boundary between NR out of band and general spurious emission domain

|  |  |
| --- | --- |
| Channel bandwidth | OOB boundary FOOB (MHz) |
| BWChannel | BWChannel + 5 |

Table 6.5.3.1-2: Requirement for general spurious emissions limits

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency Range | Maximum Level | Measurement bandwidth | NOTE |
| 9 kHz ≤ f < 150 kHz | -36 dBm | 1 kHz |  |
| 150 kHz ≤ f < 30 MHz | -36 dBm | 10 kHz |  |
| 30 MHz ≤ f < 1000 MHz | -36 dBm | 100 kHz |  |
| 1 GHz ≤ f < 5th harmonic of the upper frequency edge of the UL operating band in GHz | -30 dBm | 1 MHz |  |

#### 6.5.3.2 Spurious emissions for UE co-existence

This clause specifies the requirements for NR NTN satellite bands for UE coexistence with protected bands.

Table 6.5.3.2-1: Requirements for spurious emissions for UE co-existence

| NR NTN satellite Band | Spurious emission for UE co-existence | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| n255 | NR Band n1, n2, n3, n5, n7, n8, n12, n13, n14, n18, n20, n24, n25, n26, n28, n29, n30, n34, n38, n39, n40, n41, n48, n50, n51, n53, n65, n66, n67, n70, n71, n74, n75, n76, n85, n90, n91, n92, n93, n94, n100, n101 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n256 | NR Band n1, n3, n5, n7, n8, n12, n13, n14, n18, n20, n24, n26, n28, n29, n30, n38, n39, n40, n41, n48, n50, n51, n53, n54, n65, n66, n67, n71, n74, n75, n76, n78, n79, n85, n90, n91, n92, n93, n94, n101, n100, n101 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 33, 35 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| NR Band n2, n25, n70 | FDL\_low | - | FDL\_high | NA | NA | 3 |
| NOTE 1: The protected NR or E-UTRA bands are specified in clause 5.2 from 3GPP TS 38.101-1 [5] or 3GPP TS 36.101 [10]. FDL\_low and FDL\_high refer to each frequency band specified in Table 5.2-1 in 3GPP TS 38.101-1 [5] or 3GPP TS 36.101 [10].  NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.5.3.1-2 are permitted for each assigned NR carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x RBsize kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.  NOTE 3: The co-existence between n256 and band n2, n25 and n70 is subject to regional/national regulation. | | | | | | | |

NOTE: To simplify Table 6.5.3.2-1, NR band numbers are listed for bands which are specified only for NR operation or both E-UTRA and NR operation. E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation.

#### 6.5.3.3 Additional spurious emissions

##### 6.5.3.3.1 General

These requirements are specified in terms of an additional spectrum emission requirement. Additional spurious emission requirements are signalled by the network to indicate that the UE shall meet an additional requirement for a specific deployment scenario as part of the cell handover/broadcast message.

##### 6.5.3.3.2 Requirement for network signalling value "NS\_02N"

When "NS\_02N" is indicated in the cell, the power of any UE emission shall not exceed the levels specified in Table 6.5.3.3.2-1. This requirement also applies for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.

Table 6.5.3.3.2-1: Additional requirements for "NS\_02N"

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency band  (MHz) | Channel bandwidth / Spectrum emission limit1 (dBm) | Measurement bandwidth | NOTE |
| 5 MHz, 10 MHz, 15 MHz, 20 MHz |
| 1559≤ f ≤ 1605 | -50 | 700 Hz | Averaged over any 2 millisecond active transmission interval |
| 1605≤ f ≤ 1610 | -50 + 24/5 (f-1605) | 700Hz |  |
| 1559 ≤ f ≤ 1605 | -40 | 1MHz | Averaged over any 2 millisecond active transmission interval |
| 1605≤ f ≤ 1610 | -40 + 24/5 (f-1605) | 1MHz |  |
| NOTE: The EIRP requirement in regulation is converted to conducted requirement using a 0 dBi antenna. | | | |

### 6.5.4 Transmit intermodulation

The transmit intermodulation performance is a measure of the capability of the transmitter to inhibit the generation of signals in its non-linear elements caused by presence of the wanted signal and an interfering signal reaching the transmitter via the antenna.

UE transmit intermodulation is defined by the ratio of the mean power of the wanted signal to the mean power of the intermodulation product when an interfering CW signal is added at a level below the wanted signal at each transmitter antenna port with the other antenna port(s) if any terminated. Both the wanted signal power and the intermodulation product power are measured through NR rectangular filter with measurement bandwidth shown in Table 6.5.4-1.

The requirement of transmit intermodulation is specified in Table 6.5.4-1.

Table 6.5.4-1: Transmit Intermodulation

|  |  |  |
| --- | --- | --- |
| Wanted signal  channel bandwidth | BWChannel | |
| Interference signal  frequency offset from channel center | BWChannel | 2\*BWChannel |
| Interference CW signal level | -40 dBc | |
| Intermodulation product | < -29 dBc | < -35 dBc |
| Measurement bandwidth | The maximum transmission bandwidth configuration among the different SCS's for the channel BW as defined in Table 6.5.2.4.1-1 | |
| Measurement offset from channel center | BWChannel and 2\*BWChannel | 2\*BWChannel and 4\*BWChannel |

# 7 Conducted receiver characteristics

## 7.1 General

Unless otherwise stated the receiver characteristics are specified at the antenna connector(s) of the UE. For UE(s) with an integral antenna only, a reference antenna(s) with a gain of 0 dBi is assumed for each antenna port(s). UE with an integral antenna(s) may be taken into account by converting these power levels into field strength requirements, assuming a 0 dBi gain antenna. For UEs with more than one receiver antenna connector, identical interfering signals shall be applied to each receiver antenna port if more than one of these is used (diversity).

The levels of the test signal applied to each of the antenna connectors shall be as defined in the respective clauses below.

With the exception of clause 7.3, the requirements shall be verified with the network signalling value NS\_01 configured in Table 6.2.3.1-1.

All requriements in this section shall be verified when Doppler conditions are set to zero.

All the parameters in clause 7 are defined using the UL reference measurement channels specified in 3GPP TS 38.101-1 [5] Annex A.2.2, the DL reference measurement channels specified in 3GPP TS 38.101-1 [5] Annex A.3.2 and using the set-up specified in 3GPP TS 38.101-1 [5] Annex C.3.1.

## 7.2 Diversity characteristics

The UE is required to be equipped with a minimum of two RX antenna ports in all operating bands.

The UE shall be verified with two RX antenna ports in all supported frequency bands.

The above rules apply for all clauses with the exception of clause 7.9.

## 7.3 Reference sensitivity

### 7.3.1 General

The reference sensitivity power level REFSENS is the minimum mean power applied to each one of the UE antenna ports for all UE categories, at which the throughput shall meet or exceed the requirements for the specified reference measurement channel.

In later clauses of Clause 7 where the value of REFSENS is used as a reference to set the corresponding requirement:

in all bands, the UE shall be verified against those requirements by applying the REFSENS value in Table 7.3.2-1.

### 7.3.2 Reference sensitivity power level

The throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in Annex A3.2.2 of 3GPP TS 38.101-1 [5], with parameters specified in Table 7.3.2-1.

Table 7.3.2-1: Two antenna port reference sensitivity QPSK PREFSENS for FDD bands

| Operating band / SCS / Channel bandwidth | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | SCS kHz | 5  MHz (dBm) | 10  MHz (dBm) | 15  MHz (dBm) | 20  MHz (dBm) | 25  MHz (dBm) | 30 MHz (dBm) | 35 MHz (dBm) | 40  MHz (dBm) | 45 MHz (dBm) | 50  MHz (dBm) |
| n256 | 15 | -99.5 | -96.3 | -94.5 | -93.8 |  |  |  |  |  |  |
| 30 |  | -96.6 | -94.6 | -94.0 |  |  |  |  |  |  |
| 60 |  | -97.0 | -94.9 | -94.2 |  |  |  |  |  |  |
| n255 | 15 | -100.0 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 |  |  |  |  |  |  |
| NOTE：The transmitter shall be set to PUMAX as defined in clause 6.2.4 of 3GPP TS 38.101-1 [5]. | | | | | | | | | | | |

The reference receiver sensitivity (REFSENS) requirement specified in Table 7.3.2-1 shall be met with uplink transmission bandwidth less than or equal to that specified in Table 7.3.2-2.

less than or equal to that specified in Table 7.3.2-2.

Table 7.3.2-2: Uplink configuration for reference sensitivity

| Operating band / SCS (kHz) / Channel bandwidth (MHz) / Duplex mode | | | | | | |
| --- | --- | --- | --- | --- | --- | --- |
| Operating Band | SCS | 5 | 10 | 15 | 20 | Duplex Mode |
|  | 15 | 25 | 50 | 75 | 100 |  |
| n256 | 30 |  | 24 | 36 | 50 | FDD |
|  | 60 |  | 10 | 18 | 24 |  |
|  | 15 | 25 | 50 | 75 | [75] |  |
| n255 | 30 |  | 24 | 36 | [36] | FDD |
|  | 60 |  | 10 | 18 | [18] |  |
| NOTE: UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth (Table 5.3.2-1 of 3GPP TS 38.101-1 [5]). | | | | | | |

The minimum requirements specified in Table 7.3.2-1 shall be verified with the network signalling value NS\_01 (Table 6.2.3.1-1 of 3GPP TS 38.101-1 [5]) configured.

## 7.4 Maximum input level

Maximum input level is defined as the maximum mean power received at the UE antenna port, at which the specified relative throughput shall meet or exceed the minimum requirements for the specified reference measurement channel. The throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annex A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD as described in 3GPP TS 38.101-1 [5] Annex A.5.1.1) with parameters specified in Table 7.4-1.

Table 7.4-1: Maximum input level

|  |  |  |
| --- | --- | --- |
| **Rx Parameter** | **Units** | **Channel bandwidth (MHz)** |
| **5, 10, 15, 20** |
| Power in Transmission Bandwidth Configuration3 | dBm | -402 |
| NOTE 1: The transmitter shall be set to 4 dB below PCMAX\_L,f,c at the minimum uplink configuration specified in Table 7.3.2-2 with PCMAX\_L,f,c as defined in clause 6.2.4.  NOTE 2: Reference measurement channel is specified in 3GPP TS 38.101-1 [5] Annex A.3.2.3 for 64 QAM.  NOTE 3: Power in transmission bandwidth configuration value is rounded to the nearest 0.5dB value. | | |

## 7.5 Adjacent channel selectivity

Adjacent channel selectivity (ACS) is a measure of a receiver's ability to receive an NR signal at its assigned channel frequency in the presence of an adjacent channel signal at a given frequency offset from the centre frequency of the assigned channel. ACS is the ratio of the receive filter attenuation on the assigned channel frequency to the receive filter attenuation on the adjacent channel(s).

In Release 17, only frequency bands below 2.7GHz are considered. The NR satellite UE shall fulfil the minimum requirements specified in Table 7.5-1 for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz. These requirements apply for all values of an adjacent channel interferer in case 1 and for any SCS specified for the channel bandwidth of the wanted signal. The lower and upper range of test parameters are chosen as in Table 7.5-2 and Table 7.5-3 for verification of the requirements specified in Table 7.5-1. For these test parameters, the throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annexes A.2.2 and A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in 3GPP TS 38.101-1 [5] Annex A.5.1.1).

Table 7.5-1: ACS for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| RX parameter | Units | Channel bandwidth (MHz) | | |
| 5, 10 | 15 | 20 |
| ACS | dB | 33 | 30 | 27 |

Table 7.5-2: Test parameters for NR bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz, case 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| RX parameter | Units | Channel bandwidth (MHz) | | |
| 5, 10 | 15 | 20 |
| Power in transmission bandwidth configuration | dBm | REFSENS + 14 dB | | |
| Pinterferer4 | dBm | REFSENS + 45.5 dB | REFSENS + 42.5 dB | REFSENS + 39.5 |
| BWinterferer | MHz | 5 | | |
| Finterferer (offset)2 | MHz | BWChannel /2 + 2.5  /  -(BWChannel /2 + 2.5) | | |
| NOTE 1: The transmitter shall be set to 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in clause 7.3.2 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the wanted signal in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 3: The interferer consists of the NR interferer RMC specified in 3GPP TS 38.101-1 [5] Annex A.3.2.2 with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in 3GPP TS 38.101-1 [5] Annex A.5.1.1.  NOTE 4: Pinterferer shall be rounded to the next higher 0.5dB value. | | | | |

Table 7.5-3: Test parameters for NR bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz, case 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| RX parameter | Units | Channel bandwidth (MHz) | | |
| 5, 10 | 15 | 20 |
| Power in transmission bandwidth configuration | dBm | -71.5 | -68.5 | -65.5 |
| Pinterferer | dBm | -40 | | |
| BWinterferer | MHz | 5 | | |
| Finterferer (offset) | MHz | BWChannel /2 + 2.5  /  -(BWChannel /2 + 2.5) | | |
| NOTE 1: The transmitter shall be set to 24 dB below PCMAX\_L,f,c at the minimum UL configuration specified in clause 7.3.2 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the wanted signal in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 3: The interferer consists of the NR interferer RMC specified in 3GPP TS 38.101-1 [5] Annex A.3.2.2 with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in 3GPP TS 38.101-1 [5] Annex A.5.1.1.  NOTE 4: Pinterferer shall be rounded to the next higher 0.5dB value. | | | | |

## 7.6 Blocking characteristics

### 7.6.1 General

The blocking characteristic is a measure of the receiver's ability to receive a wanted signal at its assigned channel frequency in the presence of an unwanted interferer on frequencies other than those of the spurious response or the adjacent channels, without this unwanted input signal causing a degradation of the performance of the receiver beyond a specified limit. The blocking performance shall apply at all frequencies except those at which a spurious response occurs.

### 7.6.2 In-band blocking

For NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz in-band blocking (IBB) is defined for an unwanted interfering signal falling into the UE receive band or into the first 15 MHz below or above the UE receive band.

The throughput of the wanted signal shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annexes A.2.2 and A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in Annex A.5.1.1) with parameters specified in Table 7.6.2-1 and Table 7.6.2-2. The relative throughput requirement shall be met for any SCS specified for the channel bandwidth of the wanted signal.

**Table 7.6.2-1: In-band blocking parameters for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RX parameter** | **Units** | **Channel bandwidth (MHz)** | | |
|  |  | **5, 10** | **15** | **20** |
| Power in transmission bandwidth configuration3 | dBm | REFSENS + 6 dB | REFSENS + 7 dB | REFSENS + 9 dB |
| BWinterferer | MHz | 5 | | |
| FIoffset, case 1 | MHz | 7.5 | | |
| FIoffset, case 2 | MHz | 12.5 | | |
| NOTE 1: The transmitter shall be set to 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in clause 7.3.2 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: The interferer consists of the RMC specified in 3GPP TS 38.101-1 [5] Annex A.3.2.2 with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in Annex A.5.1.1 and 15 kHz SCS.  NOTE 3: Power in transmission bandwidth configuration shall be rounded to the next higher 0.5dB value. | | | | |

Table 7.6.2-2: In-band blocking for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Parameter | Unit | Case 1 | Case 2 |
|  | Pinterferer | dBm | -56 | -44 |
| n255,  n256 | Finterferer (offset) | MHz | -BWChannel/2 –  FIoffset, case 1  and  BWChannel/2 +  FIoffset, case 1 | ≤ -BWChannel/2 –  FIoffset, case 2  and  ≥ BWChannel/2 +  FIoffset, case 2 |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15  to  FDL\_high + 15 |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the wanted signal in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWChannel/2 – FIoffset, case 1; b: BWChannel/2 + FIoffset, case 1 | | | | |

### 7.6.3 Out-of-band blocking

For NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz out-of-band band blocking is defined for an unwanted CW interfering signal falling outside a frequency range 15 MHz below or above the UE receive band.

The throughput of the wanted signal shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annexes A.2.2 and A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in Annex A.5.1.1) with parameters specified in Table 7.6.3-1 and Table 7.6.3-2. The relative throughput requirement shall be met for any SCS specified for the channel bandwidth of the wanted signal.

**Table 7.6.3-1: Out-of-band blocking parameters for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RX parameter** | **Units** | **Channel bandwidth (MHz)** | | |
|  |  | **5, 10** | **15** | **20** |
| Power in transmission bandwidth configuration2 | dBm | REFSENS + 6 dB | REFSENS + 7 dB | REFSENS + 9 dB |
| NOTE 1: The transmitter shall be set to 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in clause 7.3.2 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Power in transmission bandwidth configuration shall be rounded to the next higher 0.5dB value. | | | | |

Table 7.6.3-2: Out of-band blocking for NR satellite bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Operating Band | Parameter | Unit | Range 1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -44 | -30 | -15 |
| n255 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| n2561 | Finterferer (CW) | MHz | -100 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -145 < f – FDL\_low ≤ -100  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 145  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| NOTE 1: Band n256 lower frequency ranges are modified to enable specific implementations  NOTE 2: void  NOTE 3: void  NOTE 4: void | | | | | |

For interferer frequencies across ranges 1, 2 and 3 in Table 7.6.3-1, a maximum of



exceptions are allowed for spurious response frequencies in each assigned frequency channel when measured using a step size of MHz withthe number of resource blocks in the downlink transmission bandwidth configuration, BWChannelthe bandwidth of the frequency channel in MHz and *n* = 1, 2, 3 for SCS = 15, 30, 60 kHz, respectively. For these exceptions, the requirements in clause 7.7 apply.

### 7.6.4 Narrow band blocking

This requirement is measure of a receiver's ability to receive a NR signal at its assigned channel frequency in the presence of an unwanted narrow band CW interferer at a frequency, which is less than the nominal channel spacing. The relative throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annexes A.2.2 and A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in Annex A.5.1.1) with parameters specified in Table 7.6.4-1.

Table 7.6.4-1: Narrow Band Blocking

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Parameter | Unit | Channel Bandwidth (MHz) | | | |
|  |  |  | 5 | 10 | 15 | 20 |
| n255,  n256 | Pw | dBm | PREFSENS + channel-bandwidth specific value below | | | |
|  |  |  | 16 | 13 | 14 | 16 |
|  | Puw (CW) | dBm | -55 | | | |
|  | Fuw (offset SCS= 15 kHz) 3 | MHz |  | | | |
|  | Fuw (offset SCS= 30 kHz)3 | MHz | NA | | | |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in clause 7.3.2 with PCMAX\_L,f,c defined in clause 6.2.4  NOTE 2: The PREFSENS power level is specified in clause 7.3.2.  NOTE 3: Fuw shall be rounded to half of SCS. | | | | | | |

## 7.7 Spurious response

Spurious response is a measure of the ability of the receiver to receive a wanted signal on its assigned channel frequency without exceeding a given degradation due to the presence of an unwanted CW interfering signal at any other frequency for which a response is obtained, i.e. for which the out-of-band blocking limit as specified in clause 7.6.3 is not met.

The throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in 3GPP TS 38.101-1 [5] Annexes A.2.2 and A.3.2 (with one sided dynamic OCNG Pattern OP.1 FDD for the DL-signal as described in Annex A.5.1.1) with parameters for the wanted signal as specified in Table 7.7-1 for NR bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz for the interferer as specified in Table 7.7-2. The relative throughput requirement shall be met for any SCS specified for the channel bandwidth of the wanted signal.

Table 7.7-1: Spurious response parameters for NR bands with FDL\_high < 2700 MHz and FUL\_high < 2700 MHz

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RX parameter** | **Units** | **Channel bandwidth (MHz)** | | |
|  |  | **5, 10** | **15** | **20** |
| Power in transmission bandwidth configuration2 | dBm | REFSENS + 6 dB | REFSENS +  7 dB | REFSENS + 9 dB |
| NOTE 1: The transmitter shall be set to 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Power in transmission bandwidth configuration value is rounded to the next higher 0.5dB value. | | | | |

Table 7.7-2: Spurious response

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Level |
| PInterferer (CW) | dBm | -44 |
| FInterferer | MHz | Spurious response frequencies |

## 7.8 Intermodulation characteristics

The definition and requirements for intermodulation characteristics specified in 3GPP TS 38.101-1 [5] clause 7.8 shall apply for NTN satellite UE.

## 7.9 Spurious emissions

The spurious emissions power is the power of emissions generated or amplified in a receiver that appear at the UE antenna connector.

The power of any narrow band CW spurious emission shall not exceed the maximum level specified in Table 7.9-1

Table 7.9-1: General receiver spurious emission requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | Measurement  bandwidth | Maximum level | NOTE |
| 30 MHz ≤ f < 1 GHz | 100 kHz | -57 dBm |  |
| 1 GHz ≤ f ≤ 12.75 GHz | 1 MHz | -47 dBm |  |
| NOTE: Unused PDCCH resources are padded with resource element groups with power level given by PDCCH as defined in 3GPP TS 38.101-1 [5] Annex C.3.1. | | | |

# 8 Conducted performance requirements

## 8.1 General

### 8.1.1 Relationship between minimum requirements and test requirements

The present document is a Single-RAT and interwork specification for NR UE, covering minimum performance requirements of both conducted and radiated requirements. Conformance to the present specification is demonstrated by fulfilling the test requirements specified in the conformance specification TS TBD [TBD].

The Minimum Requirements given in this specification make no allowance for measurement uncertainty. The test specification TS TBD [TBD] defines test tolerances. These test tolerances are individually calculated for each test. The test tolerances are used to relax the minimum requirements in this specification to create test requirements.

The measurement results returned by the test system are compared – without any modification – against the test requirements as defined by the shared risk principle.

The shared risk principle is defined in Recommendation ITU‑R M.1545 [TBD].

The applicability of each requirement is described under each sub-clause in [8.2.1] and [8.3.1].

### 8.1.2 Applicability of minimum requirements

The conducted minimum requirements specified in this specification shall be met in all applicable scenarios for FR1.

Unless otherwise stated, all minimum performance requirements defined in Clauses 8 are applicable to UE power class 3 only.

### 8.1.3 Conducted requirements

#### 8.1.3.1 Introduction

The requirements are defined for the following modes:

- Mode 1: Conditions with external noise source

- Wanted signal with power level Es is transmitted.

- External white noise source with power spectral density Noc is used.

- *Es* and *Noc* levels are selected to achieve target SNR as described in Clause 8.1.3.3.

#### 8.1.3.2 Reference point

The reference point for SNR, Es and Noc of DL signal is the UE antenna connector or connectors.

#### 8.1.3.3 SNR definition

For Mode 1 conditions conducted UE demodulation and CSI requirements the SNR is defined as:

Where

- NRX denotes the number of receiver antenna connectors and the superscript receiver antenna connector *j*.

- The above SNR definition assumes that the REs are not precoded, and does not account for any gain which can be associated to the precoding operation.

- Unless otherwise stated, the SNR refers to the SSS wanted signal.

- The downlink SSS transmit power is defined as the linear average over the power contributions in [W] of all resource elements that carry the SSS within the operating system bandwidth.

- The power ratio of other wanted signals to the SSS is defined in clause [C.3.1].

#### 8.1.3.4 Noc

##### 8.1.3.4.1 Introduction

This clause describes the Noc power level for Mode 1 conditions conducted testing of demodulation and CSI requirements.

##### 8.1.3.4.2 Noc for NR operating bands in FR1

The Noc power spectrum density shall be larger or equal to the minimum Noc power level for each operating band supported by the UE as defined in clause 8.1.3.4.2.1.

Unless otherwise stated, a fixed Noc power level of -145 dBm/Hz shall be used for all operating bands.

8.1.3.4.2.1 Derivation of Noc values for NR operating bands in FR1

The minimum Noc power level for an operating band, subcarrier spacing and channel bandwidth is derived based on the following equation:

NocBand\_X, SCS\_Y, CBW\_Z = REFSENSBand\_X, SCS\_Y, CBW\_Z – 10\*log10(12\*SCS\_Y\*nPRB) + D – SNRREFSENS + ∆thermal

where

- REFSENSBand\_X, SCS\_Y, CBW\_Z is the REFSENS value in dBm for Band X, SCS Y and CBW Z specified in Table 7.3.2-1 of TS 38.101-5 [TBD]

- 12 is the number of subcarriers in a PRB

- SCS Y is the subcarrier spacing associated with the REFSENS value

- nPRB is the maximum number of PRB for SCS Y and CBW Z associated with the REFSENS value, and is specified in Table 5.3.2-1 of TS 38.101-5 [TBD]

- D is diversity gain equal to 3 dB

- SNRREFSENS = -1 dB is the SNR used for simulation of REFSENS

- ∆thermal is the amount of dB that the wanted noise is set above UE thermal noise, giving a defined rise in total noise. ∆thermal = 16dB, giving a rise in total noise of 0.1dB, regarded as insignificant**.**

The calculated Noc value for the baseline of Band n256, 15 kHz SCS, 10 MHz CBW is -146.5 dBm/Hz.

An allowance of 1.5dB is made for future bands, giving an Noc power level of -145 dBm/Hz.

## 8.2 Demodulation performance requirements

### 8.2.1 General

#### 8.2.1.1 Applicability of requirements

##### 8.2.1.1.1 General

The minimum performance requirements are applicable to all FR1 operating bands defined in clause 5.2.

If same test is listed for different UE features/capabilities in Clauses 8.2.1.1.2, then this test shall apply for UEs which support all corresponding UE features/capabilities.

##### 8.2.1.1.2 Applicability of requirements for optional UE features

The performance requirements in Table 8.2.1.1.2-1 shall apply for UEs which support optional UE features only.

Table 8.2.1.1.2-1: Requirements applicability for optional UE features

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE feature/capability [TBD] | Test type | | Test list | Applicability notes |
| NR NTN access (nonTerrestrialNetwork-r17) | FR1 FDD | PDSCH | Clause 8.2.1.2.2.1 (Test 1-1, Test 1-2, Test 1-3, Test 1-4) |  |
| NR NTN scenario support (ntn-ScenarioSupport-r17) | FR1 FDD | PDSCH | Clause 8.2.1.2.2.1 (Test 1-1, Test 1-2, Test 1-3, Test 1-4) | The requirements apply only when *ntn-ScenarioSupport-r17* is “ngso” or is not inculded. |
| Increasing the number of HARQ processes (max-HARQ-ProcessNumber-r17) | FR1 FDD | PDSCH | Clause 8.2.1.2.2.1 (Test 1-3) |  |
| Disabled HARQ feedback for downlink transmission (harq-FeedbackDisabled-r17) | FR1 FDD | PDSCH | Clause 8.2.1.2.2.1 (Test 1-4) |  |

#### 8.2.1.2 PDSCH demodulation requirements

The parameters specified in Table 8.2.1.2-1 are valid for all PDSCH tests unless otherwise stated.

Table 8.2.1.2-1: Common test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | | Unit | Value |
| PDSCH transmission scheme | | |  | Transmission scheme 1 |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 2) | | RBs | 0 |
| Subcarrier spacing | | kHz | 15 |
| DL BWP configuration #1 | Cyclic prefix | |  | Normal |
| RB offset | | RBs | 0 |
| Number of contiguous PRB | | PRBs | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing |
| Common serving cell parameters | Physical Cell ID | |  | 0 |
| SSB position in burst | |  | First SSB in Slot #0 |
| SSB periodicity | | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring | |  | Each slot |
| Symbols with PDCCH | | Symbols | 0, 1 |
| Number of PRBs in CORESET | |  | Table 5.2-2 of 38.101-4 for tested channel bandwidth and subcarrier spacing |
| Number of PDCCH candidates and aggregation levels | |  | 1/AL8 |
| CCE-to-REG mapping type | |  | Non-interleaved |
| DCI format | |  | 1\_1 |
| TCI state | |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration | |  | Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1 |
| Cross carrier scheduling | | |  | Not configured |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS | |  | k0=0 for CSI-RS resource 1,2,3,4 |
| First OFDM symbol in the PRB used for CSI-RS | |  | l0 = 6 for CSI-RS resource 1 and 3  l0 = 10 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (X) | |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type | |  | 'No CDM’ for CSI-RS resource 1,2,3,4 |
| Density (ρ) | |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | | Slots | 15 kHz SCS: 20 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | | Slots | 15 kHz SCS:  10 for CSI-RS resource 1 and 2  11 for CSI-RS resource 3 and 4 |
| Frequency Occupation | |  | Start PRB 0  Number of PRB = ceil(BWP size/4)\*4 |
| QCL info | |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | Row index (Note 3) | |  | 3 for 2 CSI-RS ports and 5 for 4 CSI-RS ports |
| First subcarrier index in the PRB used for CSI-RS | |  | k0 = 0 |
| First OFDM symbol in the PRB used for CSI-RS | |  | l0 = 12 |
| Number of CSI-RS ports (X) | |  | Same as number of transmit antenna |
| CDM Type | |  | 'No CDM' for 1 transmit antenna  'FD-CDM2' for 2 and 4 transmit antenna |
| Density (ρ) | |  | 1 |
| CSI-RS periodicity | | Slots | 15 kHz SCS: 20 |
| CSI-RS offset | | Slots | 0 |
| Frequency Occupation | |  | Start PRB 0  Number of PRB = ceil(BWP size/4)\*4 |
| QCL info | |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | Row index (Note 3) | |  | 5 |
| First subcarrier index in the PRB used for CSI-RS | |  | k0 = 4 |
| First OFDM symbol in the PRB used for CSI-RS | |  | l0 = 12 |
| Number of CSI-RS ports (X) | |  | 4 |
| CDM Type | |  | 'FD-CDM2' |
| Density (ρ) | |  | 1 |
| CSI-RS periodicity | | Slots | 15 kHz SCS: 20 |
| CSI-RS offset | | Slots | 0 |
| Frequency Occupation | |  | Start PRB 0  Number of PRB = ceil(BWP size/4)\*4 |
| PDSCH DMRS configuration | Antenna ports indexes | |  | {1000} for Rank 1 tests |
| Position of the first DMRS for PDSCH mapping type A | |  | 2 |
| Number of PDSCH DMRS CDM group(s) without data | |  | 1 for Rank 1 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | N/A |
| QCL Type |  | N/A |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | N/A |
| QCL Type |  | N/A |
| PT-RS configuration | | |  | PT-RS is not configured |
| Maximum number of code block groups for ACK/NACK feedback | | |  | 1 |
| Maximum number of HARQ transmission | | |  | 4 |
| HARQ ACK/NACK bundling | | |  | Multiplexed |
| Redundancy version coding sequence | | |  | {0,2,3,1} |
| PDSCH & PDSCH DMRS Precoding configuration | | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with PRB bundling granularity |
| Symbols for all unused REs | | |  | OP.1 FDD as defined in Annex A.5.1.1 of 38.101-4 |
| Physical signals, channels mapping and precoding | | |  | As specified in Annex B.4.1 of 38.101-4 |
| Note 1: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.  Note 2: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing.  Note 3: Refer to Table 7.4.1.5.3-1 in [9] | | | | |

##### 8.2.1.2.1 1RX requirements

#### 8.2.1.2.2 2RX requirements

8.2.1.2.2.1 FDD

8.2.1.2.2.1.1 Minimum requirements for PDSCH Mapping Type A

The performance requirements are specified in Table 8.2.1.2.2.1.1-3 with the addition of test parameters in Table 8.2.1.2.2.1.1-2 and the downlink physical channel setup according to Annex A.3.

The test purposes are specified in Table 8.2.1.2.2.1.1-1.

Table 8.2.1.2.2.1.1-1: Tests purpose

|  |  |
| --- | --- |
| Purpose | Test index |
| Verify the PDSCH mapping Type A normal performance under 2 receive antenna conditions and with different channel models and MCS | 1-1, 1-2, 1-3, 1-4 |

Table 8.2.1.2.2.1.1-2: Test parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Value |
| Duplex mode | |  | FDD |
| Active DL BWP index | |  | 1 |
| PDSCH configuration | Mapping type |  | Type A |
|  | k0 |  | 0 |
|  | Starting symbol (S) |  | 2 |
|  | Length (L) |  | 12 |
|  | PDSCH aggregation factor |  | 1 |
|  | PRB bundling type |  | Static |
|  | PRB bundling size |  | 2 |
|  | Resource allocation type |  | Type 0 |
|  | RBG size |  | Config2 |
|  | VRB-to-PRB mapping type |  | Non-interleaved |
|  | VRB-to-PRB mapping interleaver bundle size |  | N/A |
| PDSCH DMRS configuration | DMRS Type |  | Type 1 |
|  | Number of additional DMRS |  | 1 |
|  | Maximum number of OFDM symbols for DL front loaded DMRS |  | 1 |
| CSI-RS for tracking | CSI-RS periodicity | Slots | 20 for CSI-RS resource 1,2,3,4. |
|  | CSI-RS offset | Slots | 10 for CSI-RS resource 1 and 2 11 for CSI-RS resource 3 and 4. |
| Number of HARQ Processes | |  | 16 for Test 1-1, Test 1-2 32 for Test 1-3  4 with feedback disabled, 12 with feedback enabled in 16 HARQ processes with re-Tx disable for all HARQ for Test 1-4 in which 4 disabled processes are randomly select at test configuration |
| The number of slots between PDSCH and corresponding HARQ-ACK information | |  | 10 for Test 1-1, Test 1-2, Test 1-3 N/A for Test 1-4 |
| Maximum number of HARQ transmission | |  | 4 for Test 1-1, Test 1-2, Test 1-3  Disabled for all HARQ processes  for Test 1-4 |

Table 8.2.1.2.2.1.1-3: Minimum performance for Rank 1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Test num. | Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Modulation format and code rate | Propagation condition | Correlation matrix and antenna configuration | Reference value | |
|  |  |  |  |  |  | Fraction of maximum throughput (%) | SNR (dB) |
| 1-1 | R.PDSCH.1-1.1 FDD | 10 / 15 | QPSK, 0.30 | NTN-TDLA100-200 | 1x2, ULA Low | 70 | [0.3] |
| 1-2 | R.PDSCH.1-2.1 FDD | 10 / 15 | 16QAM, 0.48 | NTN-TDLC5-200 | 1x2, ULA Low | 70 | [7.6] |
| 1-3 | R.PDSCH.1-1.1 FDD | 10 / 15 | QPSK, 0.30 | NTN-TDLC5-200 | 1x2, ULA Low | 70 | [-0.4] |
| 1-4 | R.PDSCH.1-1.1 FDD | 10 / 15 | QPSK, 0.30 | NTN-TDLA100-200 | 1x2, ULA Low | 70\* | [1.1] |

## 8.3 CSI reporting requirements

[To be updated]

Annex A (normative):  
Measurement channels

# A.1 General

## A.1.1 Throughput definition

The throughput values defined in the measurement channels specified in Annex A, are calculated and are valid per codeword. For multi-codeword transmissions, the throughput referenced in the minimum requirements is the sum of throughputs of all codewords.

# A.2 UL reference measurement channels

# A.3 DL reference measurement channels

## A.3.1 General

The transport block size (TBS) determination procedure is described in clause 5.1.3.2 of TS 38.214 [12].

Unless otherwise stated, no user data is scheduled on slot #0 within 20 ms in order to avoid SSB and PDSCH transmissions in one slot and simplify test configuration.

## A.3.2 Reference measurement channels for PDSCH performance requirements

For PDSCH reference channels if more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit).

### A.3.2.1 FDD

#### A.3.2.1.1 Reference measurement channels for SCS 15 kHz FR1

Table A.3.2.1.1-1: PDSCH Reference Channel for FDD (QPSK)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Value | | | | |
| Reference channel |  | R.PDSCH.1-1.1 FDD |  |  |  |  |
| Channel bandwidth | MHz | 10 |  |  |  |  |
| Subcarrier spacing | kHz | 15 |  |  |  |  |
| Number of allocated resource blocks | PRBs | 52 |  |  |  |  |
| Number of consecutive PDSCH symbols |  | 12 |  |  |  |  |
| Allocated slots per 2 frames | Slots | 19 |  |  |  |  |
| MCS table |  | 64QAM |  |  |  |  |
| MCS index |  | 4 |  |  |  |  |
| Modulation |  | QPSK |  |  |  |  |
| Target Coding Rate |  | 0.30 |  |  |  |  |
| Number of MIMO layers |  | 1 |  |  |  |  |
| Number of DMRS REs |  | 18 |  |  |  |  |
| Overhead for TBS determination |  | 0 |  |  |  |  |
| Information Bit Payload per Slot |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |
| For Slots i = 1,…, 19 | Bits | 3904 |  |  |  |  |
| Transport block CRC per Slot |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |
| For Slots i = 1,…, 19 | Bits | 24 |  |  |  |  |
| Number of Code Blocks per Slot |  |  |  |  |  |  |
| For Slot i = 0 | CBs | N/A |  |  |  |  |
| For Slots i = 1,…, 19 | CBs | 1 |  |  |  |  |
| Binary Channel Bits Per Slot |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |
| For Slots i = 10, 11 | Bits | 12480 |  |  |  |  |
| For Slots i =1,…, 9, 12, …, 19 | Bits | 13104 |  |  |  |  |
| Max. Throughput averaged over 2 frames | Mbps | 3.709 |  |  |  |  |
| Note 1: SS/PBCH block is transmitted in slot #0 with periodicity 20 ms  Note 2: Slot i is slot index per 2 frames | | | | | | |

Table A.3.2.1.1-2: PDSCH Reference Channel for FDD (16QAM)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Value | | | | |  |
| Reference channel |  | R.PDSCH.1-2.1 FDD |  |  |  |  |  |
| Channel bandwidth | MHz | 10 |  |  |  |  |  |
| Subcarrier spacing | kHz | 15 |  |  |  |  |  |
| Number of allocated resource blocks | PRBs | 52 |  |  |  |  |  |
| Number of consecutive PDSCH symbols |  | 12 |  |  |  |  |  |
| Allocated slots per 2 frames | Slots | 19 |  |  |  |  |  |
| MCS table |  | 64QAM |  |  |  |  |  |
| MCS index |  | 13 |  |  |  |  |  |
| Modulation |  | 16QAM |  |  |  |  |  |
| Target Coding Rate |  | 0.48 |  |  |  |  |  |
| Number of MIMO layers |  | 1 |  |  |  |  |  |
| Number of DMRS REs |  | 12 |  |  |  |  |  |
| Overhead for TBS determination |  | 0 |  |  |  |  |  |
| Information Bit Payload per Slot |  |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |  |
| For Slots i = 1,…, 19 | Bits | 13064 |  |  |  |  |  |
| Transport block CRC per Slot |  |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |  |
| For Slots i = 1,…, 19 | Bits | 24 |  |  |  |  |  |
| Number of Code Blocks per Slot |  |  |  |  |  |  |  |
| For Slot i = 0 | CBs | N/A |  |  |  |  |  |
| For Slots i = 1,…, 19 | CBs | 2 |  |  |  |  |  |
| Binary Channel Bits Per Slot |  |  |  |  |  |  |  |
| For Slot i = 0 | Bits | N/A |  |  |  |  |  |
| For Slots i = 10, 11 | Bits | 26208 |  |  |  |  |  |
| For Slots i = 1,…, 9, 12, …, 19 | Bits | 27456 |  |  |  |  |  |
| Max. Throughput averaged over 2 frames | Mbps | 12.411 |  |  |  |  |  |
| Note 1: SS/PBCH block is transmitted in slot #0 with periodicity 20 ms  Note 2: Slot i is slot index per 2 frames | | | | | | | |

Annex B (normative):  
Propagation conditions

# B.1 Static propagation condition

## B.1.1 UE Receiver with 1Rx

For 2 port transmission the channel matrix is defined in the frequency domain by

.

## B.1.2 UE Receiver with 2Rx

For 1 port transmission the channel matrix is defined in the frequency domain by

.

For 2 port transmission the channel matrix is defined in the frequency domain by

.

B.2 Multi-path fading propagation conditions

The multipath propagation conditions consist of several parts:

- A delay profile in the form of a "tapped delay-line", characterized by a number of taps at fixed positions on a sampling grid. The profile can be further characterized by the r.m.s. delay spread and the maximum delay spanned by the taps.

- A combination of channel model parameters that include the Delay profile and the Doppler spectrum that is characterized by a classical spectrum shape and a maximum Doppler frequency.

Initial channel matrix for LOS component of NTN-TDL-C channel model is equal to channel matrix of Static propagation conditions in Clause B.1.

## B.2.1 Delay profiles

The delay profiles are derived from the TR 38.811 [x] NTN-TDL models for the desired delay spread and tap resolution. After scaling the normalized delay spread values for each tap by the desired RMS delay spread, the tap delays are quantized to a delay resolution of 5ns by rounding to the nearest multiple of the delay resolution.

**Table B.2.1-1: Delay profiles for NR NTN channel models**

|  |  |  |  |
| --- | --- | --- | --- |
| Type | Model | Delay spread (r.m.s.) | Delay resolution |
| NLOS | NTN-TDLA100 | 100 ns | 5 ns |
| LOS | NTN-TDLC5 | 5 ns | 5 ns |

**Table B.2.1-2: NTN-TDLA100 (DS = 100 ns)**

|  |  |  |  |
| --- | --- | --- | --- |
| Tap # | Delay [ns] | Power [dB] | Fading distribution |
| 1 | 0 | 0 | Rayleigh |
| 2 | 110 | -4.7 | Rayleigh |
| 3 | 285 | -6.5 | Rayleigh |

**Table B.2.1-3 NTN-TDLC5 (DS = 5 ns)**

|  |  |  |  |
| --- | --- | --- | --- |
| Tap # | Delay [ns] | Power [dB] | Fading distribution |
| 1 | 0 | -0.6 | LOS path |
| 0 | -8.9 | Rayleigh |
| 2 | 60 | -21.5 | Rayleigh |
| Note 1: Tap #1 follows a Rician distribution. | | | |

## B.2.2 Combinations of channel model parameters

The propagation conditions used for the performance measurements in multi-path fading environment are indicated as a combination of a channel model name and a maximum Doppler frequency, i.e., NTN-TDLA<DS>-<Doppler>, or NTN-TDLC<DS>-<Doppler> where '<DS>' indicates the desired delay spread and '<Doppler>' indicates the maximum Doppler frequency (Hz).

Table B.2.2-1 show the propagation conditions that are used for the performance measurements in multi-path fading environment for NLOS and LOS propagation conditions.

Table B.2.2-1: Channel model parameters for NTN

|  |  |  |
| --- | --- | --- |
| Combination name | Model | Maximum Doppler frequency |
| NTN-TDLA100-200 | NTN-TDLA100 | 200 Hz |
| NTN-TDLC5-200 | NTN-TDLC5 | 200 Hz |

## B.2.3 MIMO Channel Correlation Matrices

The MIMO channel correlation matrices defined in B.2.3 apply for the antenna configuration using uniform linear arrays at both gNB and UE.

### B.2.3.1 MIMO Correlation Matrices using Uniform Linear Array (ULA)

The MIMO channel correlation matrices defined in B.2.3.1 apply for the antenna configuration using uniform linear array (ULA) at both gNB and UE.

#### B.2.3.1.1 Definition of MIMO Correlation Matrices

Table B.2.3.1.1-1 defines the correlation matrix for the gNB.

Table B.2.3.1.1-1: gNB correlation matrix

|  |  |  |
| --- | --- | --- |
|  | One antenna | Two antennas |
| gNB Correlation |  |  |

Table B.2.3.1.1-2 defines the correlation matrix for the UE:

Table B.2.3.1.1-2: UE correlation matrix

|  |  |  |
| --- | --- | --- |
|  | One antenna | Two antennas |
| UE Correlation |  |  |

Table B.2.3.1.1-3 defines the channel spatial correlation matrix. The parameters, *α* and *β* in Table B.2.3.1-3 defines the spatial correlation between the antennas at the gNB and UE.

Table B.2.3.1.1-3: correlation matrices

|  |  |
| --- | --- |
| 1x2 case |  |
| 2x1 case |  |
| 2x2 case |  |

#### B.2.3.1.2 MIMO Correlation Matrices at High, Medium and Low Level

The *α* and *β* for different correlation types are given in Table B.2.3.1.2-1.

Table B.2.3.1.2-1: The *α* and *β* parameters for ULA MIMO correlation matrices

|  |  |  |
| --- | --- | --- |
| Correlation Model | α | β |
| Low correlation | 0 | 0 |

The correlation matrices low correlation are defined in Table B.2.3.1.2-2 below.

Table B.2.3.1.2-2: MIMO correlation matrices for low correlation

|  |  |
| --- | --- |
| 1x2 case |  |
| 2x1 case |  |
| 2x2 case |  |
| Note: **I**d is the *d*×*d* identity matrix. | |

Annex C (normative):  
Downlink physical channels

# C.1 General

This annex specifies the downlink physical channels that are needed for setting a connection and channels that are needed during a connection.

# C.2 Setup (Conducted)

Table C.2-1 describes the downlink Physical Channels that are required for connection set up.

Table C.2-1: Downlink Physical Channels required for connection set-up

|  |
| --- |
| Physical Channel |
| PBCH |
| SSS |
| PSS |
| PDCCH |
| PDSCH |
| PBCH DMRS |
| PDCCH DMRS |
| PDSCH DMRS |
| CSI-RS |

# C.3 Connection (Conducted)

The following clauses, describes the downlink Physical Channels that are transmitted during a connection i.e., when measurements are done.

## C.3.1 Measurement of Performance requirements

Table C.3.1-1 is applicable for measurements in which uniform RS-to-EPRE boosting for all downlink physical channels, unless otherwise stated.

Table C.3.1-1: Downlink Physical Channels transmitted during a connection (FDD and TDD)

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value (Note 2) |
| SSS transmit power | W | Test specific |
| EPRE ratio of PSS to SSS | dB | 0 |
| EPRE ratio of PBCH to SSS | dB | 0 |
| EPRE ratio of PBCH to PBCH DMRS | dB | 0 |
| EPRE ratio of PDCCH to SSS | dB | 0 |
| EPRE ratio of PDCCH to PDCCH DMRS | dB | 0 |
| EPRE ratio of PDSCH to SSS | dB | 0 |
| EPRE ratio of PDSCH to PDSCH DMRS | dB | Test specific (Note 1) |
| EPRE ratio of CSI-RS to SSS | dB | -10\*log10(L) (Note 3) |
| EPRE ratio of OCNG to SSS | dB | 0 |
| EPRE ratio of PDCCH OCNG to SSS | dB | 0 |
| EPRE ratio of LTE CRS to NR SSS | dB | 0 (Note 4) |
| Note 1: Value is derived from Table 4.1-1 in TS 38.214 [12] based on "Number of DM-RS CDM groups without data" and "DMRS Type" parameters specified for each test.  Note 2: The value is the energy of per RE for a single antenna port before pre-coding.  Note 3:  is the CDM group size of NZP CSI-RS specified for each test.  Note 4: It is only applicable to LTE-NR coexistence tests. | | |

Annex D (informative): Void

Annex E (normative):  
Environmental conditions

# E.1 General

This annex specifies the environmental requirements of the UE. Within these limits the requirements of the present documents shall be fulfilled.

# E.2 Environmental (Conducted)

The requirements in this clause apply to all types of UE(s).

## E.2.1 Temperature

The UE shall fulfil all the requirements in the temperature range defined in Table E.2.1-1.

Table E.2.1-1: Temperature conditions

|  |  |
| --- | --- |
| Temperature | Temperature conditions |
| +15°C to +35°C | For normal conditions (with relative humidity of 25 % to 75 %) |

Outside this temperature range the UE, if powered on, shall not make ineffective use of the radio frequency spectrum. In no case shall the UE exceed the transmitted levels as defined in clause 6.2 of TS 38.101-1 [6] for extreme operation.

## E.2.2 Voltage

The UE shall fulfil all the requirements in the voltage range defined in Table E.2.2-1.

Table E.2.2-1: Voltage conditions

|  |  |
| --- | --- |
| Power source | Normal conditions  voltage |
| AC mains | nominal |
| Regulated lead acid battery | 1,1 \* nominal |
| Non regulated batteries:  Leclanché  Lithium  Mercury/nickel & cadmium | Nominal  1,1 \* Nominal  Nominal |

Outside this voltage range the UE if powered on, shall not make ineffective use of the radio frequency spectrum. In no case shall the UE exceed the transmitted levels as defined in TS 38.101-1[6, Clause 6.2] for extreme operation. In particular, the UE shall inhibit all RF transmissions when the power supply voltage is below the manufacturer declared shutdown voltage.

## E.2.3 Vibration

The UE shall fulfil all the requirements when vibrated at the following frequency/amplitudes.

Table E.2.3-1: Vibration conditions

|  |  |
| --- | --- |
| Frequency | ASD (Acceleration Spectral Density) random vibration |
| 5 Hz to 20 Hz | 0,96 m2/s3 |
| 20 Hz to 500 Hz | 0,96 m2/s3 at 20 Hz, thereafter –3 dB/Octave |

Outside the specified frequency range the UE, if powered on, shall not make ineffective use of the radio frequency spectrum. In no case shall the UE exceed the transmitted levels as defined in TS 38.101-1[6] for extreme operation.

Annex F (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-01 | RAN4#101-bis-e | R4-2203086 |  |  |  | Draft skeleton approved | 0.0.1 |
| 2022-03 | RAN4#102-e | R4-2207514 |  |  |  | Added approved TPs in RAN4#102-e including:  R4-2207332, R4-2207334, R4-2207343, R4-2207344, R4-2207391, R4-2207393, R4-2207394, R4-2207396, R4-2207400, R4-2207404, R4-2207405, R4-2207410, R4-2207411, R4-2207413, R4-2207415 | 0.1.0 |
| 2022-05 | RAN4#103-e | R4-2208641 |  |  |  | Added approved TPs in RAN4#103-e including:  R4-2208662, TP to TS 38.101-5 on Conducted transmitter characteristics  R4-2209366, TP for 38.101-5 on Output RF spectrum emissions for satellite UE except for UE coexistence  R4-2210851, Draft text proposal for Clause 3 - TS 38.101-5  R4-2210874, TP to TS 38.101-5 on 7.3 Reference Sensitivity  R4-2210876, Updates to TS 38.101-5 related to n255 A-MPR clause  R4-2210877, TP for 38.101-5 on Spurious emissions for UE coexistence  R4-2210878, TP to update TS 38.101-5 clause 7.6.3 on OOBB  R4-2211220, TP for 38.101-5 on frequency error | 0.2.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-06 | RAN#96 |  |  |  |  | Approved by plenary – Rel-17 spec under change control | 17.0.0 |
| 2022-09 | RAN#97 | RP-222035 | 0001 | 1 | F | CR to 38.101-5: Corrections on Rx requirements for NTN UE | 17.1.0 |
| 2022-09 | RAN#97 | RP-222035 | 0002 |  | F | CR to TS 38.101-5 - Tx requirements issues fixes | 17.1.0 |
| 2022-09 | RAN#97 | RP-222035 | 0003 | 1 | F | CR to TS 38.101-5 - Rx requirements issues fixes | 17.1.0 |
| 2022-12 | RAN#98-e | RP-223306 | 0005 | 1 | F | CR: 0005 Doppler test conditions for RF requirements 38.101-5 | 17.2.0 |
| 2022-12 | RAN#98-e | RP-223306 | 0006 |  | F | CR to 38.101-5: Corrections on section 5.3.3 for NTN UE | 17.2.0 |
| 2022-12 | RAN#98-e | RP-223311 | 0010 | 2 | F | CR to 38.101-5 for NTN UE RF requirements corrections | 17.2.0 |
| 2022-12 | RAN#98-e | RP-223309 | 0012 |  | F | CR addition of protection for n100 and n101 into 38.101-5 | 17.2.0 |
| 2022-12 | RAN#98-e | RP-223311 | 0013 |  | F | CR to 38.101-5: Corrections on reference for NTN UE | 17.2.0 |
| 2022-12 | RAN#98-e | RP-223303 | 0015 |  | B | Big CR for UE NTN performance requirements (TS38.101-5, Rel-17, CAT B) | 17.2.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-12 | RAN#98-e | RP-223315 | 0009 | 1 | B | CR related to Introduction of LTE TDD Band in 1670 – 1675 MHz | 18.0.0 |
| 2023-03 | RAN#99 | RP-230535 | 0016 |  | B | CR related to Introduction of NR TDD Band n54 | 18.1.0 |
| 2023-03 | RAN#99 | RP-230516 | 0018 | 1 | A | Correction of the out-of-band blocking requirements | 18.1.0 |
| 2023-06 | RAN#100 | RP-231344 | 0026 |  | A | Correction to reference measurement channels for NTN | 18.2.0 |