|  |  |
| --- | --- |
| 3GPP TS 38.113 V18.2.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  Base Station (BS) ElectroMagnetic Compatibility (EMC)  (Release 18) | |
|  | |
|  | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 7

1 Scope 9

2 References 9

3 Definitions, symbols and abbreviations 11

3.1 Definitions 11

3.2 Symbols 13

3.3 Abbreviations 14

4 Test conditions 14

4.1 General 14

4.2 Arrangements for establishing a communication link 15

4.3 Narrow band responses on receivers 15

4.4 Exclusion bands 16

4.4.1 Transmitter exclusion band 16

4.4.2 Receiver exclusion band 16

4.5 BS test configurations 17

4.6 Manufacturer declarations 18

5 Performance assessment 18

5.1 General 18

5.2 Assessment of throughput in Downlink 18

5.3 Assessment of throughput in Uplink 19

5.4 Ancillary equipment 19

6 Performance criteria 19

6.1 Performance criteria for continuous phenomena for BS 19

6.2 Performance criteria for transient phenomena for BS 21

6.3 Performance criteria for continuous phenomena for Ancillary equipment 21

6.4 Performance criteria for transient phenomena for Ancillary equipment 22

7 Applicability overview 22

7.1 Emission 22

7.2 Immunity 23

8 Emission 24

8.1 Test configurations 24

8.1.1 (Void) 24

8.1.2 (Void) 24

8.1.3 (Void) 24

8.1.4 (Void) 24

8.1.5 (Void) 24

8.2 Radiated emission 24

8.2.1 Radiated emission, BS 24

8.2.1.1 Definition 25

8.2.1.2 Test method 25

8.2.1.3 Limits 25

8.2.1.4 Interpretation of the measurement results 26

8.2.2 Radiated emission, ancillary equipment 27

8.2.2.1 Definition 27

8.2.2.2 Test method 27

8.2.2.3 Limits 27

8.3 Conducted emission DC power input/output port 28

8.3.1 Definition 28

8.3.2 Test method 28

8.3.3 Limits 28

8.4 Conducted emissions, AC mains power input/output port 28

8.4.1 Definition 29

8.4.2 Test method 29

8.4.3 Limits 29

8.5 Conducted emissions, telecommunication port 29

8.5.1 Definition 29

8.5.2 Test method 29

8.5.3 Limits 29

8.6 Harmonic current emissions (AC mains input port) 30

8.7 Voltage fluctuations and flicker (AC mains input port) 30

9 Immunity 30

9.1 Test configurations 30

9.1.1 (Void) 31

9.1.2 (Void) 31

9.1.3 (Void) 31

9.1.4 (Void) 31

9.1.5 (Void) 31

9.2 RF electromagnetic field (80 MHz to 6000 MHz) 31

9.2.1 Definition 31

9.2.2 Test method and level 31

9.2.3 Performance criteria 32

9.3 Electrostatic discharge 32

9.3.1 Definition 32

9.3.2 Test method and level 33

9.3.3 Performance criteria 33

9.4 Fast transients common mode 33

9.4.1 Definition 33

9.4.2 Test method and level 33

9.4.3 Performance criteria 33

9.5 RF common mode (0.15 MHz - 80 MHz) 34

9.5.1 Definition 34

9.5.2 Test method and level 34

9.5.3 Performance criteria 34

9.6 Voltage dips and interruptions 34

9.6.1 Definition 35

9.6.2 Test method and level 35

9.6.3 Performance criteria 35

9.7 Surges, common and differential mode 35

9.7.1 Definition 35

9.7.2 Test method and level 36

9.7.2.1 Test method for telecommunication ports directly connected to outdoor cables 36

9.7.2.2 Test method for telecommunication ports connected to indoor cables 36

9.7.2.3 Test method for AC power ports 36

9.7.3 Performance criteria 36

Annex A (informative): Change history 37

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document covers the assessment of NR and NR with NB-IoT in-band operation Base Station (BS) and ancillary equipment in respect of Electromagnetic Compatibility (EMC).

The present document specifies the applicable requirements, procedures, test conditions, performance assessment and performance criteria for NR and NR with NB-IoT in-band operation base stations and associated ancillary equipment in the following categories:

- BS equipped with antenna connectors or *TAB connectors* which are possible to be terminated during EMC testing, meeting the *BS type 1-C* and *BS type* *1-H* RF requirements of TS 38.104 [2], with conformance demonstrated by compliance to TS 38.141-1 [3].

- BS not equipped with antenna connectors nor *TAB connectors*, i.e. with antenna elements radiating during the EMC testing, meeting the *BS type 1-O* and *BS type* *2-O* RF requirements of TS 38.104 [2], with conformance demonstrated by compliance to TS 38.141-2 [4].

Technical requirements related to the antenna and *TAB connectors* are not included in the present document. These are found in the relevant NR BS product standards TS 38.104 [2], 3GPP TS 38.141-1[3], and 3GPP TS 38.141-2 [4].

The environment classification used in the present document refers to the residential, commercial and light industrial environment classification used in IEC 61000‑6-1 [7], IEC 61000-6-3 [8] and IEC 61000-6-8 [33].

The EMC requirements have been selected to ensure an adequate level of compatibility for apparatus at residential, commercial and light industrial environments. The levels, however, do not cover extreme cases which may occur in any location but with low probability of occurrence.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception".

[3] 3GPP TS 38.141-1: "NR; Base Station (BS) conformance testing Part 1: Conducted conformance testing".

[4] 3GPP TS 38.141-2: "NR; Base Station (BS) conformance testing Part 2: Radiated conformance testing".

[5] 3GPP TS 37.113: "E-UTRA, UTRA and GSM/EDGE; Multi-Standard Radio (MSR) Base Station (BS) Electromagnetic Compatibility (EMC)".

[6] 3GPP TS 37.114: "Active Antenna System (AAS) Base Station (BS) Electromagnetic Compatibility (EMC)".

[7] IEC 61000-6-1: "Electromagnetic compatibility (EMC) - Part 6-1: Generic standards - Immunity for residential, commercial and light-industrial environments".

[8] IEC 61000-6-3: "Electromagnetic compatibility (EMC) - Part 6-3: Generic standards - Emission standard for equipment in residential environments".

[9] IEC 60050-161: "International Electrotechnical Vocabulary (IEV) - Part 161: Electromagnetic compatibility".

[10] void

[11] CISPR 32: "Electromagnetic compatibility of multimedia equipment - Emission requirements".

[12] void

[13] IEC 61000-3-2: "Electromagnetic compatibility (EMC) - Part 3-2: Limits - Limits for harmonic current emissions (equipment input current ≤ 16 A per phase)".

[14] IEC 61000-3-12: "Electromagnetic compatibility (EMC) - Part 3-12: Limits - Limits for harmonic currents produced by equipment connected to public low-voltage system with input current >16 A and ≤ 75 A per phase".

[15] IEC 61000-3-3: "Electromagnetic compatibility (EMC) - Part 3-3: Limits - Limitation of voltage changes, voltage fluctuations and flicker in low-voltage supply systems, for equipment with rated current ≤ 16 A per phase and not subject to conditional connection".

[16] IEC 61000-3-11: "Electromagnetic compatibility (EMC) - Part 3-11: Limits – Limitation of voltage changes, voltage fluctuations and flicker in low-voltage supply systems - Equipment with rated current ≤ 75 A and subject to conditional connections".

[17] IEC 61000-4-2: "Electromagnetic compatibility (EMC) - Part 4-2: Testing and measurement techniques - Electrostatic discharge immunity test".

[18] IEC 61000-4-3:2006+AMD1:2007+AMD2:2010 CSV: "Electromagnetic compatibility (EMC) - Part 4-3: Testing and measurement techniques - Radiated, radio-frequency, electromagnetic field immunity test".

[19] IEC 61000-4-4: "Electromagnetic compatibility (EMC) - Part 4-4: Testing and measurement techniques - Electrical fast transient/burst immunity test".

[20] IEC 61000-4-5: "Electromagnetic compatibility (EMC) - Part 4-5: Testing and measurement techniques - Surge immunity test".

[21] IEC 61000-4-6: "Electromagnetic compatibility (EMC) - Part 4-6: Testing and measurement techniques - Immunity to conducted disturbances, induced by radio frequency fields".

[22] IEC 61000-4-11: "Electromagnetic compatibility (EMC) - Part 4-11: Testing and measurement techniques - Voltage dips, short interruptions and voltage variations immunity tests".

[23] ETSI EN 301 489-1: "ElectroMagnetic Compatibility (EMC) standard for radio equipment and services; Part 1: Common technical requirements; Harmonised Standard covering the essential requirements of article 3.1(b) of Directive 2014/53/EU and the essential requirements of article 6 of Directive 2014/30/EU".

[24] Recommendation ITU-R SM.329-12: "Unwanted emissions in the spurious domain".

[25] 3GPP TS 37.105: "Active Antenna System (AAS) Base Station (BS) transmission and reception".

[26] Recommendation ITU-R SM.1539-1: "Variation of the boundary between the out-of-band and spurious domains required for the application of Recommendations ITU-R SM.1541 and ITU-R SM.329".

[27] 3GPP TS 38.101-4: "NR; User Equipment (UE) radio transmission and reception; Part 4: Performance requirements".

[28] ETSI EN 301 489-50: "Electromagnetic compatibility (EMC) standard for radio equipment and services; Part 50: Specific conditions for cellular communication base station (BS), repeater and ancillary equipment; Harmonised standard covering the essential requirements of article 3.1(b) of the Directive 2014/53/EU".

[29] IEC 61000-4-21: "Electromagnetic compatibility (EMC) - Part 4-21: Testing and measurement techniques - Reverberation chamber test methods".

[30] CISPR 16-1-4: 2019-01: "Specification for radio disturbance and immunity measuring apparatus and methods – Part 1-4: Radio disturbance and immunity measuring apparatus – Antennas and test sites for radiated disturbance measurements"

[31] CISPR 16-4-2: " Specification for radio disturbance and immunity measuring apparatus and methods - Part 4-2: Uncertainties, statistics and limit modelling - Measurement instrumentation uncertainty, Amendment 2"

[32] ETSI TR 100 028-1: "Electromagnetic compatibility and Radio spectrum Matters (ERM); Uncertainties in the measurement of mobile radio equipment characteristics, part 1"

[33] IEC 61000-6-8:"Electromagnetic compatibility (EMC) - Part 6-8: Generic standards - Emission standard for professional equipment in commercial and light-industrial locations".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**ancillary equipment:** electrical or electronic equipment, that is intended to be used with a receiver or transmitter

NOTE: It is considered as an ancillary equipment if:

the equipment is intended for use with a receiver or transmitter to provide additional operational and/or control features to the radio equipment, (e.g. to extend control to another position or location); and

the equipment cannot be used on a stand alone basis to provide user functions independently of a receiver or transmitter; and

the receiver or transmitter, to which it is connected, is capable of providing some intended operation such as transmitting and/or receiving without the ancillary equipment (i.e. it is not a sub-unit of the main equipment essential to the main equipment basic functions).

**antenna port:** for EMC purposes, port for connection of an antenna used for intentional transmission and/or reception of radiated RF energy, equivalent to an RF antenna connector/*TAB connector* in TS 37.105 [25].

**BS type 1-C:** NR base station operating at FR1 with requirements set consisting only of conducted requirements defined at individual antenna connectors.

**BS type 1-H:** NR base station operating at FR1 with a requirement set consisting of conducted requirements defined at individual *TAB connectors* and OTA requirements defined at RIB.

**BS type 1-O:** NR base station operating at FR1 with a requirement set consisting only of OTA requirements defined at the RIB.

**BS type 2-O:** NR base station operating at FR2 with a requirement set consisting only of OTA requirements defined at the RIB.

**channel bandwidth:** the RF bandwidth supporting a single NR RF carrier with the transmission bandwidth configured in the uplink or downlink of a cell. The *channel bandwidth* is measured in MHz and is used as a reference for transmitter and receiver RF requirements.

**continuous phenomena:** electromagnetic disturbance, the effects of which on a particular device or equipment cannot be resolved into a succession of distinct effects (IEC 60050-161 [9]).

**enclosure port:** physical boundary of the equipment through which electromagnetic fields may radiate or impinge.

NOTE: In the case of *integral antenna* equipment, this port is inseparable from the antenna port.

**exclusion band:** frequency range(s) not subject to test or assessment.

**free-space open area test site:** reference test site with precautions to ensure that reflections do not influence the measurement.

NOTE: The free-space open area test site (FSOATS) is the concept of the test site. A practical approximation is a Fully-Anechoic Room (FAR).

**fully-anechoic room:** shielded enclosure, the internal surfaces of which are lined with radio-frequency-energy absorbing material (i.e. RF absorber) that absorbs electromagnetic energy in the frequency range of interest.

**integral antenna:** antenna designed for permanent connection to the equipment and considered part of the enclosure port.

NOTE: An *integral antenna* may be fitted internally or externally.

**lower RF bandwidth edge:** the frequency of the lower edge of the Base Station RF bandwidth, used as a frequency reference point for transmitter and receiver requirements.

**NB-IoT operation in NR in-band:** NB-IoT is operating in-band when it is located within a NR transmission bandwidth configuration plus 15 kHz at each edge but not within the NR minimum guard band GBChannel.

**NB-IoT operation in NR guard band:** NB-IoT is operating in guard band when it is located within a NR BS channel bandwidth but is not NB-IoT operation in NR in-band.

**operating band:** frequency range in which NR operates (paired or unpaired), that is defined with a specific set of technical requirements.

**port:** particular interface of EUT used for EMC requirements testing purposes.

NOTE: Any connection point on EUT intended for connection of cables to or from EUT during the EMC testing is considered as a port.

EXAMPLE 1: Examples of ports for *BS type 1-C* and *BS type 1-H* are as presented in figure 3.1‑1:



Figure 3.1-1: Examples of *port*s for *BS type 1-C* and *BS type 1-H*

EXAMPLE 2: Examples of ports for *BS type 1-O* and *BS type 2-O* (i.e. with no *antenna ports*) are as presented in figure 3.1-2:



Figure 3.1-2: Examples of *port*s for *BS type 1-O* and *BS type 2-O*

**receiver exclusion band:** band of frequencies over which no tests of radiated immunity of a receiver are made, and expressed relative to the BS receive band.

**semi-anechoic chamber:** shielded enclosure in which all surfaces except the metal floor are covered with material that absorbs electromagnetic energy (i.e. RF absorber) in the frequency range of interest.

**signal port**: portintended for the interconnection of components of an EUT, or between an EUT and associated equipment and used in accordance with relevant functional specifications (for example for the maximum length of cable connected to it).

**spatial exclusion zone:** range of angles where no tests of radiated immunity are made for *BS type 1-O* or *BS type 2-O* (i.e. half sphere around the EUT's radiating direction).

**TAB connector:** *transceiver array boundary* connector

**Throughput:** number of payload bits successfully received per second for a reference measurement channel in a specified reference condition.

**transceiver array boundary:** conducted interface between the *transceiver unit* array and the composite antenna.

**transceiver unit:** active unit consisting of transmitter and/or receiver which transmits and/or receives radio signals, and which may include passive RF filters.

**telecommunication port:** ports which are intended to be connected to telecommunication networks (e.g. public switched telecommunication networks, integrated services digital networks), local area networks (e.g. Ethernet, Token Ring) and similar networks.

NOTE: *Telecommunication port* is called "wired network port" in CISPR 32 [11] and ETSI EN 301 489-1 [23].

**transient phenomena:** pertaining to or designating a phenomena or a quantity which varies between two consecutive steady states during a time interval short compared with the time-scale of interest (IEC 60050-161 [9]).

**transmitter exclusion band:** band of frequencies over which no tests of radiated immunity of a transmitter are made and is expressed relative to the carrier frequencies used (the carrier frequencies of the base stations activated transmitter(s)).

**upper RF bandwidth edge:** the frequency of the upper edge of the Base Station RF bandwidth, used as a frequency reference point for transmitter and receiver requirements.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

β Bandwidth

BWChannel Channel bandwidth

ΔfOBUE Maximum offset of the *operating band* unwanted emissions mask from the downlink *operating band* edge

ΔfOOB Maximum offset of the out-of-band boundary from the uplink *operating band* edge

FDL,low The lowest frequency of the downlink *operating band*

FDL,high The highest frequency of the downlink *operating band*

FUL,low The lowest frequency of the uplink *operating band*

FUL,high The highest frequency of the uplink *operating band*

ΔfRIexclusion Maximum offset of the Radiated Immunity exclusion band from the uplink *operating band* edge for test without *spatial exclusion zone* applied

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

AC Alternating Current

AMN Artificial Mains Network

BC Band Category

BS Base Station

CA Carrier Aggregation

CDN Coupling/Decoupling Network

CS Capability Set

DC Direct Current

EIRP Equivalent Isotropic Radiated Power

EMC Electromagnetic Compatibility

e.r.p. Effective Radiated Power

ESD Electrostatic Discharge

EUT Equipment Under Test

FR Frequency Range

FAR Fully-Anechoic Room

FRC Fixed Reference Channel

FSOATS Free Space OATS

NB-IoT Narrowband – Internet of Things

NC Non Contiguous

NG Next Generation

NGC Next Generation Core

NR New Radio

NR-ARFCN NR Absolute Radio Frequency Channel Number

NRTC NR Test Configuration

NTC Test Configuration for Non-contiguous operation

NSA Normalized Site Attenuation

OATS Open Area Test Site

RAT Radio Access Technology

RF Radio Frequency

RIB Radiated Interface Boundary

rms root mean square

RSM Reference Site Method

SAC Semi Anechoic Chamber

SC Single Carrier

SDL Supplementary Downlink

TC Test Configuration

UL Uplink

# 4 Test conditions

## 4.1 General

Requirements throughout the EMC specifications are in some cases defined separately for different frequency ranges (FR). The frequency ranges FR1 and FR2 are defined in subclause 5.1 of TS 38.104 [2].

The equipment shall be tested in normal test environment defined in the corresponding BS conformance testing specification TS 38.141-1 [3] for *BS type 1-C* and *BS type 1-H*, or TS 38.141-2 [4] for *BS type 1-O* and *BS type 2-O*. The test conditions shall be recorded in the test report.

For BS capable of multi-band operation, the requirements in the present document apply for each supported *operating band* unless otherwise stated. *Operating bands* shall be activated according to the test configuration in subclause 4.5. Tests shall be performed relating to each type of port and all *operating bands* shall be assessed during the tests.

The manufacturer shall declare the supported *operating band(s)* according to the list of NR *operating bands* defined in TS 38.104 [2].

NOTE 1: NR *operating bands* for *BS type 1-C* and *BS type 1-H*, are declared by the manufacturer according to the declaration D.3 specified in TS 38.141-1 [3], table 4.6-1.

NOTE 2: NR *operating bands* for *BS type 1-O* and *BS type 2-O,* are declared by the manufacturer according to the declaration D.4 specified in TS 38.141-2 [4], table 4.6-1.

## 4.2 Arrangements for establishing a communication link

The wanted RF input signal nominal frequency shall be selected by setting the NR Absolute Radio Frequency Channel Number (NR-ARFCN) to an appropriate number, as defined in TS 38.104 [2], clause 5.4.2.3.

A communication link shall be set up with a suitable test system capable of evaluating the required performance criteria (hereafter called "the test system") at the radio interface and *telecommunication port(s)* (the NG interface). The test system shall be located outside of the test environment.

When the EUT is required to be in the transmit/receive mode, the following conditions shall be met:

- For the *BS type 1-C* and *BS type 1-H* testing, the EUT shall be commanded to operate at rated transmit power;

- For the *BS type 1-O* and *BS type 2-O* testing, the EUT transmit power shall be configured as stated in subclause 8.1 for emission test and subclause 9.1 for immunity test accordingly;

- Adequate measures shall be taken to avoid the effect of the unwanted signal on the measuring equipment;

- The wanted input signal level shall be set to a level where the performance is not limited by the receiver noise floor or strong signal effects.

NOTE: 15 dB above the conducted reference sensitivity level has been used as an example of wanted input signal level in legacy 3GPP EMC specifications for establishing a communication link.

For immunity tests clause 4.3 shall apply and the conditions shall be as follows.

## 4.3 Narrow band responses on receivers

Responses on receivers or duplex transceivers occurring during the immunity test at discrete frequencies which are narrow band responses (spurious responses), are identified by the following method:

- if during an immunity test the quantity being monitored goes outside the specified tolerances (clause 6), it is necessary to establish whether the deviation is due to a narrow band response or to a wide band (EMC) phenomenon. Therefore, the test shall be repeated with the unwanted signal frequency increased, and then decreased by 2 x BWChannel MHz, where BWChannel is the channel bandwidth as defined in TS 38.104 [2], clause 5.3;

- if the deviation disappears in either one or both of the above MHz offset cases, then the response is considered as a narrow band response;

- if the deviation does not disappear, this may be due to the fact that the offset has made the frequency of the unwanted signal correspond to the frequency of another narrow band response. Under these circumstances the procedure is repeated with the increase and decrease of the frequency of the unwanted signal set to 2.5 x BWChannel MHz;

- if the deviation does not disappear with the increased and/or decreased frequency, the phenomenon is considered wide band and therefore an EMC problem and the equipment fails the test.

For immunity test narrow band responses are disregarded.

For BS capable of multi-band operation, all supported *operating bands* shall be considered for narrowband responses.

## 4.4 Exclusion bands

### 4.4.1 Transmitter exclusion band

The*transmitter exclusion band* for BS is the frequency range over which no tests of radiated immunity of a transmitter are made. The *transmitter exclusion band* only applies to BS type 1-O.

The *transmitter exclusion band* is defined as:

FDL,low – ΔfOBUE<f < FDL,high + ΔfOBUE

Where:

Values of FDL,low and FDL,high are defined for each *operating band* in TS 38.104 [2], clause 5.2.

The value of ΔfOBUE is derived considering the width of the *operating band*, and is defined in TS 38.104 [2], clause 6.6.2.

For BS capable of multi-band operation, the total *transmitter exclusion band* is a combination of the *exclusion bands* for each *operating band* supported by BS.

NOTE 1: The *transmitter exclusion bands* do not apply for SUL bands.

NOTE 2: As the radiated immunity testing is defined in the frequency range 80 MHz to 6 GHz, there is no *transmitter exclusion band* defined for *BS type 2-O*.

### 4.4.2 Receiver exclusion band

The *receiver exclusion band* for BS is the frequency range over which no tests of radiated immunity of a receiver are made.

The *receiver exclusion band* is defined as:

FUL,low – ΔfOOB<f < FUL,high + ΔfOOB

Where:

Values of FUL,low and FUL,high are defined for each *operating band* in TS 38.104 [2], clause 5.2.

The value of ΔfOOB is derived considering the width of the *operating band*, and is defined in TS 38.104 [2], clause 7.4.2.2.

In case the *spatial exclusion zone* (as depicted in figure 9.2.2-1) is not used during the EMC RI testing, the receiver exclusion band for *BS type 1-O* is defined as:

FUL,low – ΔfRIexclusion < f < FUL,high + ΔfRIexclusion

Where the values of ΔfRIexclusion are defined in table 4.4.2-1.

Table 4.4.2-1: Maximum ΔfRIexclusion offset outside the uplink operating band

|  |  |
| --- | --- |
| *Operating band* characteristics | ΔfRIexclusion (MHz) |
| 100 MHz ≥ FUL,high – FUL,low | 60 |
| 100 MHz < FUL,high – FUL,low | 200 |

For BS capable of multi-band operation, the total *receiver exclusion band* is a combination of the *exclusion bands* for each *operating band* supported by BS.

NOTE 1: The *receiver exclusion bands* do not apply for SDL bands.

NOTE 2: As the radiated immunity testing is defined in the frequency range 80 MHz to 6 GHz, there is no *receiver exclusion band* defined for *BS type 2-O*.

## 4.5 BS test configurations

The present clause defines the BS test configurations that shall be used for demonstrating conformance. A single NR carrier shall be used for testing of single-carrier capable BS.

Single carrier configuration (SC) tests shall be performed using signal with narrowest supported *BS channel bandwidth* with the smallest supported subcarrier spacing declared per *operating band* in TS 38.141-1 [3] clause 4.6 (see declaration D.14), and TS 38.141-2 [4] clause 4.6 (see declaration D.7).

For other NR base stations, the test configurations in table 4.5-1 and table 4.5-2 shall be used. The NR test configurations (NRTCx) are defined in TS 38.141-1 [3], clause 4.7 for *BS type 1-C* and *BS type 1-H* and in TS 38.141-2 [4], clause 4.8 for *BS type 1-O* and *BS type 2-O*.

Table 4.5-1: Test configurations for *BS type 1-C* and *BS type 1-H*

| BS test case | BS capable of multi-carrier and/or CA in a single band | | | BS capable of multi-band operation | |
| --- | --- | --- | --- | --- | --- |
|  | Contiguous spectrum capable BS | C and NC capable BS with identical parameters | C and NC capable BS with different parameters | BS capable of multi-band operation with common connector | BS capable of multi-band operation with separate connector |
| Emission tests | NRTC1 | NRTC3 | NRTC1, NRTC3 | NRTC1/3 (Note 1), NRTC5 | NRTC1/3 (Note 1), NRTC5 (Note 2) |
| Immunity tests | NRTC1 | NRTC3 | NRTC1, NRTC3 | NRTC1/3 (Note 1), NRTC5 | NRTC1/3 (Note 1), NRTC5 (Note 3) |
| Note 1: NRTC1 and/or NRTC3 shall be applied in each supported operating band.  Note 2: For single-band operation test, other antenna connector(s) is (are) terminated.  Note 3: NRTC5 is only applicable for multi-band receiver. | | | | | |

Table 4.5-2: Test configurations for *BS type 1-O*

| BS test | Single band RIB | | | Multi-band RIB |
| --- | --- | --- | --- | --- |
|  | Contiguous spectrum capable BS | C and NC capable BS with identical parameters | C and NC capable BS with different parameters |  |
| Emission tests | NRTC1 | NRTC3 | NRTC1, NRTC3 | NRTC1/3 (Note), NRTC5 |
| Immunity tests | NRTC1 | NRTC3 | NRTC1, NRTC3 | NRTC5 |
| Note: NRTC1 and/or NRTC3 shall be applied in each supported operating band. | | | | |

Table 4.5-3: Test configurations for *BS type 2-O*

| BS test case | Single band RIB | | |
| --- | --- | --- | --- |
|  | Contiguous spectrum capable BS | C and NC capable BS with identical parameters | C and NC capable BS with different parameters |
| Emission tests | NRTC1 | NRTC3 | NRTC1, NRTC3 |
| Immunity tests | NRTC1 | NRTC3 | NRTC1, NRTC3 |

## 4.6 Manufacturer declarations

The following EMC-specific manufacturer’s declarations listed in table 4.6-1 are required to be provided by the manufacturer for NR BS requirements testing.

NOTE: The below listed manufacturer’s declarations are supplementary to declarations covered in TS 38.141-1 [3] and/or TS 38.141-2 [4].

Table 4.6-1 EMC-specific manufacturer declarations

|  |  |  |
| --- | --- | --- |
| Declaration identifier | Declaration | Description |
| DEMC.1  (NOTE) | Ports intended to be used with cables less than 3 m | Declaration of any port(s) intended to be used with cables less than 3 m. |
| NOTE: This manufacturer declaration is optional. | | |

# 5 Performance assessment

## 5.1 General

The following information shall be recorded in or annexed to the test report:

- the primary functions of the radio equipment to be tested during and after the EMC testing;

- the intended functions of the radio equipment which shall be in accordance with the documentation accompanying the equipment;

- the method to be used to verify that a communications link is established and maintained;

- the user-control functions and stored data that are required for normal operation and the method to be used to assess whether these have been lost after EMC stress;

- the *ancillary equipment* to be combined with the radio equipment for testing (where applicable);

- the information about *ancillary equipment* intended to be used with the radio equipment;

- information about the common and/or band-specific active RF components and other hardware blocks for a communication link in BS capable of multi-band operation;

- an exhaustive list of ports (and RIBs), classified as either power or signal/control. Power ports shall further be classified as AC or DC power.

Performance assessment of a BS with multiple enclosures may be done separately for the BS part with the Radio digital unit and the Radio unit respectively, according to the manufacturer's choice.

A communication link used by more than one *operating band*, shall be assessed on all *operating band*s. Communication link(s) and/or radio performance parameters for the *operating band*s can during the test be assessed simultaneously or separately for each band, depending on the test environment capability.

## 5.2 Assessment of throughput in Downlink

A communication link shall be established between the transmitter (via port for the *BS type 1-C* and *BS type 1-H*, or via RIB for the *BS type 1-O* and *BS type 2-O*) and the test equipment. Test equipment shall meet the requirements for the throughput assessment defined in TS 38.101-4 [27] for the bearer used in the immunity tests. The level of the signal supplied to the equipment should be within the range for which the assessment of throughput is not impaired. Power control shall be OFF during the immunity testing.

## 5.3 Assessment of throughput in Uplink

The value of the throughput at the output of the receiver shall be monitored at NG interface by using suitable test equipment.

## 5.4 Ancillary equipment

At the manufacturer's discretion the test may be performed on the *ancillary equipment* separately or on a representative configuration of the combination of radio and *ancillary equipment*. In each case EUT is tested against all applicable immunity and emission clauses of the present document and in each case, compliance enables the *ancillary equipment* to be used with different radio equipment.

# 6 Performance criteria

## 6.1 Performance criteria for continuous phenomena for BS

The test should, where possible, be performed using a bearer with the characteristics of data rate and throughput defined in table 6.1-1, table 6.1-1a, table 6.1-1b and table 6.1-2. If the test is not performed using one of these bearers (for example, of none of them are supported by the BS), the characteristics of the bearer used shall be recorded in the test report.

The throughput in table 6.1-1, table 6.1-1a, table 6.1-1b and table 6.1-2 is stated relative to the maximum throughput of the FRC.

The BS uplink and downlink paths shall each meet the performance criteria defined in table 6.1-1, table 6.1-1a, table 6.1-1b and table 6.1-2 during the test. If the uplink and downlink paths are evaluated as a one loop then the criteria is two times the throughput reduction shown in table 6.1-1, table 6.1-1a, table 6.1-1b and table 6.1-2 (i.e. throughput > 90 % instead of throughput > 95 %). After each test case BS shall operate as intended with no loss of user control function, stored data and the communication link shall be maintained.

Table 6.1-1: FR1 performance criteria for continuous phenomena for BS

|  |  |  |  |
| --- | --- | --- | --- |
| NR channel bandwidth (MHz) as defined in TS 38.104 section 5.3.2-1 [2] | Sub-carrier spacing (kHz) | Bearer information data rate  (Note 3)  (as in annex A.1 in TS 38.104 [2]) | Performance criteria  (Note 1, Note 2) |
| 3 | 15 | G-FR1-A1-7 | Throughput > 95 %,  no loss of service |
| 5, 10, 15 | 15 | G-FR1-A1-21 for NR with NB-IoT in-band operation |  |
| 10, 15 | 30 | G-FR1-A1-1 |  |
| 10, 15 | 60 | G-FR1-A1-10 for NR with NB-IoT in-band operation |  |
| 20 to 50 | 15 | G-FR1-A1-2 |  |
| 20 to 100 | 30 | G-FR1-A1-3 |  |
| 20 to 100 | 60 | G-FR1-A1-4 |  |
| NOTE 1: The performance criteria, throughput > 95 %, no loss of service, applies also if a bearer with another characteristics is used in the test.  NOTE 2: The performance criteria, throughput > 90 %, no loss of service, applies instead if the uplink and downlink paths are evaluated as a one loop.  NOTE 3: These reference measurement channels are not applied for bands n46, n96 and n102. | | | |

Table 6.1-1a: Performance criteria for continuous phenomena for band n46

|  |  |  |  |
| --- | --- | --- | --- |
| NR channel bandwidth (MHz) as defined in TS 38.104 section 5.3.2-1 [2] | Sub-carrier spacing (kHz) | Bearer information data rate  (as in annex A.1 in TS 38.104 [2]) | Performance criteria (Note 1, Note 2) |
| 10 | 15 | G-FR1-A1-12 | Throughput > 95 %  no loss of service |
| 30 | G-FR1-A1-13 |  |
| 60 | G-FR1-A1-3 |  |
| 20 | 15 | G-FR1-A1-14 |  |
| 30 | G-FR1-A1-15 |  |
| 60 | G-FR1-A1-6 |  |
| 40 | 15 | G-FR1-A1-16 |  |
| 30 | G-FR1-A1-17 |  |
| 60 | G-FR1-A1-6 |  |
| 60 | 30 | G-FR1-A1-18 |  |
| 60 | G-FR1-A1-6 |  |
| 80 | 30 | G-FR1-A1-19 |  |
| 60 | G-FR1-A1-6 |  |
| NOTE 1: The performance criteria, throughput > 95 %, no loss of service, applies also if a bearer with another characteristics is used in the test.  NOTE 2: The performance criteria, throughput > 90 %, no loss of service, applies instead if the uplink and downlink paths are evaluated as a one loop. | | | |

Table 6.1-1b: Performance criteria for continuous phenomena for bands n96 and n102

|  |  |  |  |
| --- | --- | --- | --- |
| NR channel bandwidth (MHz) as defined in TS 38.104 section 5.3.2-1 [2] | Sub-carrier spacing (kHz) | Bearer information data rate  (as in annex A.1 in TS 38.104 [2]) | Performance criteria (Note 1, Note 2) |
| 20 | 15 | G-FR1-A1-14 | Throughput > 95 %  no loss of service |
| 30 | G-FR1-A1-15 |  |
| 60 | G-FR1-A1-6 |  |
| 40 | 15 | G-FR1-A1-16 |  |
| 30 | G-FR1-A1-17 |  |
| 60 | G-FR1-A1-6 |  |
| 60 | 30 | G-FR1-A1-18 |  |
| 60 | G-FR1-A1-6 |  |
| 80 | 30 | G-FR1-A1-19 |  |
| 60 | G-FR1-A1-6 |  |
| NOTE 1: The performance criteria, throughput > 95 %, no loss of service, applies also if a bearer with another characteristics is used in the test.  NOTE 2: The performance criteria, throughput > 90 %, no loss of service, applies instead if the uplink and downlink paths are evaluated as a one loop. | | | |

Table 6.1-2: FR2 performance criteria for continuous phenomena for BS

|  |  |  |  |
| --- | --- | --- | --- |
| NR channel bandwidth (MHz) | Sub-carrier spacing (kHz) | Bearer information data rate  (as in annex A.1 in TS 38.104 [2]) | Performance criteria  (Note 1, Note 2) |
| 50, 100, 200 | 60 | G-FR2-A1-1 | Throughput > 95 %,  no loss of service |
| 50 | 120 | G-FR2-A1-2 |  |
| 100, 200, 400 | 120 | G-FR2-A1-3 |  |
| NOTE 1: The performance criteria, throughput > 95 %, no loss of service, applies also if a bearer with another characteristics is used in the test.  NOTE 2: The performance criteria, throughput > 90 %, no loss of service, applies instead if the uplink and downlink paths are evaluated as a one loop. | | | |

## 6.2 Performance criteria for transient phenomena for BS

At the conclusion of the total test (comprising the series of individual exposures to transient phenomena) the EUT shall operate as intended with no user noticeable loss of control functions or stored data. At the conclusion of each exposure the EUT shall operate with no user noticeable loss of the communication link. The channel bandwidth, sub-carrier spacing and bearer information data rate should be chosen based on manufacturers declarations (see declaration D.14 in TS 38.141-1 [3] and/or D.7 in TS 38/141-2 [4]) and defined according to table 6.1-1, table 6.1-1a, table 6.1-1b and table 6.1-2.

## 6.3 Performance criteria for continuous phenomena for Ancillary equipment

The apparatus shall continue to operate as intended during and after the test. No degradation of performance or loss of function is allowed below the performance level specified by the manufacturer, when the apparatus is used as intended. The performance level may be replaced by a permissible performance loss. If the minimum performance level or the permissible performance loss is not specified by the manufacturer, either of these may be derived from the product description and documentation and what the user may reasonably expect from the apparatus if used as intended.

## 6.4 Performance criteria for transient phenomena for Ancillary equipment

The apparatus shall continue to operate as intended after the test. No degradation of performance or loss of function is allowed below the performance level specified by the manufacturer, when the apparatus is used as intended. The performance level may be replaced by a permissible performance loss. During the test, degradation of performance is however allowed. If the minimum performance level or the permissible performance loss is not specified by the manufacturer, either of these may be derived from the product description and documentation and what the user may reasonably expect from the apparatus if used as intended.

# 7 Applicability overview

## 7.1 Emission

Table 7.1-1: Emission requirements applicability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Phenomenon | Application | Equipment test requirement | | Reference  clause in the present document | Reference  standard |
|  |  | BS equipment | Ancillary equipment |  |
| Radiated emission | Enclosure | applicable for *BS type 1-C* and *BS type 1-H*  (Note 1) | not applicable | 8.2.1 | ITU-R SM.329 [24] |
| Radiated emission | Enclosure of *ancillary equipment* | not applicable | applicable | 8.2.2 | CISPR 32 [11] |
| Conducted emission | DC power input/output port | applicable | applicable | 8.3 | CISPR 32 [11] |
| Conducted emission | AC mains input/output port | applicable | applicable | 8.4 | CISPR 32 [11] |
| Conducted emission | *Telecommunication port* | applicable | applicable | 8.5 | CISPR 32 [11] |
| Harmonic current emissions | AC mains input port | applicable | applicable | 8.6 | IEC 61000-3-2 [13] or  IEC 61000-3-12 [14]  (NOTE 2) |
| Voltage fluctuations and flicker | AC mains input port | applicable | applicable | 8.7 | IEC 61000-3-3 [15] or  IEC 61000-3-11 [16]  (NOTE 2) |
| NOTE 1: Radiated emission requirements for *BS type 1-O* and *BS type 2-O* are described in clause 8.2.1.  NOTE 2: Selection of the reference IEC specification is based on the rated input current of the EUT’s power supply. | | | | | |

## 7.2 Immunity

Table 7.2-1: Immunity requirements applicability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Phenomenon | Application | Equipment test requirement | | Reference  clause in the present document | Reference  standard |
|  |  | BS equipment | Ancillary equipment |  |
| RF electro­magnetic field (80 – 6000 MHz) | Enclosure | applicable | applicable | 9.2 | IEC 61000‑4‑3 [18] |
| Electrostatic discharge | Enclosure | applicable | applicable | 9.3 | IEC 61000‑4‑2 [17] |
| Fast transients common mode | Signal, telecommunications and control ports, DC and AC power input ports | applicable | applicable | 9.4 | IEC 61000‑4‑4 [19] |
| RF common mode  0.15 - 80 MHz | Signal, telecommunications and control ports, DC and AC power input ports | applicable | applicable | 9.5 | IEC 61000‑4‑6 [21] |
| Voltage dips and interruptions | AC mains power input *port*s | applicable | applicable | 9.6 | IEC 61000‑4‑11 [22] |
| Surges, common and differential mode | AC power input *port*s and *telecommunications port* | applicable | applicable | 9.7 | IEC 61000‑4‑5 [20] |

# 8 Emission

## 8.1 Test configurations

This clause defines the configurations for emission tests as follows:

- The equipment shall be tested under normal test conditions as specified in the functional standards;

- The test configuration shall be as close to normal intended use as possible;

- If the equipment is part of a system, or can be connected to ancillary equipment, then it shall be acceptable to test the equipment while connected to the minimum configuration of *ancillary equipment* necessary to exercise the ports;

- If the equipment has a large number of ports, then a sufficient number shall be selected to simulate actual operation conditions and to ensure that all the different types of termination are tested;

- The test conditions, test configuration and mode of operation shall be recorded in the test report;

- Ports which in normal operation are connected shall be connected to an *ancillary equipment* or to a representative piece of cable correctly terminated to simulate the input/output characteristics of the *ancillary equipment*; in case of *BS type 1-H*, *antenna port*s shall be correctly terminated;

- For *BS type 1-O* and *BS type 2-O* without *antenna ports* but intentionally radiating through the *antenna array*, the equipment shall be placed in a test setup suitable for the radiated power;

- Ports which are not connected to cables during normal operation, e.g. service connectors, programming connectors, temporary connectors etc. shall not be connected to any cables for the purpose of EMC testing. Where cables have to be connected to these ports, or interconnecting cables have to be extended in length in order to exercise the EUT, precautions shall be taken to ensure that the evaluation of the EUT is not affected by the addition or extension of these cables;

- The test arrangements for transmitter and receiver clauses of the transceiver are described separately for the sake of clarity. However, where possible the test of the transmitter clause and receiver clause of the EUT may be carried out simultaneously to reduce test time.

### 8.1.1 (Void)

### 8.1.2 (Void)

### 8.1.3 (Void)

### 8.1.4 (Void)

### 8.1.5 (Void)

## 8.2 Radiated emission

### 8.2.1 Radiated emission, BS

This test is applicable to *BS type 1-C* and *BS type 1-H*. This test shall be performed on a representative configuration of BS.

For *BS type 1-O* and *BS type 2-O*, the radiated emission is covered by radiated spurious emission requirement in TS 38.104 [2], conforming to the test requirement in TS 38.141-2 [4].

#### 8.2.1.1 Definition

This test assesses the ability of BS to limit unwanted emission from the *enclosure port*.

#### 8.2.1.2 Test method

a) A test site fulfilling the requirements of ITU-R SM.329 [24] shall be used. The BS shall be placed on a non-conducting support and shall be operated from a power source via a RF filter to avoid radiation from the power leads. One of the following two alternative measurement methods shall be used:

1) Field strength method measurement

The test method shall be in accordance with CISPR 32 [11]. The field strength measurements shall be performed on a test site that is validated according to the methods and requirements of CISPR 16-1-4 [30].

Unless otherwise stated, measurements are conducted at 3 m or 10 m on an open area test site (OATS) or semi anechoic chamber (SAC) for frequencies up to 1 GHz, or at 3 m on a free space open area test site (FSOATS) or fully-anechoic room (FAR) for frequencies above 1 GHz. Unless otherwise stated, all measurements are done with RMS detector and with the -3 dB bandwidth of the measuring filter equal to the reference bandwidth in table 8.2.1.3-1.

NOTE 1: Test site validation methods for radiated emissions tests are defined in CISPR 16-1-4 [30], clause 6 and 7. Examples of test site validation methods are listed below:

- 30 - 1000 MHz frequency range: Normalized Site Attenuation (NSA), Reference Site Method (RSM).

- 1 - 18 GHz frequency range: SVSWR standard test procedure, SVSWR reciprocal test procedure.

2) Substitution method measurement (also called a substitution method)

Mean power of any spurious components shall be detected by the test antenna and measuring receiver (e.g. a spectrum analyser). At each frequency at which a component is detected, the BS shall be rotated and the height of the test antenna adjusted to obtain maximum response, and the effective radiated power (e.r.p.) of that component determined by a substitution measurement. The measurement shall be repeated with the test antenna in the orthogonal polarization plane. Unless otherwise stated, all measurements are done as mean power (RMS).

NOTE 2: Effective radiated power (e.r.p.) refers to the radiation of a half wave tuned dipole instead of an isotropic antenna. There is a constant difference of 2.15 dB between e.i.r.p. and e.r.p, as defined in ITU-R SM.329 annex 1 [24].

e.r.p. (dBm)  EIRP (dBm)  2.15

b) The BS shall transmit with maximum power declared by the manufacturer with all transmitters active. Set the base station to transmit a signal as stated in clause 4.5.

c) The received power shall be measured over the frequency range from 30 MHz to FDL,low - ΔfOBUE and from FDL,high + ΔfOBUE up to 12750 MHz. For some *operating bands*, the upper limit is higher than 12.75 GHz in order to comply with the 5th harmonic limit of the downlink *operating band*, as specified in ITU-R SM.329 [24].The video bandwidth shall be approximately three times the resolution bandwidth. If this video bandwidth is not available on the measuring receiver, it shall be the maximum available and at least 1 MHz. Unless otherwise stated, all measurements are done as mean power (RMS).

#### 8.2.1.3 Limits

The frequency boundary and reference bandwidths for the detailed transitions of the limits between the requirements for out of band emissions and spurious emissions are based on ITU-R Recommendations SM.329 [24] and SM.1539 [26].

The *BS type 1-C* and *BS type 1-H* shall meet the limits below:

Table 8.2.1.3-1: Limits for radiated emissions from BS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Frequency range | e.r.p.  (dBm) | Field strength at 3 m (dBµV/m)  (NOTE 4) | Field strength at 10 m  (dBµV/m)  (NOTE 4) | Reference bandwidth | Notes |
| 30 MHz ≤ f < 1000 MHz | -36 | 65.4 (NOTE 5) | 54.9 (NOTE 5) | 100 kHz |  |
| 1 GHz ≤ f < 12.75 GHz | -30 | 67.4 | Not applicable | 1 MHz |  |
| 12.75 GHz ≤ f < 5th harmonic of the upper frequency edge of the DL operating band in GHz | -30 | 67.4 | Not applicable | 1 MHz | NOTE 1 |
| 12.75 GHz - 26 GHz | -30 | 67.4 | Not applicable | 1 MHz | NOTE 6 |
| FDL,low - ΔfOBUE < f < FDL,high +ΔfOBUE | Not defined | Not defined | Not defined | Not defined | NOTE 2,3 |
| NOTE 1: This frequency range applies only for operating bands for which the 5th harmonic of the upper frequency edge of the DL operating band is reaching beyond 12.75 GHz.  NOTE 2: For BS capable of multi-band operation, the frequency ranges relating to the RF bandwidths of all supported *operating bands* apply.  NOTE 3: ΔfOBUE is defined in clause 6.6.1 of TS 38.104 [2].  NOTE 4: The field strength measurements shall be conducted on OATS or SAC for frequencies up to 1 GHz, or on FSOATS or FAR for frequencies above 1 GHz.  NOTE 5: Limits for radiated emissions are translated from the e.r.p. limit of -36 dBm into the field strength limit of 61.4 dBµV/m (at 3m) or 50.9 dBµV/m (at 10m), and increased by the site gain value of 4 dB. The value of the site gain is based on ITU-R Recommendations SM.329 [24].  NOTE 6: Applies only for band n46, n96 and n102. | | | | | |

#### 8.2.1.4 Interpretation of the measurement results

The interpretation of the results recorded in a test report for the radiated emission measurements described in the present document shall be as follows:

- the measured value related to the corresponding limit will be used to decide whether an equipment meets the requirements of the present document;

- the value of the measurement uncertainty for the measurement of each parameter shall be included in the test report;

- the recorded value of the measurement uncertainty shall be, for each measurement, equal to or lower than the figures in table 8.2.1-4-1 for BS.

Table 8.2.1.4-1 specifies the maximum measurement uncertainty of the test system. The test system shall enable the equipment under test to be measured with an uncertainty not exceeding the specified values. All tolerances and uncertainties are absolute values, and are valid for a confidence level of 95 %, unless otherwise stated.

A confidence level of 95 % is the measurement uncertainty tolerance interval for a specific measurement that contains 95% of the performance of a population of test equipment.

Table 8.2.1.4-1: Maximum measurement uncertainty (BS)

|  |  |  |
| --- | --- | --- |
| Parameter | Uncertainty for EUT dimension ≤ 1 m  (NOTE 2) | Uncertainty for EUT dimension >1 m  (NOTE 2) |
| Effective radiated RF power between 30 MHz and 180 MHz | ±6 dB | ±6 dB |
| Effective radiated RF power between 180 MHz and 4 GHz | ±4 dB | ±6 dB |
| Effective radiated RF power between 4 GHz and 12,75 GHz | ±6 dB | ±9 dB (NOTE 1) |
| Effective radiated RF power between 12,75 GHz and 26 GHz | ±6 dB | ±9 dB (NOTE 1) |
| Field strength between 30 MHz and 12,75 GHz | ±6 dB | ±6 dB |
| Field strength between 12,75 GHz and 26 GHz | ±6 dB | ±6 dB |
| NOTE 1: This value may be reduced to ±6 dB when further information on the potential radiation characteristic of the EUT is available.  NOTE 2: These MU values estimates and are not based on the MU budget calculations. For more background on MU derivation analyses refer to CISPR 16-4-2 [31] and ETSI TR 100 028-1 [32]. | | |

NOTE: If the Test System for a test is known to have a measurement uncertainty greater than that specified in table 8.2.1.4-1, this equipment can still be used, provided that an adjustment is made follows:

Any additional uncertainty in the Test System over and above that specified in table 8.2.1.4-1 is used to tighten the test requirements, i.e. making the test harder to pass.

This procedure will ensure that a test system not compliant with table 8.2.1.4-1 does not increase the probability of passing an EUT that would otherwise have failed a test if a test system compliant with table 8.2.1.4-1 had been used.

### 8.2.2 Radiated emission, ancillary equipment

This test is only applicable to *ancillary equipment* not incorporated in the radio equipment and intended to be measured on a stand-alone basis, as declared by the manufacturer. This test shall be performed on a representative configuration of the *ancillary equipment*.

This test is not applicable for *ancillary equipment* incorporated in the radio equipment, or for *ancillary equipment* intended to be measured in combination with the radio equipment. In these cases, the requirements of the relevant product standard for the effective use of the radio spectrum shall apply.

#### 8.2.2.1 Definition

This test assesses the ability of *ancillary equipment* to limit unwanted emission from the *enclosure port*.

#### 8.2.2.2 Test method

The test method shall be in accordance with CISPR 32 [11].

#### 8.2.2.3 Limits

The *ancillary equipment* shall meet the limits according to CISPR 32 [11] table A.4 and table A.5.

For the referred limit values, the following shall apply:

- Where the limits value varies over a given frequency range, it changes linearly with respect to the logarithm of the frequency.

- Where there is a step in the relevant limit, the lower value shall be applied at the transition frequency.

Table 8.2.2.3-1: (Void)

Table 8.2.2.3-2: (Void)

Alternatively, for *ancillary equipment* intended to be used in telecommunication centres only, the class A limits given in CISPR 32 [11], annex A, table A.2 and table A.3 may be used.

## 8.3 Conducted emission DC power input/output port

This test is applicable to equipment which may have DC cables longer than 3 m.

If the DC power cable of the radio equipment is intended to be less than 3 m in length, and intended only for direct connection to a dedicated AC to DC power supply, then the measurement shall be performed only on the AC power input of that power supply as specified in clause 8.4.

This test shall be performed on a representative configuration of the radio equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 8.3.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to limit internal noise from the DC power input/output ports.

### 8.3.2 Test method

The test method shall be in accordance with CISPR 32 [11] and the Artificial Mains Network (AMN) shall be connected to a DC power source.

In the case of DC output ports, the ports shall be connected via an AMN to a load drawing the rated current of the source.

A measuring receiver shall be connected to each AMN measurement port in turn and the conducted emission recorded.

The equipment shall be installed with a ground plane as defined in CISPR 32 [11]. The reference earth point of the AMN shall be connected to the reference ground plane with a conductor as short as possible.

### 8.3.3 Limits

The equipment shall meet the limits according to CISPR 32 [11] table A.9, which are defined for average detector receiver and for quasi-peak detector receiver. If the average limit is met when using a quasi‑peak detector, the equipment shall be deemed to meet both limits and measurement with the average detector receiver is not necessary.

Where there is a step in the referred limit values, the lower value shall be applied at the transition frequency.

Table 8.3.3-1: (Void)

## 8.4 Conducted emissions, AC mains power input/output port

This test is applicable to equipment powered by the AC mains.

This test is not applicable to AC output ports which are connected directly (or via a circuit breaker) to the AC power port of the EUT.

This test shall be performed on a representative configuration of the radio equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 8.4.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to limit internal noise from the AC mains power input/output ports.

### 8.4.2 Test method

The test method shall be in accordance with CISPR 32 [11].

### 8.4.3 Limits

The equipment shall meet the limits according to CISPR 32 [11] table A.10, which are defined for the average detector receiver and for quasi-peak detector receiver. If the average limit is met when using a quasi‑peak detector, the equipment shall be deemed to meet both limits and measurement with the average detector receiver is not necessary.

For the referred limit values following shall apply:

Where the limits value varies over a given frequency range, it changes linearly with respect to the logarithm of the frequency.

Where there is a step in the relevant limit, the lower value shall be applied at the transition frequency.

Table 8.4.3-1: (Void)

Alternatively, for equipment intended to be used in telecommunication centres the limits given in CISPR 32 [11] table A.9 shall be used.

Table 8.4.3-2: (Void)

## 8.5 Conducted emissions, telecommunication port

This test is applicable for radio equipment and/or *ancillary equipment* for fixed use which have *telecommunication ports*.

This test shall be performed on a representative configuration of radio equipment, the associated *ancillary equipment*, or a representative configuration of the combination of radio and *ancillary equipment*.

### 8.5.1 Definition

This test assesses the EUT unwanted emission present at the *telecommunication ports*.

### 8.5.2 Test method

The test method shall be in accordance with CISPR 32 [11].

### 8.5.3 Limits

The *telecommunication po*rts shall meet the limits according to CISPR 32 [11] table A.12.

For the referred limit values, following shall apply:

Where the limits value varies over a given frequency range, it changes linearly with respect to the logarithm of the frequency.

Where there is a step in the relevant limit, the lower value shall be applied at the transition frequency.

Table 8.5.3-1: (Void)

Alternatively, for equipment intended to be used in telecommunication centres only, the limits given in CISPR 32 [11] table A.11 may be used.

Table 8.5.3-2: (Void)

## 8.6 Harmonic current emissions (AC mains input port)

The requirements of IEC 61000‑3‑2 [13] for harmonic current emission apply for equipment covered by the scope of the present document. For equipment with an input current greater than 16 A per phase, IEC 61000-3-12 [14] applies.

## 8.7 Voltage fluctuations and flicker (AC mains input port)

The requirements of IEC 61000‑3‑3 [15] for voltage fluctuations and flicker apply for equipment covered by the scope of the present document. For equipment with an input current greater than 16 A per phase, IEC 61000-3-11 [16] applies.

# 9 Immunity

## 9.1 Test configurations

This clause defines the configurations for immunity tests as follows:

- the equipment shall be tested under normal test conditions as specified in the functional standards;

- during the test, the RF output power may be reduced to a power level sufficient for establishing and maintaining the required communication link;

- the test configuration shall be as close to normal intended use as possible;

- if the equipment is part of a system, or can be connected to *ancillary equipment*, then it shall be acceptable to test the equipment while connected to the minimum configuration of *ancillary equipment* necessary to exercise the ports;

- if the equipment has a large number of ports, then a sufficient number shall be selected to simulate actual operation conditions and to ensure that all the different types of termination are tested;

- the test conditions, test configuration and mode of operation shall be recorded in the test report;

- ports which in normal operation are connected shall be connected to an *ancillary equipment* or to a representative piece of cable correctly terminated to simulate the input/output characteristics of the *ancillary equipment*. In case of *BS type 1-C and BS type 1-H*, *antenna ports* shall be correctly terminated;

- ports which are not connected to cables during normal operation, e.g. service connectors, programming connectors, temporary connectors etc. shall not be connected to any cables for the purpose of EMC testing. Where cables have to be connected to these ports, or interconnecting cables have to be extended in length in order to exercise the EUT, precautions shall be taken to ensure that the evaluation of the EUT is not affected by the addition or extension of these cables;

- immunity tests on the entire NR BS shall be performed by establishing communication links at the radio interface (e.g. with the mobile simulator) and the NG interface (e.g. with an NGC simulator) and evaluating the throughput (see figures 9.1-1 and 9.1-2);

- immunity tests shall be performed on both the uplink and downlink paths. The tests shall also include both the radio interface and the NG interface. Throughput evaluation may be carried out at either interface, where appropriate, and the measurements for the uplink and downlink paths may be carried out as a single path looped at either the radio interface or NG interface. In case of looping is used care have to be taken that the throughput information doesn't change due to looping;

- for NR BS capable of multi-band operation, communication links shall be established in such a way that all *operating band*(s) are activated during the test according to the applicable test configurations in clause 4.5. Performance assessment may be done separately for each *operating band*.



Figure 9.1-1: Communication link set up for *BS type 1-C*/*BS type 1-H* immunity measurement



Figure 9.1-2: Communication link set up for *BS type 1-O*/*BS type 2-O* immunity measurement

### 9.1.1 (Void)

### 9.1.2 (Void)

### 9.1.3 (Void)

### 9.1.4 (Void)

### 9.1.5 (Void)

## 9.2 RF electromagnetic field (80 MHz to 6000 MHz)

The test shall be performed on a representative configuration of the equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 9.2.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to operate as intended in the presence of a radio frequency electromagnetic field disturbance at the enclosure.

### 9.2.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑3 [18], which specifies test methodology based on anechoic chamber. The use of reverberation chamber test method according to IEC 61000-4-21 [29], clause 6.1 and Annex D as alternative method is allowed.

The following requirements shall apply:

- The test level shall be 3 V/m amplitude modulated to a depth of 80 % by a sinusoidal audio signal of 1 kHz;

- The stepped frequency increments shall be 1 % of the momentary frequency;

- The test shall be performed over the frequency range 80 MHz - 6000 MHz; with the exception of the exclusion band for receivers (see clause 4.4);

- Responses in stand-alone receivers or receivers which are part of transceivers occurring at discrete frequencies which are narrow band responses, shall be disregarded, see clause 4.3;

- The frequencies selected during the test shall be recorded in the test report.

- For the test method in accordance with IEC 61000-4-3[18], the *spatial exclusion zone* can be chosen to protect the base station receiver. For the frequency range above 690 MHz (according to ETSI EN 301 489-50 [28]), the EMC RF electromagnetic field immunity requirement with a level of 10 V/m applies on the non-radiating faces of the *BS type 1-O* or *BS type 2-O,* as depicted on figure 9.2.2-1.

NOTE: Depending on the BS implementation, application of the spatial exclusion to all radiating faces of the BS may not allow proper execution of the RI testing. In such cases, to protect the *BS type 1-O* or *BS type 2-O* receiver(s), exclusion bands shall be considered, as in table 4.4.2-1.




Figure 9.2.2-1: EMC RF electromagnetic field immunity requirement testing directions for *BS type 1-O* and *BS type 2-O* (horizontal plane depicted) with the *spatial exclusion zone* applied

### 9.2.3 Performance criteria

**Base station:**

The performance criteria of clause 6.1 shall apply.

**Ancillary equipment:**

The performance criteria of clause 6.3 shall apply.

## 9.3 Electrostatic discharge

The test shall be performed on a representative configuration of the radio equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 9.3.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to operate as intended in the event of an electrostatic discharge.

### 9.3.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑2 [17]:

- for contact discharge, the equipment shall pass at ±4 kV;

- for air discharge shall pass at ±8 kV;

- electrostatic discharge shall be applied to all exposed surfaces of the EUT except where the user documentation specially indicates a requirement for appropriate protective measures.

NOTE: Ensure that the EUT is fully discharged between each ESD exposure.

### 9.3.3 Performance criteria

**Base station:**

The performance criteria of clause 6.2 shall apply.

**Ancillary equipment:**

The performance criteria of clause 6.4 shall apply.

## 9.4 Fast transients common mode

The test shall be performed on AC mains power input ports.

This test shall be performed on *signal ports*, *telecommunication ports*, *control ports* and DC power input/outputports if the cables may be longer than 3 m.

Where this test is not carried out on a port or any other ports because the manufacturer declares in EMCD.1 (see table 4.6-1) that it is not intended to be used with cables longer than 3 m, a list of ports which were not tested for this reason shall be included in the test report.

This test shall be performed on a representative configuration of the equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 9.4.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to operate as intended in the event of fast transients present on one of the input/output ports.

### 9.4.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑4 [19]:

- The test level for *signal ports*, *telecommunication ports* and *control ports* shall be 0.5 kV open circuit voltage as given in IEC 61000‑4‑4 [19];

- The test level for DC power input/output ports shall be 0.5 kV open circuit voltage as given in IEC 61000‑4‑4 [19];

- The test level for AC mains power input ports shall be 1 kV open circuit voltage as given in IEC 61000‑4‑4 [19].

For AC and DC power input ports the transients shall be applied (in parallel) to all the conductors in the cable with reference to the cabinet reference earth (true common mode) and the source impedance shall be 50 Ω.

### 9.4.3 Performance criteria

**Base station:**

The performance criteria of clause 6.2 shall apply.

**Ancillary equipment:**

The performance criteria of clause 6.4 shall apply.

## 9.5 RF common mode (0.15 MHz - 80 MHz)

The test shall be performed on AC mains power input/output ports.

This test shall be performed on *signal ports*, telecommunication *port*s, control and DC power input/output ports, which may have cables longer than 3 m.

Where this test is not carried out on a port or any other ports because the manufacturer declares in EMCD.1 (see table 4.6-1) that it is not intended to be used with cables longer than stated above, a list of ports which were not tested shall be included in the test report.

This test shall be performed on a representative configuration of the equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

NOTE: This test can also be performed using the clamp injection method, where appropriate, see IEC 61000‑4‑6 [21].

### 9.5.1 Definition

This test assesses the ability of radio equipment and *ancillary equipment* to operate as intended in the presence of a radio frequency electromagnetic disturbance.

### 9.5.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑6 [21]:

- The test signal shall be amplitude modulated to a depth of 80 % by a sinusoidal audio signal of 1 kHz;

- The stepped frequency increments shall be 50 kHz in the frequency range 150 kHz to 5 MHz and 1% frequency increment of the momentary frequency in the frequency range 5 MHz to 80 MHz;

- The test level shall be severity level 2 as given in IEC 61000‑4‑6 [21] corresponding to 3 V rms, at a transfer impedance of 150 Ω;

- The test shall be performed over the frequency range 150 kHz - 80 MHz;

- The injection method to be used shall be selected according to the basic standard IEC 61000-4-6 [21];

- Responses of stand-alone receivers or receivers which are part of transceivers occurring at discrete frequencies which are narrow band responses, shall be disregarded, see clause 4.3;

- The frequencies of the immunity test signal selected and used during the test shall be recorded in the test report.

### 9.5.3 Performance criteria

**Base station:**

The performance criteria of clause 6.1 shall apply.

**Ancillary equipment:**

The performance criteria of clause 6.3 shall apply.

## 9.6 Voltage dips and interruptions

The tests shall be performed on AC mains power input ports.

These tests shall be performed on a representative configuration of the equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 9.6.1 Definition

These tests assess the ability of radio equipment and *ancillary equipment* to operate as intended in the event of voltage dips and interruptions present on the AC mains power input ports.

### 9.6.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑11 [22], wherethe test levels shall be:

- Voltage dip: 0 % residual voltage for 0.5 cycle;

- Voltage dip: 0 % residual voltage for 1 cycle;

- Voltage dip: 70 % residual voltage for 25/30 cycles (at 50/60 Hz);

- Voltage interruption: 0 % residual voltage for 250/300 cycles (at 50/60 Hz).

### 9.6.3 Performance criteria

For a 0 % residual voltage dip test, the performance criteria for transient phenomena shall be applied:

- Criteria 6.2 for base station

- Criteria 6.4 for *ancillary equipment*

For a 70% residual voltage dip test and for voltage interruption test, the following applies:

1. In the case where the equipment is fitted with or connected to a battery back-up, the following performance criteria shall be applied:

- Criteria 6.2 for base station

- Criteria 6.4 for *ancillary equipment*

2. In the case where the equipment is powered solely from the AC mains supply (without the use of a parallel battery back-up) volatile user data may have been lost and if applicable the communication link need not to be maintained and lost functions should be recoverable by user or operator:

- No unintentional responses shall occur at the end of the test, when the voltage is restored to nominal

- In the event of loss of communications link or in the event of loss of user data, this fact shall be recorded in the test report.

## 9.7 Surges, common and differential mode

The tests shall be performed on AC mains power input ports.

This test shall be additionally performed on *telecommunication port*s.

These tests shall be performed on a representative configuration of the equipment, the associated *ancillary equipment*, or representative configuration of the combination of radio and *ancillary equipment*.

### 9.7.1 Definition

These tests assess the ability of radio equipment and *ancillary equipment* to operate as intended in the event of surges being present at the AC mains power input ports and *telecommunication ports*.

### 9.7.2 Test method and level

The test method shall be in accordance with IEC 61000-4-5 [20].

The requirements and evaluation of test results given in clause 9.7.2.1 (t*elecommunication port*s, outdoor cables), clause 9.7.2.2 (*telecommunication ports*, indoor cables) and clause 9.7.2.3 (AC power ports) shall apply, but no test shall be required where normal functioning cannot be achieved, because of the impact of the CDN on the EUT.

#### 9.7.2.1 Test method for telecommunication ports directly connected to outdoor cables

The test level for t*elecommunications port*s, intended to be directly connected to the telecommunications network via outdoor cables, shall be 1 kV line to ground as given in IEC 61000-4-5 [20]. In this case the total output impedance of the surge generator shall be in accordance with the basic standard IEC 61000-4-5 [20].

The test generator shall provide the 1.2/50 μs pulse as defined in IEC 61000-4-5 [20].

#### 9.7.2.2 Test method for telecommunication ports connected to indoor cables

The test level for telecommunication *port*s, intended to be connected to indoor cables (longer than 10 m) shall be 0.5 kV line to ground. In this case the total output impedance of the surge generator shall be in accordance with the basic standard IEC 61000-4-5 [20].

The test generator shall provide the 1.2/50 μs pulse as defined in IEC 61000-4-5 [20].

#### 9.7.2.3 Test method for AC power ports

The test level for AC power input *port*s shall be 2 kV line to ground, and 1 kV line to line, with the output impedance of the surge generator as given in IEC 61000-4-5 [20].

In telecommunication centres 1 kV line to ground and 0.5 kV line to line shall be used.

The test generator shall provide the 1.2/50 μs pulse as defined in IEC 61000-4-5 [20].

### 9.7.3 Performance criteria

**Base station:**

The performance criteria of clause 6.2 shall apply.

**Ancillary equipment:**

The performance criteria of clause 6.4 shall apply.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-08 | RAN4#84 | R4-1708861 |  |  |  | Specification Skeleton | 0.0.1 |
| 2017-10 | RAN4#84bis | R4-1711984 |  |  |  | Capture TPs approved in RAN4#84bis:  R4-1711815, "Draft TS 38.113 v0.0.1"  R4-1711828, "TP to TS 38.113: antenna ports for EMC"  R4-1711829, "TP to TS 38.113 Section 2 (References)"  R4-1711830, "TP to TS 38.113 Section 3 (Definitions, symbols and abbreviations)"  R4-1711831, "TP to TS 38.113 Section 7 (Applicability Overview)"  R4-1711832, "TP to TS 38.113 Section 8 (Emmision)"  R4-1711833, "TP to TS 38.113 Section 9 (Immunity)" | 0.0.2 |
| 2017-12 | RAN4#85 | R4-1714545 |  |  |  | Capture TPs approved in RAN4#85:  R4-1714297,"TP to TS 38.113 ESD test level"  R4-1714299,"TP to TS 38.113 section 2 ,3 and 7"  R4-1714429,"TP to Section 4.4 in TS 38.113 (NR) Receiver exclusion bands (radiated immunity)"  R4-1714301,"TP to Section 8.2 (Radiated Emission Limits) of TS 38.113"  R4-1712749,"TP for TS 38.113 introduction of band n71" | 0.1.0 |
| 2017-12 | RAN#78 | RP-172420 |  |  |  | v1.0.0 submitted for plenary approval | 1.0.0 |
| 2017-12 | RAN#78 |  |  |  |  | Approved by plenary – Rel-15 spec under change control | 15.0.0 |
| 2018-03 | RAN#79 | RP-180264 | 0002 |  | F | CR to TS 38.113  Cat.F draftCRs  R4-1801258 Draft CR to TS 38.113 Symbol(clause 3.2)  R4-1803309 [NR] DraftCR 38113 Rx exclusion (4.4.2)  R4-1803313 DraftCR to TS 38.113 subclause 5.1 and 5.4  R4-1803314 DraftCR to TS 38.113 subclause 8.2.1.2 radiated emission test method\_v2  R4-1803315 DraftCR to TS 38.113 subclause 9.1.1\_v3 | 15.1.0 |
| 2018-03 | RAN#79 | RP-180264 | 0003 |  | B | CR to TS 38.113  Cat.B draftCRs  R4-1802055 - Draft CR to Section 6.3 in TS 38.113 (NR) Performance criteria for continuous phenomena for Ancillary equipment  R4-1802056 - Draft CR to Section 6.4 in TS 38.113 (NR) Performance criteria for transient phenomena for Ancillary equipment  R4-1802057 - Draft CR to Section 8.4 in TS 38.113 (NR) Test method for conducted emissions AC mains power input output port  R4-1803318 [NR] DraftCR 38113 Test conditions (4) | 15.1.0 |
| 2018-06 | RAN#80 | RP-181076 | 0004 |  | F | CR to TS 38.113  Implementation of endorsed draft CRs from RAN4 #86bis and RAN4 #87 | 15.2.0 |
| 2018-09 | RAN#81 | RP-181896 | 0005 |  | F | CR to TS 38.113: Implementation of endorsed draft CRs from RAN4#88 | 15.3.0 |
| 2018-12 | RAN#82 | RP-182361 | 0008 | 1 | F | CR to TS 38.113 | 15.4.0 |
| 2019-03 | RAN#83 | RP-190403 | 0009 |  | F | CR to TS 38.113  Implementation of endorsed draftCRs in RAN4#90:  R4-1900565 - Draft CR to TS 38.113subclause 9.2.2, ZTE  R4-1900566 - Draft CR to TS 38.113subclause 9.7.2.1, ZTE  R4-1902330 - Draft CR to TS 38.113 Symbol (subclause 3 and 8.2.1), ZTE  R4-1902332 - Draft CR to TS 38.113subclause 7.1 and 8.3.2, ZTE  R4-1902334 - Draft CR to TS 38.113 Exclusion Bands for Radiated Immunity Test, Ericsson  R4-1902340 - Draft CR to TS 38.113 on FR1 and FR2 definitions, Ericsson  R4-1902331 - draft CR to 38.113 - NR BS EMC\_v1, Nokia | 15.5.0 |
| 2019-06 | RAN#84 | RP-191240 | 0011 |  | F | CR to TS 38.113  Endorsed draft CRs in RAN4#90Bis:  R4-1903562 Draft CR to TS 38.113 subclause 4.5  R4-1903636 - Draft CR to TS 38.113 Addition of NR to the scope  R4-1905151 [EMC] CR 38.113 editorials  R4-1905152 - Draft CR to TS 38.113 Correction reference TR 38.817-2  R4-1905154 [EMC] CR 38.113 exclusion updates, R15  Endorsed draft CRs in RAN4#91:  R4-1907703 Draft CR to TS 38.113 (subclause 3.2,3.3,4.4.2)  R4-1907705 Draft CR to TS 38.113 (subclause 8.2.1) | 15.6.0 |
| 2019-09 | RAN#85 | RP-192046 | 0012 |  | F | CR to 38.113 Editorial Corrections | 15.7.0 |
| 2019-12 | RAN#86 | RP-193036 | 0014 | 2 | F | CR to TS 38.113 Correction on abbreviations(subclause 3.3 & 8.2.1.2) | 15.8.0 |
| 2019-12 | RAN#86 | RP-193036 | 0015 | 2 | F | CR to TS 38.113 Correction on definitions subclause 3.1 | 15.8.0 |
| 2019-12 | RAN#86 | RP-193036 | 0016 | 2 | F | CR to TS 38.113 Editorial Corrections(clause 2 & subclause 3.1)\_r1 | 15.8.0 |
| 2020-03 | RAN#87 | RP-200399 | 0017 | 1 | F | CR to TS 38.113 Add the transmitter exclusion band for NR BS(subclause 4.4.1) | 15.9.0 |
| 2020-06 | RAN#88 | RP-200986 | 0020 | 1 | F | [R15]CR to TS 38.113 Add the reverberation chamber for radiated immunity testing (clause 2) | 15.10.0 |
| 2020-07 | RAN#88 | - | - | - | - | Update to Rel-16 version (MCC) | 16.0.0 |
| 2020-09 | RAN#89 | RP-201512 | 0022 |  | A | CR to TS 38.113: direct field strength measurements for the EMC RE, Rel-16 | 16.1.0 |
| 2020-12 | RAN#90 | RP-202488 | 0030 |  | A | CR to TS 38.113: correction of the scope and other technical improvements, Rel-16 | 16.2.0 |
| 2020-12 | RAN#90 | RP-202489 | 0024 | 1 | A | CR to TS 38.113 on Voltage dips and interruptions, Release 16 | 16.2.0 |
| 2021-03 | RAN#91 | RP-210117 | 0036 |  | A | CR to TS 38.113: Radiated emission test method | 16.3.0 |
| 2021-06 | RAN#92 | RP-211086 | 0038 |  | A | CR to TS 38.113: Radiated emission, ancillary equipment | 16.4.0 |
| 2021-06 | RAN#92 | RP-211081 | 0040 | 1 | A | CR to TS 38.113 on Performance criteria for transient phenomena, Release 16 | 16.4.0 |
| 2021-09 | RAN#93 | RP-211922 | 0044 |  | A | Big CR for TS 38.113 Maintenance (Rel-16, CAT A) | 16.5.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-03 | RAN#95 |  |  |  |  | Update to Rel-17 version (MCC) | 17.0.0 |
| 2022-06 | RAN#96 | RP-221655 | 0050 |  | A | Big CR for TS 38.113 Maintenance (Rel-17, CAT A) | 17.1.0 |
| 2022-09 | RAN#97 | RP-222023 | 0053 |  | F | Big CR for TS 38.113 Maintenance (Rel-17, CAT F) | 17.2.0 |
| 2023-03 | RAN#99 | RP-230505 | 0056 |  | A | TS 38.113: Corrections in clause 1 Scope and clause 9 Immunity | 17.3.0 |
| 2023-06 | RAN#100 | RP-231358 | 0058 | 1 | F | CR on TS 38.113 NR BS performance criteria | 17.4.0 |
| 2023-09 | RAN#101 | RP-232502 | 0062 |  | A | [NR\_newRAT-Core] CR on TS 38.113 NR BS reference maintenance R17 | 17.5.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2023-09 | RAN#101 | RP-232515 | 0059 |  | B | CR to TS 38.113 on introduction of 3 MHz channel bandwidth in clause 6.1 | 18.0.0 |
| 2023-12 | RAN#102 | RP-233372 | 0069 | 1 | F | [NR\_newRAT-Perf, TEI18] CR to TS 38.113: framework for the EMC-specific manufacturer's declarations, Rel-18 | 18.1.0 |
| 2024-03 | RAN#103 | RP-240555 | 0072 |  | A | (NB\_IOT, LTE\_LAA-Core (band 46), NR\_6GHz\_unlic\_full, NR\_6GHz\_unlic\_EU) CR to TS 38.113 on introduction of NR with in-band NB-IoT | 18.2.0 |