|  |  |
| --- | --- |
| 3GPP TS 38.412 V18.1.0(2024-06) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NG-RAN;  NG signalling transport  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  https://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 5

2 References 5

3 Definitions and abbreviations 5

3.1 Definitions 5

3.2 Abbreviations 6

4 NG signalling bearer 6

4.1 Functions and protocol stack 6

5 Data link layer 7

6 IP layer 7

7 Transport layer 7

Annex A (informative): Change history 9

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the standards for signalling transport to be used across NG interface. NG interface is a logical interface between the NG-RAN and the 5GC. The present document describes how the NGAP signalling messages are transported over NG.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] IETF RFC 4960: "Stream Control Transmission Protocol".

[3] 3GPP TS 23.501: "System Architecture for the 5G System".

[4] 3GPP TS 23.502: "Procedures for the 5G System".

[5] IETF RFC 8200 (2017-07): "Internet Protocol, Version 6 (IPv6) Specification".

[6] IETF RFC 791 (1981-09): "Internet Protocol".

[7] IETF RFC 2474 (1998-12): "Definition of the Differentiated Services Field (DS Field) in the IPv4 and IPv6 Headers".

[8] IETF RFC 6083 (2011-01): "Datagram Transport Layer Security (DTLS) for Stream Control Transmission Protocol (SCTP)".

[9] IETF RFC 6335 (2011-08): "Internet Assigned Numbers Authority (IANA) Procedures for the Management of the Service Name and Transport Protocol Port Number Registry".

[10] [IANA: "Stream Control Transmission Protocol (SCTP) Parameters", [https://www.iana.org/assignments/sctp-parameters/sctp-parameters.xhtml#sctp-parameters-25].](https://protect2.fireeye.com/v1/url?k=31323334-501cfaf3-313273af-454445554331-a3aa580897d3b339&q=1&e=6241cae7-b7ce-4642-9749-8f914a97c86d&u=http%3A%2F%2Fwww.openmobilealliance.org%2F)[11] IANA: “Service Name and Transport Protocol Port Number Registry”, [<https://www.iana.org/assignments/service-names-port-numbers/service-names-port-numbers.xhtml>].

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**NG:** interface between a NG-RAN node and a 5GC, providing an interconnection point between the NG-RAN and the 5GC.

**NG-C**: Reference point for the control plane protocol between NG-RAN and AMF.

**SCTP endpoint:** as defined in IETF RFC 4960 (2007-09) [5]

**SCTP association:** as defined in IETF RFC 4960 (2007-09) [5]

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

IP Internet Protocol

SCTP Stream Control Transmission Protocol

DiffServ Differentiated Service

PPP Point to Point Protocol

IANA Internet Assigned Number Authority

AMF Access and Mobility management Function

# 4 NG signalling bearer

## 4.1 Functions and protocol stack

NG-C signalling bearer provides the following functions:

- Provision of reliable transfer of NGAP message over NG-C interface.

- Provision of networking and routeing function.

- Provision of redundancy in the signalling network.

- Support for flow control and congestion control.

The protocol stack for NG-C Signalling Bearer is shown in figure 4.1-1 and details on each protocol are described in the following clauses.



Figure 4.1-1: NG-C signalling bearer protocol stack

The Transport Network Layer is based on IP transport, comprising SCTP on top of IP.

# 5 Data link layer

The support of any suitable Data Link Layer protocol, e.g. PPP, Ethernet, etc., shall not be prevented.

# 6 IP layer

The 5GC and NG-RAN shall support IPv6 (IETF RFC 8200 [5]) and/or IPv4 (IETF RFC 791 [6]).

The IP layer of NG-C only supports point-to-point transmission for delivering NG AP message.

The 5GC and NG-RAN shall support the Diffserv Code Point marking as described in IETF RFC 2474 [7].

# 7 Transport layer

SCTP (IETF RFC 4960 [2]) shall be supported as the transport layer of NG-C signalling bearer. The Payload Protocol Identifier (ppid) to be used by SCTP for the application layer protocol NGAP and for DTLS over SCTP (IETF RFC 6083 [8]) is assigned by IANA in [10]. The byte order of the ppid shall be big-endian.

SCTP refers to the Stream Control Transmission Protocol developed by the Sigtran working group of the IETF for the purpose of transporting various signalling protocols over IP network.

NG-RAN node and AMF shall support a configuration with a single SCTP association per NG-RAN node/AMF pair. Configurations with multiple SCTP endpoints per NG-RAN node/AMF pair should be supported. When configurations with multiple SCTP associations are supported, the AMF may request to dynamically add/remove SCTP associations between the NG-RAN node/AMF pair. Within the set of SCTP associations established between one AMF and NG-RAN node pair, the AMF may request the NG-RAN node to restrict the usage of SCTP association for certain types of NG-C signalling. If no restriction information is provided for an SCTP association, any type of NG-C signalling is allowed via the SCTP association. Selection of the SCTP association by the NG-RAN node and the AMF is specified in TS 23.501 [3] and TS 23.502 [4]. The NG-RAN node shall establish the SCTP association. The SCTP Destination Port number value to be used by NGAP is assigned by IANA in [11]. When the AMF requests to dynamically add additional SCTP associations between the NG-RAN node/AMF pair, the SCTP Destination Port number value may be the one assigned by IANA in [11], or any dynamic port value (IETF RFC 6335 [9]). When the configuration with multiple SCTP endpoints per NG-RAN node is supported and the NG-RAN node wants to add additional SCTP endpoints, the RAN configuration update procedure shall be the first NGAP procedure triggered on an additional TNLA of an already setup NG-C interface instance after the TNL association has become operational, and the AMF shall associate the TNLA to the NG-C interface instance using the included Global RAN node ID.

Between one AMF and NG-RAN node pair:

- A single pair of stream identifiers shall be reserved over at least one SCTP association for the sole use of NGAP elementary procedures that utilize non UE-associated signalling.

- At least one pair of stream identifiers over one or several SCTP associations shall be reserved for the sole use of NGAP elementary procedures that utilize UE-associated signallings. However, a few pairs (i.e. more than one) should be reserved.

- For a single UE-associated signalling, the NG-RAN node shall use one SCTP association and one SCTP stream, and the SCTP association/stream should not be changed during the communication of the UE-associated signalling until after current SCTP association is failed or removed, or TNL binding update is performed as described in TS 23.502 [3].

Transport network redundancy can be achieved by SCTP multi-homing between two end-points, of which one or both is assigned with multiple IP addresses. SCTP end-points shall support a multi-homed remote SCTP end-point. For SCTP endpoint redundancy, an SCTP endpoint (in the NG-RAN node or AMF) may send an INIT, at any time for an already established SCTP association, which the other SCTP endpoint shall handle as defined in IETF RFC 4960 [2] in subclause 5.2.

The SCTP congestion control may, using an implementation specific mechanism, initiate higher layer protocols to reduce the signalling traffic at the source and prioritise certain messages.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-01 | RAN3-AH-1801 | R3-180541 |  |  |  | Reflected agreed TP in RAN3-AH-1801 in 2018-01 (Sophia Antipolis) | 0.2.0 |
| 2018-03 | RAN3#99 | R3-181587 |  |  |  | Reflected agreed TP in RAN3#99 in 2018-03 (Athens) | 0.3.0 |
| 2018-05 | RAN3#100 | R3-183591 |  |  |  | Reflected agreed TP in RAN3#100 in 2018-05 (Busan) and made some editorial corrections | 0.4.0 |
| 2018-06 | RAN#80 | RP-180681 |  |  |  | Submitted to RAN plenary for Approval | 1.0.0 |
| 2018-06 | RAN#80 | - | - | - | - | Specification approved at TSG-RAN and placed under change control | 15.0.0 |
| 2018-09 | RAN#81 | RP-181920 | 0001 |  | F | Updated reference to IPv6 | 15.1.0 |
| 2018-09 | RAN#81 | RP-181922 | 0003 |  | F | NR Corrections (38.412 Baseline CR covering RAN3#101 agreements) | 15.1.0 |
| 2019-07 | RAN#84 | RP-191395 | 0008 | 1 | F | Clarify the support for multiple TNL Endpoints in the NG-RAN node | 15.2.0 |
| 2019-09 | RAN#85 | RP-192166 | 0010 | 1 | F | CR on PPID value for DTLS over SCTP | 15.3.0 |
| 2019-09 | RAN#85 | RP-192167 | 0011 | 1 | F | Use of SCTP ports for multiple TNLA | 15.3.0 |
| 2019-12 | RAN#86 | RP-192915 | 0012 | - | F | Ambiguity with multiple SCTP associations in 38.412 | 15.4.0 |
| 2020-03 | RAN#87-e | RP-200425 | 0013 | - | F | Rapporteur’s Update for 38.412 | 16.0.0 |
| 2020-09 | RAN#89-e | RP-201954 | 0015 | 2 | A | SCTP association change when current SCTP association is failed | 16.1.0 |
| 2022-03 | SA#95-e |  |  |  |  | Promotion to Release 17 without technical change | 17.0.0 |
| 2023-06 | RAN#100 | RP-231075 | 0021 | 2 | A | Corrections on TNL association addition, update and removal | 17.1.0 |
| 2024-03 | SA#103- | - | - | - | - | Update to Rel-18 version (MCC) | 18.0.0 |
| 2024-06 | RAN#104 | RP-241113 | 0022 | 2 | D | Correction on NGAP PPID and Destination Port Number over SCTP | 18.1.0 |