|  |  |
| --- | --- |
| 3GPP TS 38.521-1 V18.2.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) conformance specification;  Radio transmission and reception;  Part 1: Range 1 Standalone;  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 21

1 Scope 22

2 References 22

3 Definitions, symbols and abbreviations 23

3.1 Definitions 23

3.2 Symbols 24

3.3 Abbreviations 26

4 General 28

4.1 Relationship between minimum requirements and test requirements 28

4.2 Applicability of minimum requirements 28

4.3 Specification suffix information 29

4.4 Test points analysis 29

4.5 Applicability and test coverage rules 29

4.6 Pass fail decision rule of test case 29

5 Operating bands and Channel arrangement 30

5.1 General 30

5.2 Operating bands 30

5.2A Operating bands for CA 33

5.2A.1 Intra-band CA 33

5.2A.2 Inter-band CA 34

5.2A.2.1 Inter-band CA (two bands) 35

5.2A.2.2 Inter-band CA (three bands) 38

5.2A.2.3 Inter-band CA (four bands) 38

5.2B Operating bands for DC 39

5.2C Operating band combination for SUL 39

5.2D Operating bands for UL MIMO 40

5.2E Operating band for V2X 40

5.2E.1 V2X operating bands 40

5.2E.2 V2X operating bands for concurrent operation 41

5.2J Operating band for ATG 41

5.3 UE channel bandwidth 41

5.3.1 General 41

5.3.2 Maximum transmission bandwidth configuration 42

5.3.3 Minimum guard band and transmission bandwidth configuration 42

5.3.4 RB alignment 44

5.3.5 UE channel bandwidth per operating band 44

5.3.6 Asymmetric channel bandwidths 48

5.3A UE channel bandwidth for CA 49

5.3A.1 General 49

5.3A.2 Maximum transmission bandwidth configuration for CA 49

5.3A.3 Minimum guard band and transmission bandwidth configuration for CA 50

5.3A.4 Void 51

5.3A.5 UE channel bandwidth per operating band for CA 51

5.3E Channel bandwidth for V2X 52

5.3E.1 General 52

5.3E.2 Channel bandwidth for V2X concurrent operation 53

5.3I Channel bandwidth for RedCap 53

5.4 Channel arrangement 53

5.4.1 Channel spacing 53

5.4.1.1 Channel spacing for adjacent NR carriers 53

5.4.2 Channel raster 53

5.4.2.1 NR-ARFCN and channel raster 53

5.4.2.2 Channel raster to resource element mapping 54

5.4.2.3 Channel raster entries for each operating band 54

5.4.3 Synchronization raster 57

5.4.3.1 Synchronization raster and numbering 57

5.4.3.2 Synchronization raster to synchronization block resource element mapping 57

5.4.3.3 Synchronization raster entries for each operating band 58

5.4.4 TX–RX frequency separation 61

5.4A Channel arrangement for CA 62

5.4A.1 Channel spacing for CA 62

5.4A.2 Channel raster for CA 63

5.4A.3 Synchronization raster for CA 63

5.4A.4 Tx-Rx frequency separation for CA 63

5.4E Channel arrangement for V2X 63

5.4E.1 Channel spacing 63

5.4E.2 Channel raster 63

5.4E.2.1 NR-ARFCN and channel raster 63

5.4E.2.2 Channel raster to resource element mapping 64

5.4E.2.3 Channel raster entries for each operating band 64

5.4E.3 Synchronization raster for V2X 64

5.5 Void 64

5.5A Configurations for CA 64

5.5A.0 General 64

5.5A.1 Configurations for intra-band contiguous CA 64

5.5A.2 Configurations for intra-band non-contiguous CA 68

5.5A.3 Configurations for inter-band CA 68

5.5A.3.1 Configurations for inter-band CA (two bands) 69

5.5A.3.2 Configurations for inter-band CA (three bands) 79

5.5A.3.3 Configurations for inter-band CA (four bands) 86

5.5B Configurations for DC 88

5.5C Configurations for SUL 89

6 Transmitter characteristics 91

6.1 General 91

6.1A General 93

6.1E General 104

6.1F General 108

6.1J General 109

6.2 Transmitter power 109

6.2.1 UE maximum output power 109

6.2.2 UE maximum output power reduction 118

6.2.3 UE additional maximum output power reduction 151

6.2.4 Configured transmitted power 360

6.2A Transmitter power for CA 366

6.2A.1 UE maximum output power for CA 366

6.2A.1.0 Minimum conformance requirements 366

6.2A.1.0.1 Void 366

6.2A.1.0.2 Void 366

6.2A.1.0.3 UE maximum output power for Inter-band CA 366

6.2A.1.0.4 UE maximum output power for Intra-band contiguous CA 369

6.2A.1.0.5 UE maximum output power for Intra-band non-contiguous CA 370

6.2A.1.1 UE maximum output power for CA (2UL CA) 370

6.2A.2 UE maximum output power reduction for CA 375

6.2A.2.0 Minimum conformance requirements 375

6.2A.2.0.1 FFS 375

6.2A.2.0.2 FFS 375

6.2A.2.0.3 Maximum Power Reduction for Inter-band CA 375

6.2A.2.0.4 Maximum Power Reduction for Intra-band contiguous CA 375

6.2A.2.0.5 Maximum Power Reduction for Intra-band non-contiguous CA 378

6.2A.2.1 UE maximum output power reduction for CA (2UL CA) 380

6.2A.3 UE additional maximum output power reduction for CA 405

6.2A.3.0 Minimum conformance requirements 405

6.2A.3.0.1 UE additional maximum output power reduction for Intra-band contiguous CA 405

6.2A.3.0.1.1 A-MPR for CA\_NS\_04 406

6.2A.3.0.1.1.2 Non-contiguous allocations 406

6.2A.3.0.1.1.3 AMPRIM3 to meet -25dBm/MHz 407

6.2A.3.0.2 FFS 407

6.2A.3.0.3 UE additional maximum output power reduction for inter-band CA 407

6.2A.3.1 UE additional maximum output power reduction for CA (2UL CA) 409

6.2A.4 Configured output power for CA 420

6.2A.4.0 Minimum conformance requirements 420

6.2A.4.0.1 Configured transmitted power level 420

6.2A.4.0.2 ΔTIB,c for CA 427

6.2A.4.0.2.1 FFS 428

6.2A.4.0.2.2 FFS 428

6.2A.4.0.2.3 ΔTIB,c for Inter-band CA 428

6.2A.4.1 Configured transmitted power for CA (2UL CA) 432

6.2B Transmitter power for NR-DC 439

6.2B.0 General 439

6.2B.1 UE maximum output power for NR-DC 439

6.2B.1.0 Minimum conformance requirements 439

6.2B.1.0.1 FFS 439

6.2B.1.0.2 FFS 439

6.2B.1.0.3 UE maximum output power for inter-band NR-DC 439

6.2B.1.1 UE maximum output power for NR-DC 439

6.2B.2 UE maximum output power reduction for NR-DC 442

6.2B.2.0 Minimum conformance requirements 442

6.2B.2.0.1 FFS 442

6.2B.2.0.2 FFS 442

6.2B.2.0.3 UE maximum output power reduction for Inter-band NR-DC 442

6.2B.2.1 UE maximum output power reduction for NR-DC 442

6.2B.3 UE additional maximum output power reduction for NR-DC 443

6.2B.3.0 Minimum conformance requirements 443

6.2B.3.0.1 FFS 443

6.2B.3.0.2 FFS 443

6.2B.3.0.3 UE additional maximum output power reduction for inter-band NR-DC 443

6.2B.3.1 UE additional maximum output power reduction for NR-DC 444

6.2B.4 Configured output power for NR-DC 445

6.2B.4.0 Minimum conformance requirements 445

6.2B.4.0.1 Configured transmitted power level for NR-DC 445

6.2B.4.0.2 ΔTIB,c for NR-DC 448

6.2B.4.0.2.1 FFS 449

6.2B.4.0.2.2 FFS 449

6.2B.4.0.2.3 Void 449

6.2B.4.1 Configured transmitted power level for NR-DC 449

6.2C Transmitter power for SUL 451

6.2C.1 Configured transmitted power for SUL 451

6.2C.2 ΔTIB,c 455

6.2C.3 UE maximum output power for SUL 455

6.2C.3\_1 Void 458

6.2C.4 UE maximum output power reduction for SUL 458

6.2C.5 UE additional maximum output power reduction for SUL 469

6.2D Transmitter power for UL MIMO 508

6.2D.1 UE maximum output power for UL MIMO 508

6.2D.1\_1 UE maximum output power for SUL with UL MIMO 513

6.2D.2 UE maximum output power reduction for UL MIMO 465

6.2D.2\_1 UE maximum output power reduction for SUL with UL MIMO 491

6.2D.3 UE additional maximum output power reduction for UL MIMO 496

6.2D.3\_1 UE additional maximum output power reduction for SUL with UL MIMO 548

6.2D.4 Configured transmitted power for UL MIMO 561

6.2D.4\_1 Configured transmitted power for SUL with UL MIMO 565

6.2E Transmitter power for V2X 568

6.2E.1 UE maximum output power for V2X 568

6.2E.1.0 Minimum conformance requirements 568

6.2E.1.1 UE maximum output power for V2X / non-concurrent operation 569

6.2E.1.1D UE maximum output power for V2X / non-concurrent operation / SL-MIMO 569

6.2E.2 UE maximum output power reduction for V2X 569

6.2E.2.0 Minimum conformance requirements 569

6.2E.2.1 UE maximum output power reduction for V2X / non-concurrent operation 571

6.2E.2.1D UE maximum output power reduction for V2X / non-concurrent operation / SL-MIMO 575

6.2E.2.2 UE maximum output power reduction for V2X / concurrent operation 578

6.2E.3 UE additional maximum output power reduction for V2X 580

6.2E.3.0 Minimum conformance requirements 580

6.2E.3.1 UE additional maximum output power reduction for V2X / non-concurrent operation 586

6.2E.3.1D UE additional maximum output power reduction for V2X / non-concurrent operation / SL-MIMO 599

6.2E.3.2 UE maximum output power reduction for V2X / concurrent operation 607

6.2F Transmitter power for shared spectrum channel access 608

6.2F.1 UE maximum output power for shared spectrum channel access 608

6.2F.1A UE maximum output power for CA for shared spectrum access 611

6.2F.2 UE maximum output power reduction for shared spectrum access 612

6.2F.3 UE additional maximum output power reduction for shared spectrum access 616

6.2F.4 Configured transmitted power for shared spectrum access 627

6.2G Transmitter power for Tx Diversity 629

6.2G.1 UE maximum output power for Tx Diversity 629

6.2G.2 UE maximum output power reduction for Tx Diversity 642

6.2G.3 UE additional maximum output power reduction for Tx Diversity 677

6.2G.4 Configured transmitted power for Tx Diversity 696

6.2H Transmitter power for CA with UL MIMO 701

6.2H.1 Transmitter power for intra-band UL contiguous CA with UL MIMO 701

6.2H.1.1 UE maximum output power for intra-band UL contiguous CA with UL MIMO 701

6.2H.1.2 UE maximum output power reduction for intra-band UL contiguous CA with UL MIMO 702

6.2H.1.3 UE additional maximum output power reduction for intra-band UL contiguous CA with UL MIMO 705

6.2H.1.4 Configured transmitted power for intra-band UL contiguous CA with UL MIMO 709

6.2H.2 713

6.2H.3 Transmitter power for inter-band UL CA with UL MIMO 713

6.2H.3.1 UE maximum output power for inter-band UL CA with UL MIMO 713

6.2H.3.2 UE maximum output power reduction for inter-band UL CA with UL MIMO 713

6.2I Transmitter power for RedCap 713

6.2I.1 UE maximum output power for RedCap 713

6.2I.2 Void 715

6.2I.3 Void 715

6.2I.4 Void 715

6.2J Transmitter power for ATG 715

6.2J.1 UE maximum output power for ATG 715

6.2J.2 Configured transmitted power 717

6.3 Output power dynamics 720

6.3.1 Minimum output power 720

6.3.2 Transmit OFF power 722

6.3.3 Transmit ON/OFF time mask 723

6.3.3.1 General 723

6.3.3.2 General ON/OFF time mask 724

6.3.3.3 Transmit power time mask for slot and short or subslot boundaries 728

6.3.3.4 PRACH time mask 728

6.3.3.5 Void 735

6.3.3.6 SRS time mask 735

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 746

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 746

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 746

6.3.4 Power control 746

6.3.4.1 General 746

6.3.4.2 Absolute power tolerance 746

6.3.4.3 Relative power tolerance 749

6.3.4.4 Aggregate power tolerance 765

6.3A Output power dynamics for CA 822

6.3A.1 Minimum output power for CA 822

6.3A.1.0 Minimum conformance requirements 822

6.3A.1.1 Minimum output power for CA (2UL CA) 822

6.3A.2 Transmit OFF power for CA 825

6.3A.2.0 Minimum conformance requirements 825

6.3A.2.1 Transmit OFF power for CA (2UL CA) 826

6.3A.3 Transmit ON/OFF time mask for CA 827

6.3A.3.0 Minimum conformance requirements 827

6.3A.3.0.1 Transmit ON/OFF time mask for intra-band contiguous CA 827

6.3A.3.0.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 827

6.3A.3.0.3 Transmit ON/OFF time mask for inter-band CA 827

6.3A.3.1 Transmit ON/OFF time mask for CA (2UL CA) 832

6.3A.3.1\_1 Void 839

6.3A.3.2 Time mask for switching between two uplink carriers 839

6.3A.3.3 Time mask for switching between two uplink carriers with two transmit antenna connectors 844

6.3A.3.4 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors (3UL CA) 848

6.3A.3.5 Time mask for switching between two uplink bands with two transmit antenna connectors (3UL CA) 853

6.3A.4 Power control for CA 860

6.3A.4.1 Absolute power tolerance for CA 860

6.3A.4.1.0 Minimum conformance requirements 860

6.3A.4.1.1 Absolute power tolerance for CA (2UL CA) 860

6.3A.4.2 Relative power tolerance for CA 863

6.3A.4.2.0 Minimum conformance requirements 863

6.3A.4.2.1 Relative power tolerance for CA (2UL CA) 864

6.3A.4.3 Aggregate power tolerance for CA 872

6.3A.4.3.0 Minimum conformance requirements 872

6.3A.4.3.1 Aggregate power tolerance for CA (2UL CA) 872

6.3B Output power dynamics for NR-DC 877

6.3B.1 Minimum output power for NR-DC 877

6.3B.2 Transmit OFF power for NR-DC 877

6.3B.3 Transmit ON/OFF time mask for NR-DC 877

6.3C Output power dynamics for SUL 877

6.3C.1 Minimum output power for SUL 877

6.3C.2 Transmit OFF power for SUL 879

6.3C.3 Transmit ON/OFF time mask for SUL 879

6.3C.3.0 Minimum conformance requirements 879

6.3C.3.0.1 General ON/OFF time mask for SUL 879

6.3C.3.0.2 Time mask for switching between two uplink carriers 880

6.3C.3.0.3 Time mask for switching between two uplink carriers with two transmit antenna connectors 881

6.3C.3.0.4 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 882

6.3C.3.0.5 Time mask for switching between two uplink carriers 883

6.3C.3.1 General transmit ON/OFF time mask for SUL 884

6.3C.3.2 General transmit ON/OFF time mask for switching between two uplink carriers 886

6.3C.3.3 General transmit ON/OFF time mask for switching between two uplink carriers with two transmit antenna connectors 890

6.3C.3.4 General transmit ON/OFF time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 894

6.3C.3.5 General transmit ON/OFF time mask for switching between two uplink bands with two transmit antenna connectors 899

6.3C.4 Power control for SUL 904

6.3C.4.1 Absolute power tolerance for SUL 904

6.3C.4.2 Relative power tolerance for SUL 906

6.3C.4.3 Aggregate power tolerance for SUL 914

6.3D Output power dynamics for UL MIMO 917

6.3D.1 Minimum output power for UL MIMO 917

6.3D.1\_1 Minimum output power for SUL with UL MIMO 919

6.3D.2 Transmit OFF power for UL MIMO 921

6.3D.2\_1 Transmit OFF power for SUL with UL MIMO 923

6.3D.3 Transmit ON/OFF time mask for UL MIMO 924

6.3D.3\_1 Transmit ON/OFF time mask for SUL with UL MIMO 928

6.3D.4 Power control for UL MIMO 933

6.3D.4.1 Absolute power tolerance for UL MIMO 933

6.3D.4.1\_1 Absolute power tolerance for SUL with UL MIMO 937

6.3D.4.2 Relative power tolerance for UL MIMO 940

6.3D.4.2\_1 Relative power tolerance for SUL with UL MIMO 951

6.3D.4.3 Aggregate power tolerance for UL MIMO 958

6.3D.4.3\_1 Aggregate power tolerance for SUL with UL MIMO 960

6.3E Output power dynamics for V2X 962

6.3E.1 Minimum output power for V2X 962

6.3E.1.0 Minimum conformance requirements 962

6.3E.1.1 Minimum output power for V2X / non-concurrent operation 962

6.3E.1.1D Minimum output power for V2X / non-concurrent operation / SL-MIMO 964

6.3E.2 Transmit OFF power for V2X 967

6.3E.2.0 Minimum conformance requirements 967

6.3E.2.1 Transmit OFF power for V2X / non-concurrent operation 967

6.3E.2.1D Transmit OFF power for V2X / non-concurrent operation / SL-MIMO 968

6.3E.2.2 Transmit OFF power for V2X / con-current operation 969

6.3F Output power dynamics for shared spectrum channel access 969

6.3F.1 Minimum output power 969

6.3F.2 Transmit OFF power for shared spectrum channel access 972

6.3F.3 Transmit ON/OFF time mask for shared spectrum channel access 973

6.3F.3.1 General 973

6.3F.3.2 General ON/OFF time mask 973

6.3F.4 Power control for shared spectrum access 976

6.3F.4.1 General 976

6.3F.4.2 Absolute power tolerance for shared spectrum access 976

6.3F.4.3 Relative power tolerance for shared spectrum channel access 979

6.3G Output power dynamics for Tx Diversity 990

6.3G.1 Minimum output power for Tx Diversity 990

6.3G.2 Transmit OFF power for Tx Diversity 991

6.3G.3 Transmit ON/OFF time mask for Tx Diversity 992

6.3G.3.1 General ON/OFF time mask for Tx Diversity 992

6.3G.3.2 PRACH time mask for Tx Diversity 994

6.3G.3.3 SRS time mask for Tx Diversity 996

6.3G.4 Power control for Tx Diversity 998

6.3G.4.1 Absolute power tolerance for Tx Diversity 998

6.3G.4.2 Relative power tolerance for Tx Diversity 999

6.3G.4.3 Aggregate power tolerance for Tx Diversity 1007

6.3H Output power dynamics for CA with UL MIMO 1008

6.3H.1 Output power dynamics for intra-band UL contiguous CA with UL MIMO 1008

6.3H.1.1 Minimum output power for intra-band UL contiguous CA with UL MIMO 1008

6.3H.1.2 Transmit OFF power for intra-band UL contiguous CA with UL MIMO 1010

6.3H.1.3 Transmit ON/OFF time mask for intra-band UL contiguous CA with UL MIMO 1011

6.3H.1.4 Power control for intra-band UL contiguous CA with UL MIMO 1017

6.3H.1.4.0 Minimum conformance requirements 1017

6.3H.1.4.1 Absolute power tolerance for intra-band UL contiguous CA with UL MIMO 1017

6.3H.1.4.2 Relative power tolerance for intra-band UL contiguous CA with UL MIMO 1017

6.3H.1.4.3 Aggregate power tolerance for intra-band UL contiguous CA with UL MIMO 1018

6.3J Output power dynamics for ATG 1018

6.3J.1 Minimum output power for ATG 1018

6.3J.2 Transmit OFF power for ATG 1021

6.4 Transmit signal quality 1022

6.4.1 Frequency error 1022

6.4.2 Transmit modulation quality 1024

6.4.2.1 Error Vector Magnitude 1024

6.4.2.1a Error Vector Magnitude including symbols with transient period 1032

6.4.2.2 Carrier leakage 1036

6.4.2.3 In-band emissions 1040

6.4.2.4 EVM equalizer spectrum flatness 1046

6.4.2.5 EVM equalizer spectrum flatness for Pi/2 BPSK 1049

6.4.2.6 Phase continuity requirements for DMRS bundling 1053

6.4A Transmit signal quality for CA 1057

6.4A.1 Frequency error for CA 1057

6.4A.1.0 Minimum conformance requirements 1057

6.4A.1.1 Frequency error for CA (2UL CA) 1057

6.4A.2 Transmit modulation quality for CA 1060

6.4A.2.0 General 1060

6.4A.2.0.1 Transmit modulation quality for intra-band contiguous CA 1060

6.4A.2.0.2 Transmit modulation quality for intra-band contiguous CA 1060

6.4A.2.1 Error Vector Magnitude for CA 1061

6.4A.2.1.0 Minimum conformance requirements 1061

6.4A.2.1.1 Error Vector Magnitude for CA (2UL CA) 1061

6.4A.2.2 Carrier leakage for CA 1065

6.4A.2.2.0 Minimum conformance requirements 1065

6.4A.2.2.1 Carrier leakage for CA (2UL CA) 1066

6.4A.2.3 In-band emissions for CA 1069

6.4A.2.3.0 Minimum conformance requirements 1069

6.4A.2.3.1 In-band emissions for CA (2UL CA) 1074

6.4B Transmit signal quality for NR-DC 1082

6.4B.1 Frequency error for NR-DC 1082

6.4B.2 Transmit modulation quality for NR-DC 1082

6.4B.2.1 Error Vector Magnitude for NR-DC 1082

6.4B.2.2 Carrier leakage for NR-DC 1082

6.4B.2.3 In-band emissions for NR-DC 1082

6.4C Transmit signal quality for SUL 1082

6.4C.1 Frequency error for SUL 1082

6.4C.2 Transmit modulation quality for SUL 1084

6.4C.2.1 Error Vector Magnitude for SUL 1084

6.4C.2.2 Carrier leakage for SUL 1086

6.4C.2.3 In-band emissions for SUL 1087

6.4C.2.4 EVM equalizer spectrum flatness for SUL 1089

6.4C.2.5 EVM equalizer spectrum flatness for Pi/2 BPSK for SUL 1090

6.4D Transmit signal quality for UL MIMO 1092

6.4D.1 Frequency error for UL MIMO 1092

6.4D.1\_1 Frequency error for SUL with UL MIMO 1094

6.4D.2 Transmit modulation quality for UL MIMO 1096

6.4D.2.1 Error Vector Magnitude for UL MIMO 1096

6.4D.2.1\_1 Error Vector Magnitude for SUL with UL MIMO 1100

6.4D.2.2 Carrier leakage for UL MIMO 1102

6.4D.2.2\_1 Carrier leakage for SUL with UL MIMO 1105

6.4D.2.3 In-band emissions for UL MIMO 1107

6.4D.2.3\_1 In-band emissions for SUL with UL MIMO 1110

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 1112

6.4D.2.4\_1 EVM equalizer spectrum flatness for SUL with UL MIMO 1115

6.4D.3 Time alignment error for UL MIMO 1118

6.4D.3\_1 Time alignment error for SUL with UL MIMO 1120

6.4D.4 Requirements for coherent UL MIMO 1121

6.4E Transmit signal quality for V2X 1124

6.4E.1 Frequency error for V2X 1124

6.4E.2 Transmit modulation quality for V2X 1124

6.4E.2.1 General 1124

6.4E.2.2 Error Vector Magnitude for V2X 1124

6.4E.2.2.1 Error Vector Magnitude for V2X / non-concurrent operation 1124

6.4E.2.2.1D Error Vector Magnitude for V2X / non-concurrent operation / SL-MIMO 1125

6.4E.2.4 In-band emissions for V2X 1127

6.4E.2.4.1 In-band emissions for V2X / non-concurrent operation 1127

6.4E.2.4.1D In-band emissions for V2X / non-concurrent operation / SL-MIMO 1130

6.4E.2.4.2 In-band emissions for V2X / con-current operation 1131

6.4E.2.5 EVM equalizer spectrum flatness for V2X 1133

6.4E.2.5.1 EVM equalizer spectrum flatness for V2X / non-concurrent operation 1133

6.4E.2.5.1D EVM equalizer spectrum flatness for V2X / non-concurrent operation / SL-MIMO 1135

6.4E.2.5.2 EVM equalizer spectrum flatness for V2X / con-current operation 1136

6.4F Transmit signal quality for shared spectrum channel access 1138

6.4F.1 Frequency error 1138

6.4F.2 Transmit modulation quality 1139

6.4F.2.0 General 1139

6.4F.2.1 Error Vector Magnitude 1139

6.4F.2.2 Carrier leakage 1142

6.4F.2.3 In-band emissions 1145

6.4F.2.4 EVM equalizer spectrum flatness 1151

6.4G Transmit signal quality for Tx Diversity 1154

6.4G.1 Frequency error for Tx Diversity 1154

6.4G.2 Transmit modulation quality for Tx Diversity 1154

6.4G.2.1 Error Vector Magnitude for Tx Diversity 1155

6.4G.2.2 Carrier leakage for Tx Diversity 1158

6.4G.2.3 In-band emissions for Tx Diversity 1159

6.4G.2.4 EVM equalizer spectrum flatness for Tx Diversity 1161

6.4H Transmit signal quality for CA with UL MIMO 1163

6.4H.1 Transmit signal quality for intra-band UL contiguous CA with UL MIMO 1163

6.4H.1.1 Frequency error for intra-band UL contiguous CA with UL MIMO 1163

6.4H.1.2 Transmit modulation quality for intra-band UL contiguous CA with UL MIMO 1165

6.4H.1.2.0 General 1165

6.4H.1.2.1 Error Vector Magnitude for intra-band UL contiguous CA with UL MIMO 1165

6.4H.1.2.2 Carrier leakage for intra-band UL contiguous CA with UL MIMO 1167

6.4H.1.2.3 In-band emissions for intra-band UL contiguous CA with UL MIMO 1169

6.4H.1.3 Time alignment error for intra-band UL contiguous CA with UL MIMO 1174

6.4H.1.4 Coherent UL MIMO for intra-band UL contiguous CA with UL MIMO 1176

6.5 Output RF spectrum emissions 1178

6.5.0 General 1178

6.5.1 Occupied bandwidth 1178

6.5.2 Out of band emission 1180

6.5.2.1 General 1180

6.5.2.2 Spectrum emission mask 1181

6.5.2.3 Additional spectrum emission mask 1189

6.5.2.4 Adjacent channel leakage ratio 1196

6.5.2.4.1 NR ACLR 1196

6.5.2.4.2 UTRA ACLR 1200

6.5.3 Spurious emissions 1201

6.5.3.1 General spurious emissions 1202

6.5.3.2 Spurious emissions for UE co-existence 1204

6.5.3.3 Additional spurious emissions 1240

6.5.4 Transmit intermodulation 1267

6.5A Output RF spectrum emissions for CA 1270

6.5A.1 Occupied bandwidth for CA 1270

6.5A.1.0 Minimum conformance requirements 1270

6.5A.1.0.1 Void 1270

6.5A.1.0.1a Occupied bandwidth for Intra-band contiguous CA 1270

6.5A.1.0.2 Occupied bandwidth for Intra-band non-contiguous CA 1270

6.5A.1.0.3 Occupied bandwidth for Inter-band CA 1270

6.5A.1.1 Occupied bandwidth for CA (2UL CA) 1270

6.5A.2 Out of band emission for CA 1273

6.5A.2.1 General 1273

6.5A.2.2 Spectrum emission mask 1273

6.5A.2.2.0 Minimum conformance requirements 1274

6.5A.2.2.1 Spectrum emission mask for CA (2UL CA) 1274

6.5A.2.3 Additional spectrum emission mask for CA 1280

6.5A.2.3.0 Minimum conformance requirements 1280

6.5A.2.3.1 Additional spectrum emission mask for CA (2UL CA) 1280

6.5A.2.4 Adjacent channel leakage ratio 1282

6.5A.2.4.1 NR ACLR 1282

6.5A.2.4.1.0 Minimum conformance requirements 1282

6.5A.2.4.1.0.3 NR ACLR for Inter-band CA 1283

6.5A.2.4.1.1 NR ACLR for CA (2UL CA) 1284

6.5A.2.4.2 UTRA ACLR 1287

6.5A.2.4.2.0 Minimum conformance requirements 1287

6.5A.2.4.2.1 UTRA ACLR for CA (2UL CA) 1287

6.5A.3 Spurious emission for CA 1289

6.5A.3.1 General spurious emissions for CA 1289

6.5A.3.1.0 Minimum conformance requirements 1289

6.5A.3.1.1 General spurious emissions for CA (2UL CA) 1290

6.5A.3.2 Spurious emission for UE co-existence 1302

6.5A.3.2.0 Minimum conformance requirements 1302

6.5A.3.2.0.0 General 1302

6.5A.3.2.0.1 Spurious emissions for UE co-existence for intra-band contiguous CA 1302

6.5A.3.2.0.2 Void 1306

6.5A.3.2.0.2a Spurious emissions for UE co-existence for Intra-band non-contiguous CA 1306

6.5A.3.2.0.3 Spurious emissions for UE co-existence for Inter-band CA 1306

6.5A.3.2.1 Spurious emissions for UE co-existence for CA (2UL CA) 1314

6.5A.3.3 Additional spurious emissions for CA 1327

6.5A.3.3.0 Minimum conformance requirements 1327

6.5A.3.3.1 Additional spurious emissions for CA (2UL CA) 1327

6.5A.4 Transmit intermodulation for CA 1329

6.5A.4.0 Minimum conformance requirements 1329

6.5A.4.1 Transmit intermodulation for CA (2UL CA) 1330

6.5B Output RF spectrum emissions for NR-DC 1333

6.5B.1 Occupied bandwidth for NR-DC 1333

6.5B.2 Out of band emission for NR-DC 1333

6.5B.2.1 General 1333

6.5B.2.2 Spectrum emission mask 1334

6.5B.2.4 Adjacent channel leakage ratio 1334

6.5B.3 Spurious emission for NR-DC 1334

6.5B.4 Transmit intermodulation for NR-DC 1334

6.5C Output RF spectrum emissions for SUL 1334

6.5C.1 Occupied bandwidth for SUL 1334

6.5C.2 Out of band emission for SUL 1335

6.5C.2.1 General 1335

6.5C.2.2 Spectrum emission mask for SUL 1335

6.5C.2.3 Additional spectrum emission mask for SUL 1339

6.5C.2.4 Adjacent channel leakage ratio for SUL 1340

6.5C.2.4.1 NR ACLR for SUL 1340

6.5C.2.4.2 UTRA ACLR for SUL 1341

6.5C.3 Spurious emissions for SUL 1342

6.5C.3.1 General spurious emissions for SUL 1342

6.5C.3.2 Spurious emissions for UE co-existence for SUL 1344

6.5C.3.3 Additional spurious emissions for SUL 1345

6.5C.4 Transmit intermodulation for SUL 1362

6.5D Output RF spectrum emissions for UL MIMO 1364

6.5D.1 Occupied bandwidth for UL MIMO 1364

6.5D.1\_1 Void 1366

6.5D.1\_2 Occupied bandwidth for SUL with UL MIMO 1366

6.5D.2 Out of band emission for UL MIMO 1368

6.5D.2.1 General 1368

6.5D.2.2 Spectrum emission mask for UL MIMO 1368

6.5D.2.2\_1 Spectrum emission mask for SUL with UL MIMO 1374

6.5D.2.3 Additional spectrum emission mask for UL MIMO 1379

6.5D.2.4 Adjacent channel leakage ratio for UL MIMO 1382

6.5D.2.4.1 NR ACLR for UL MIMO 1382

6.5D.2.4.1\_1 NR ACLR for SUL with UL MIMO 1384

6.5D.2.4.2 UTRA ACLR for UL MIMO 1385

6.5D.2.4.2\_1 UTRA ACLR for SUL with UL MIMO 1387

6.5D.2\_1 Void 1391

6.5D.3 Spurious emissions for UL MIMO 1391

6.5D.3.1 General spurious emissions for UL MIMO 1391

6.5D.3.2 Spurious emissions for UE co-existence for UL MIMO 1393

6.5D.3.3 Additional spurious emissions for UL MIMO 1395

6.5D.3\_1 Spurious emissions for UL MIMO (Rel-16 onward) 1401

6.5D.3\_1.1 General spurious emissions for UL MIMO (Rel-16 onward) 1401

6.5D.3\_1.2 Spurious emission for UE co-existence for UL MIMO (Rel-16 onward) 1402

6.5D.3\_1.3 Additional spurious emissions for UL MIMO (Rel-16 onward) 1403

6.5D.3\_2 Spurious emissions for SUL with UL MIMO 1406

6.5D.3\_2.1 General spurious emissions for SUL with UL MIMO 1406

6.5D.3\_2.2 Spurious emissions for UE co-existence for SUL with UL MIMO 1408

6.5D.3\_2.3 Additional spurious emissions for SUL with UL MIMO 1410

6.5D.4 Transmit intermodulation for UL MIMO 1415

6.5D.4\_1 Transmit intermodulation for SUL with UL MIMO 1417

6.5E Output RF spectrum emissions for V2X 1419

6.5E.1 Occupied bandwidth for V2X 1419

6.5E.2 Out of band emission for V2X 1419

6.5E.2.1 General 1419

6.5E.2.2 Spectrum emission mask for V2X 1419

6.5E.2.2.1 Spectrum emission mask for V2X / non-concurrent operation 1419

6.5E.2.2.1D Spectrum emission mask for V2X / non-concurrent operation / SL-MIMO 1423

6.5E.2.3 Additional Spectrum emission mask for V2X 1426

6.5E.2.3.0 Minimum conformance requirements 1426

6.5E.2.3.1 Additional Spectrum emission mask for V2X / non-concurrent operation 1427

6.5E.2.3.1D Additional Spectrum emission mask for V2X / non-concurrent operation / SL-MIMO 1430

6.5E.2.4 Adjacent channel leakage ratio for V2X 1432

6.5E.2.4.1 Adjacent channel leakage ratio for V2X / non-concurrent operation 1432

6.5E.2.4.1D Adjacent channel leakage ratio for V2X / non-concurrent operation / SL-MIMO 1435

6.5E.3 Spurious emissions for V2X 1437

6.5E.3.1 General spurious emissions for V2X 1437

6.5E.3.2 Spurious emissions for UE co-existence for V2X 1437

6.5E.3.2.1 Spurious emissions for UE co-existence for V2X / non-concurrent operation 1437

6.5E.3.2.1D Spurious emissions for UE co-existence for V2X / non-concurrent operation / SL-MIMO 1438

6.5E.3.3 Additional spurious emissions requirements for V2X 1439

6.5E.3.3.0 Minimum conformance requirements 1439

6.5E.3.3.0.1 Requirements for network signalling value "NS\_33" 1439

6.5E.3.3.1 Additional spurious emissions requirements for V2X / non-concurrent operation 1440

6.5F Output RF spectrum emissions for shared spectrum channel access 1442

6.5F.1 Occupied bandwidth for shared spectrum channel access 1442

6.5F.2 Out of band emission for shared spectrum channel access 1444

6.5F.2.1 General 1444

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 1444

6.5F.2.4 Adjacent channel leakage ratio for operation with shared spectrum channel access 1448

6.5F.2.4.1 Shared spectrum channel access ACLR 1448

6.5F.2.4.2 Shared spectrum channel access ACLR with additional requirement for NS\_29 1450

6.5F.3 Spurious emissions for shared spectrum channel access 1452

6.5F.3.1 General spurious emissions 1452

6.5F.3.2 Spurious emissions for UE co-existence 1454

6.5F.3.3 Additional spurious emissions for shared spectrum channel access 1454

6.5F.4 Transmit intermodulation for shared spectrum channel access 1460

6.5G Output RF spectrum emissions for Tx Diversity 1462

6.5G.1 Occupied bandwidth for Tx Diversity 1462

6.5G.2 Out of band emission for Tx Diversity 1463

6.5G.2.1 Spectrum emission mask for Tx Diversity 1463

6.5G.2.2 Additional spectrum emission mask for Tx Diversity 1471

6.5G.2.3 Adjacent channel leakage ratio for Tx Diversity 1474

6.5G.2.3.1 NR ACLR for Tx Diversity 1474

6.5G.2.3.2 UTRA ACLR for Tx Diversity 1476

6.5G.3 Spurious emission for Tx Diversity 1477

6.5G.3.1 General spurious emissions for Tx Diversity 1477

6.5G.3.2 Spurious emissions for UE co-existence for Tx Diversity 1478

6.5G.3.3 Additional spurious emissions for Tx Diversity 1479

6.5G.4 Transmit intermodulation for Tx Diversity 1480

6.5H Output RF spectrum emissions for CA with UL MIMO 1481

6.5H.1 Output RF spectrum emissions for intra-band UL contiguous CA with UL MIMO 1481

6.5H.1.1 Occupied bandwidth for intra-band UL contiguous CA for UL MIMO 1481

6.5H.1.2 Out of band emission for intra-band UL contiguous CA for UL MIMO 1483

6.5H.1.2.0 Minimum conformance requirements 1483

6.5H.1.2.1 Spectrum emission mask for intra-band UL contiguous CA for UL MIMO 1483

6.5H.1.2.2 Additional spectrum emission mask for intra-band UL contiguous CA for UL MIMO 1485

6.5H.1.2.3 NR ACLR for intra-band UL contiguous CA for UL MIMO 1487

6.5H.1.3 Spurious emission for intra-band UL contiguous CA for UL MIMO 1489

6.5H.1.3.0 Minimum conformance requirements 1489

6.5H.1.3.1 General spurious emissions for intra-band UL contiguous CA for UL MIMO 1489

6.5H.1.3.2 Spurious emissions for UE co-existence for intra-band UL contiguous CA for UL MIMO 1491

6.5H.1.3.3 Additional spurious emissions for intra-band UL contiguous CA for UL MIMO 1494

6.5H.1.4 Transmit intermodulation for intra-band UL contiguous CA for UL MIMO 1495

6.5J Output RF spectrum emissions for ATG 1497

6.5J.0 General 1497

6.5J.1 Occupied bandwidth for ATG 1498

6.5J.2 Out of band emission for ATG 1500

6.5J.2.1 General 1500

6.5J.3 Spurious emissions for ATG 1500

6.5J.3.0 General 1500

6.5J.3.1 General spurious emissions for ATG 1500

7 Receiver characteristics 1503

7.1 General 1503

7.1A General 1504

7.1I General 1504

7.1J General for ATG 1504

7.2 Diversity characteristics 1504

7.2J Diversity characteristics for ATG 1504

7.3 Reference sensitivity 1504

7.3.1 General 1504

7.3.2 Reference sensitivity power level 1505

7.3.3 ΔRIB,c 1371

7.3A Reference sensitivity for CA 1371

7.3A.0 Minimum conformance requirements 1372

7.3A.0.1 General 1372

7.3A.0.2 Reference sensitivity power level for CA 1372

7.3A.0.2.1 Reference sensitivity power level for Intra-band contiguous CA 1372

7.3A.0.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 1372

7.3A.0.2.3 Reference sensitivity power level for Inter-band CA 1373

7.3A.0.2.4 Void 1373

7.3A.0.3 ΔRIB,c for CA 1374

7.3A.0.3.1 General 1374

7.3A.0.3.2 ΔRIB,c for Inter-band CA 1374

7.3A.0.4 Reference sensitivity exceptions due to UL harmonic interference for CA 1380

7.3A.0.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 1385

7.3A.0.6 Reference sensitivity exceptions due to cross band isolation for CA 1402

7.3A.1 Reference sensitivity power level for 2DL CA without exception 1405

7.3A.1\_1 Reference sensitivity power level for 2DL CA exceptions 1415

7.3A.2 Reference sensitivity power level for 3DL CA without exceptions 1441

7.3A.2\_1 Reference sensitivity power level for 3DL CA exceptions 1449

7.3A.3 Reference sensitivity power level for 4DL CA 1467

7.3A.4 Reference sensitivity power level for 5DL CA 1475

7.3B Reference sensitivity for NR-DC 1475

7.3C Reference sensitivity for SUL 1475

7.3C.0 Minimum conformance requirements 1475

7.3C.0.1 General 1475

7.3C.0.2 Minimum conformance requirements for Reference sensitivity power level 1476

7.3C.0.3 ΔRIB,c for SUL 1477

7.3C.1 General 1478

7.3C.2 Reference sensitivity power level for SUL 1479

7.3C.3 Reference sensitivity power level for SUL (3CC) 1492

7.3D Reference sensitivity for UL MIMO 1492

7.3D.1 General 1492

7.3D.2 Reference sensitivity power level for UL MIMO 1493

7.3D.2\_1 Reference sensitivity power level for SUL with UL MIMO 1494

7.3D.2\_2 Reference sensitivity power level for SUL with UL MIMO (3CC) 1496

7.3E Reference sensitivity for V2X 1497

7.3E.1 General 1497

7.3E.2 Reference sensitivity for V2X / non-concurrent operation 1497

7.3F Reference sensitivity for shared spectrum channel access 1500

7.3F.1 General 1500

7.3F.2 Reference sensitivity power level 1500

7.3F.3 ΔRIB,c 1504

7.3G Reference sensitivity for Tx Diversity 1505

7.3I Reference sensitivity for RedCap 1505

7.3I.1 General 1505

7.3I.2 Reference sensitivity power level for RedCap 1505

7.3J Reference sensitivity for ATG 1527

7.3J.1 General 1527

7.4 Maximum input level 1527

7.4A Maximum input level for CA 1530

7.4A.0 Minimum conformance requirements 1530

7.4A.0.1 Maximum input level for Intra-band contiguous CA 1530

7.4A.0.2 Maximum input level for Intra-band non-contiguous CA 1530

7.4A.0.3 Maximum input level for Inter-band CA 1530

7.4A.1 Maximum input level for CA (2DL CA) 1531

7.4A.2 Maximum input level for CA (3DL CA) 1535

7.4A.3 Maximum input level for CA (4DL CA) 1539

7.4A.4 Maximum input level for CA (5DL CA) 1543

7.4B Maximum input level for NR-DC 1546

7.4D Maximum input level for UL MIMO 1546

7.4D\_1 Maximum input level for SUL with UL MIMO 1548

7.4J Maximum input level for ATG 1550

7.5 Adjacent channel selectivity 1553

7.5A Adjacent channel selectivity for CA 1560

7.5A.0 Minimum conformance requirements 1560

7.5A.0.1 Adjacent channel selectivity for Intra-band contiguous CA 1560

7.5A.0.2 Adjacent channel selectivity Intra-band non-contiguous CA 1562

7.5A.0.3 Adjacent channel selectivity Inter-band CA 1563

7.5A.1 Adjacent channel selectivity for CA (2DL CA) 1563

7.5A.2 Adjacent channel selectivity for CA (3DL CA) 1574

7.5A.3 Adjacent channel selectivity for CA (4DL CA) 1586

7.5A.4 Adjacent channel selectivity for CA (5DL CA) 1596

7.5B Adjacent channel selectivity for NR-DC 1604

7.5D Adjacent channel selectivity for UL MIMO 1604

7.5D\_1 Adjacent channel selectivity for SUL with UL MIMO 1606

7.5F Adjacent channel selectivity 1607

7.5F.1 Adjacent channel selectivity for shared spectrum channel access 1607

7.5J Adjacent channel selectivity for ATG 1610

7.6 Blocking characteristics 1616

7.6.1 General 1616

7.6.2 In-band blocking 1617

7.6.3 Out-of-band blocking 1623

7.6.4 Narrow band blocking 1630

7.6A Blocking characteristics for CA 1633

7.6A.1 General 1633

7.6A.2 Inband blocking for CA 1633

7.6A.2.0 Minimum requirements 1633

7.6A.2.0.1 In-band blocking for Intra-band contiguous CA 1633

7.6A.2.0.2 In-band blocking for Intra-band non-contiguous CA 1635

7.6A.2.0.3 In-band blocking for Inter-band CA 1635

7.6A.2.1 In-band blocking for CA (2DL CA) 1636

7.6A.2.2 In-band Blocking for CA (3DL CA) 1643

7.6A.2.3 In-band Blocking for CA (4DL CA) 1654

7.6A.3 Out-of-band blocking for CA 1662

7.6A.3.0 Minimum conformance requirements 1662

7.6A.3.0.1 Out-of-band blocking for Intra-band contiguous CA 1662

7.6A.3.0.2 Out-of-band blocking for Intra-band non-contiguous CA 1663

7.6A.3.0.3 Out-of-band blocking for Inter-band CA 1663

7.6A.3.1 Out-of-band blocking for CA (2DL CA) 1665

7.6A.3.2 Out-of-band blocking for CA (3DL CA) 1672

7.6A.3.3 Out-of-band blocking for CA (4DL CA) 1680

7.6A.4 Narrow band blocking for CA 1686

7.6A.4.0 Minimum conformance requirements 1686

7.6A.4.0.1 Narrow band blocking for Intra-band contiguous CA 1686

7.6A.4.0.2 Narrow band blocking for Intra-band non-contiguous CA 1686

7.6A.4.0.3 Narrow band blocking for Inter-band CA 1687

7.6A.4.1 Narrow band blocking for CA (2DL CA) 1687

7.6A.4.2 Narrow band blocking for CA (3DL CA) 1691

7.6A.4.3 Narrow band blocking for CA (4DL CA) 1694

7.6B Blocking characteristics for NR-DC 1697

7.6C Blocking characteristics for SUL 1697

7.6C.1 General 1697

7.6C.2 In-band blocking for SUL 1697

7.6C.2\_1 Inband Blocking for SUL with DL CA 1698

7.6C.2\_1.1 Inband Blocking for SUL with 2 DL CA 1698

7.6C.3 Out-of-band blocking for SUL 1701

7.6C.3\_1 Out-of-band blocking for SUL with DL CA 1703

7.6C.3\_1.1 Out-of-band Blocking for SUL with 2 DL CA 1703

7.6D Blocking characteristics for UL MIMO 1707

7.6D.1 General 1707

7.6D.2 In-band blocking for UL MIMO 1707

7.6D.2\_1 In-band blocking for SUL with UL MIMO 1709

7.6D.3 Out-of-band blocking for UL MIMO 1710

7.6D.3\_1 Out-of-band blocking for SUL with UL MIMO 1711

7.6D.4 Narrow band blocking for UL MIMO 1713

7.6D.4\_1 Void 1714

7.6E Blocking characteristics for V2X 1714

7.6E.1 General 1714

7.6E.2 In-band blocking for V2X 1715

7.6E.2.0 Minimum conformance requirements 1715

7.6E.2.1 In-band blocking for V2X / non-concurrent operation 1715

7.6E.2.2 In-band blocking for V2X / con-current operation 1715

7.6E.3 Out-of-band blocking for V2X 1716

7.6E.3.0 Minimum conformance requirements 1716

7.6E.3.1 Out-of-band blocking for V2X / non-concurrent operation 1716

7.6E.3.2 Out-of-band blocking for V2X / con-current operation 1716

7.6F Blocking characteristics for shared spectrum channel access 1716

7.6F.1 General 1716

7.6F.2 In-band blocking 1717

7.6F.2.1 In-band blocking for shared spectrum channel access 1717

7.6F.2.1.1 Test purpose 1717

7.6F.2.1.2 Test applicability 1717

7.6F.2.1.3 Minimum conformance requirements 1717

7.6F.2.1.4 Test description 1718

7.6F.2.1.5 Test requirement 1719

7.6F.2.2 In-band blocking for Intra-band contiguous shared spectrum channel access CA 1720

7.6F.3 Out-of-band blocking 1720

7.6J.2 In-band blocking for ATG 1724

7.6J.3 Out-of-band blocking for ATG 1729

7.7 Spurious response 1735

7.7A Spurious response for CA 1738

7.7A.0 Minimum conformance requirements 1738

7.7A.0.1 Minimum conformance requirements for intra-band contiguous CA 1738

7.7A.0.2 Void 1738

7.7A.0.3 Minimum conformance requirements for inter-band CA 1738

7.7A.0.4 Minimum conformance requirements for intra-band non-contiguous CA 1738

7.7A.1 Spurious response for CA (2DL CA) 1739

7.7A.2 Spurious response for CA (3DL CA) 1740

7.7A.3 Spurious response for CA (4DL CA) 1741

7.7B Spurious response for NR-DC 1742

7.7D Spurious response for UL MIMO 1742

7.7D\_1 Spurious response for SUL with UL MIMO 1743

7.7E Spurious response for V2X 1744

7.7E.0 Minimum conformance requirements 1744

7.7E.1 Spurious response for V2X / non-concurrent operation 1744

7.7E.2 Spurious response for V2X / con-current operation 1744

7.7F Spurious response for shared spectrum channel access 1744

7.7F.1 Spurious response for shared spectrum channel access 1744

7.7F.1.1 Test Purpose 1744

7.7F.1.2 Test Applicability 1745

7.7F.1.3 Minimum Conformance Requirements 1745

7.7F.1.4 Test Description 1745

7.7F.1.5 Test Requirements 1746

7.7F.2 Intra-band contiguous shared spectrum channel access CA 1746

7.7J Spurious response for ATG 1746

7.8 Intermodulation characteristics 1748

7.8.1 General 1748

7.8.2 Wide band Intermodulation 1748

7.8A Intermodulation characteristics for CA 1754

7.8A.1 General 1754

7.8A.2 Wide band Intermodulation for CA 1754

7.8A.2.0 Minimum conformance requirements 1754

7.8A.2.0.1 Wide band Intermodulation for Intra-band contiguous CA 1754

7.8A.2.0.2 Wide band intermodulation for Intra-band non-contiguous CA 1755

7.8A.2.0.3 Wide band Intermodulation for Inter-band CA 1755

7.8A.2.1 Wide band Intermodulation for CA (2DL CA) 1756

7.8A.2.2 Wide band Intermodulation for CA (3DL CA) 1762

7.8A.2.3 Wide band Intermodulation for CA (4DL CA) 1768

7.8B Intermodulation characteristics for NR-DC 1772

7.8D Intermodulation characteristics for UL MIMO 1772

7.8D.1 General 1772

7.8D.2 Wide band Intermodulation for UL MIMO 1772

7.8D.2\_1 Wide band Intermodulation for SUL with UL MIMO 1774

7.8E Intermodulation characteristics for V2X 1775

7.8E.1 General 1775

7.8E.2 Wide band Intermodulation for V2X 1776

7.8E.2.0 Minimum conformance requirements 1776

7.8E.2.1 Wide band Intermodulation for V2X / non-concurrent operation 1776

7.8E.2.2 Wide band Intermodulation for V2X / con-current operation 1776

7.8F Intermodulation characteristics for shared spectrum channel access 1776

7.8F.1 General 1776

7.8F.2 Wide band Intermodulation for shared spectrum channel access 1777

7.8J Intermodulation characteristics for ATG 1780

7.8J.1 General 1780

7.8J.2 Wide band intermodulation for ATG 1780

7.9 Spurious emissions 1783

7.9A Spurious emissions for CA 1785

7.9A.0 Minimum conformance requirements 1785

7.9A.1 Spurious emissions for CA (2DL CA) 1785

7.9B Spurious emissions for NR-DC 1787

7.9J Spurious emissions for ATG 1787

Annex A (normative): Measurement channels 1964

A.1 General 1964

A.2 UL reference measurement channels 1964

A.2.1 General 1964

A.2.2 Reference measurement channels for FDD 1965

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 1965

A.2.2.2 DFT-s-OFDM QPSK 1966

A.2.2.3 DFT-s-OFDM 16QAM 1967

A.2.2.4 DFT-s-OFDM 64QAM 1968

A.2.2.5 DFT-s-OFDM 256QAM 1969

A.2.2.6 CP-OFDM QPSK 1970

A.2.2.7 CP-OFDM 16QAM 1971

A.2.2.8 CP-OFDM 64QAM 1973

A.2.2.9 CP-OFDM 256QAM 1974

A.2.3 Reference measurement channels for TDD 1976

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 1976

A.2.3.2 DFT-s-OFDM QPSK 1976

A.2.3.3 DFT-s-OFDM 16QAM 1976

A.2.3.4 DFT-s-OFDM 64QAM 1976

A.2.3.5 DFT-s-OFDM 256QAM 1976

A.2.3.6 CP-OFDM QPSK 1976

A.2.3.7 CP-OFDM 16QAM 1976

A.2.3.8 CP-OFDM 64QAM 1976

A.2.3.9 CP-OFDM 256QAM 1976

A.3 DL reference measurement channels 1976

A.3.1 General 1976

A.3.2 DL reference measurement channels for FDD 1979

A.3.2.1 General 1979

A.3.2.2 FRC for receiver requirements for QPSK 1980

A.3.2.3 FRC for maximum input level for 64QAM 1983

A.3.2.4 FRC for maximum input level for 256 QAM 1986

A.3.2.5 FRC for maximum input level for 1024 QAM 1989

A.3.3 DL reference measurement channels for TDD 1992

A.3.3.1 General 1992

A.3.3.2 FRC for receiver requirements for QPSK 1994

A.3.3.3 FRC for maximum input level for 64QAM 1997

A.3.3.4 FRC for maximum input level for 256 QAM 2000

A.3.3.5 FRC for maximum input level for 1024 QAM 2003

A.4 CSI reference measurement channels 2006

A.5 OFDMA Channel Noise Generator (OCNG) 2006

A.5.1 OCNG Patterns for FDD 2006

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 2006

A.5.2 OCNG Patterns for TDD 2006

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 2006

A.6 2006

A.7 V2X reference measurement channels 2007

A.7.1 General 2007

A.7.2 FRC for V2X receiver requirements for QPSK 2007

A.7.3 FRC for maximum input level for 64QAM 2009

A.7.4 FRC for maximum input level for 256QAM 2010

A.7.5 FRC for transmitter requirements 2012

Annex B (normative): Propagation Conditions 2016

B.0 No interference 2016

Annex C (normative): Downlink physical channels 2016

C.0 Downlink signal levels 2016

C.1 General 2017

C.2 Setup 2017

C.3 Connection 2018

C.3.0 Measurement of Transmitter Characteristics 2018

C.3.1 Measurement of Receiver Characteristics 2019

Annex D (normative): Characteristics of the Interfering Signal 2019

D.1 General 2019

D.2 Interference signals 2020

Annex E (normative): Global In-Channel TX-Test 2021

E.1 General 2021

E.2 Signals and results 2021

E.2.1 Basic principle 2021

E.2.2 Output signal of the TX under test 2021

E.2.3 Reference signal 2021

E.2.4 Measurement results 2022

E.2.5 Measurement points 2022

E.3 Signal processing 2023

E.3.1 Pre FFT minimization process 2023

E.3.2 Timing of the FFT window 2023

E.3.3 Post FFT equalisation 2024

E.4 Derivation of the results 2025

E.4.1 EVM 2025

E.4.2 Averaged EVM 2025

E.4.3 In-band emissions measurement 2026

E.4.4 EVM equalizer 2028

E.4.4.1 EVM equalizer spectrum flatness 2028

E.4.4.2 EVM equalizer spectral shaping filter 2029

E.4.5 Frequency error and Carrier leakage 2029

E.4.6 EVM of Demodulation reference symbols (EVMDMRS) 2029

E.4.6.1 1st average for EVM DMRS 2030

E.4.6.2 Final average for EVM DMRS 2031

E.4.7 Modified signal under test 2031

E.4.8 EVM measurement for dual Tx 2033

E.4.9 Phase offset measurement for DMRS bundling 2033

E.4.9.1 Measurement point 2033

E.4.9.2 Symbols used 2033

E.4.9.3 Modified test signal 2033

E.4.9.4 Phase offset measurement 2033

E.5 EVM and inband emissions for PUCCH 2034

E.5.1 Basic principle 2034

E.5.2 Output signal of the TX under test 2034

E.5.3 Reference signal 2034

E.5.4 Measurement results 2034

E.5.5 Measurement points 2034

E.5.6 Pre FFT minimization process 2035

E.5.7 Timing of the FFT window 2035

E.5.8 Post FFT equalisation 2035

E.5.9 Derivation of the results 2036

E.5.9.1 EVMPUCCH 2036

E.5.9.2 Averaged EVMPUCCH 2036

E.5.9.3 In-band emissions measurement 2037

E.5.9.4 EVM measurement for dual Tx 2038

E.6 EVM for PRACH 2038

E.6.1 Basic principle 2038

E.6.2 Output signal of the TX under test 2038

E.6.3 Reference signal 2038

E.6.4 Measurement results 2038

E.6.5 Measurement points 2039

E.6.6 Pre FFT minimization process 2039

E.6.7 Timing of the FFT window 2039

E.6.8 Post FFT equalisation 2040

E.6.9 Derivation of the results 2040

E.6.9.1 EVMPRACH 2040

E.6.9.2 Averaged EVMPRACH 2041

E.6.9.3 EVM measurement for dual Tx 2041

E.7 reserved 2041

E.8 EVM for UL MIMO 2041

E.8.1 General 2041

E.8.2 MIMO Equalization 2043

E.8.3 Layer processing 2043

Annex F (normative): Measurement uncertainties and Test Tolerances 2044

F.1 Acceptable uncertainty of Test System (normative) 2044

F.1.0 General 2044

F.1.1 Measurement of test environments 2044

F.1.2 Measurement of transmitter 2044

F.1.3 Measurement of receiver 2061

F.2 Interpretation of measurement results (normative) 2067

F.3 Test Tolerance and Derivation of Test Requirements (informative) 2067

F.3.1 Measurement of test environments 2067

F.3.2 Measurement of transmitter 2067

F.3.3 Measurement of receiver 2082

F.4 Uplink power window 2086

F.4.1 Introduction 2086

F.4.2 Setting the power window above a requirement 2087

F.4.2.1 NR FR1 2087

F.4.3 Setting the power window below a requirement 2087

F.4.3.1 NR FR1 2087

F.4.4 Setting the power window centred on a target value 2087

F.4.4.1 NR FR1 2087

Annex G (normative): Uplink Physical Channels 2087

G.0 Uplink Signal Levels 2087

G.1 General 2087

G.2 Set-up 2089

G.3 Connection 2089

G.3.0 Measurement of Transmitter Characteristics 2089

G.3.1 Measurement of Receiver Characteristics 2089

G.3.2 Measurement of Performance Requirements 2089

Annex H (normative): Statistical Testing 2090

H.1 General 2090

H.2 Statistical testing of receiver characteristics 2090

H.2.1 General 2090

H.2.2 Mapping throughput to error ratio 2090

H.2.3 Design of the test 2091

H.2.4 Numerical definition of the pass fail limits 2092

H.2.5 Pass fail decision rules 2093

H.2.6 Theory to derive the pass fail limits (Informative) 2093

H.2.6.1 Numerical definition of the pass-fail limits 2093

H.2.6.2 Simulation to derive the pass-fail limits for testing 95% throughput 2094

H.2A Statistical testing of receiver characteristics with CA 2095

H.2A.1 General 2095

H.2A.2 Mapping throughput to error ratio 2095

H.2A.3 Design of the test 2095

H.2A.4 Pass fail decision rules 2095

Annex I (normative): ModifiedMPR-Behaviour 2096

I.1 Indication of modified MPR behaviour 2096

Annex J (normative): 2099

J.0 General 2100

J.1 Measurement Point 2100

J.2 Relative Phase Error Measurement 2101

J.2.1 Symbols and subcarriers used 2101

J.2.2 CFO (carrier frequency offset) correction 2101

J.2.3 Steps of the measurement method 2101

Annex K (informative): Change history 2103