|  |  |
| --- | --- |
| 3GPP TS 38.521-2 V18.2.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) conformance specification;  Radio transmission and reception;  Part 2: Range 2 Standalone  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 17

1 Scope 18

2 References 18

3 Definitions, symbols and abbreviations 19

3.1 Definitions 19

3.2 Symbols 21

3.3 Abbreviations 23

4 General 24

4.1 Relationship between minimum requirements and test requirements 24

4.2 Applicability of minimum requirements 24

4.3 Specification suffix information 25

4.4 Test point analysis 25

4.5 Applicability and test coverage rules 25

5 Operating bands and channel arrangement 26

5.1 General 26

5.2 Operating bands 26

5.2A Operating bands for CA 27

5.2A.1 Intra-band CA 27

5.2A.2 Void 27

5.2A.3 Inter-band CA 27

5.2D Operating bands for UL MIMO 27

5.3 UE Channel bandwidth 27

5.3.1 General 27

5.3.2 Maximum transmission bandwidth configuration 28

5.3.3 Minimum guardband and transmission bandwidth configuration 28

5.3.4 RB alignment 30

5.3.5 Channel bandwidth per operating band 30

5.3A UE Channel bandwidth for CA 31

5.3A.1 General 31

5.3A.2 Minimum guardband and transmission bandwidth configuration for CA 31

5.3A.3 RB alignment with different numerologies for CA 32

5.3A.4 UE channel bandwidth per operating band for CA 33

5.3D Channel bandwidth for UL MIMO 34

5.4 Channel arrangement 34

5.4.1 Channel spacing 34

5.4.1.1 Channel spacing for adjacent NR carriers 34

5.4.2 Channel raster 35

5.4.2.1 NR-ARFCN and channel raster 35

5.4.2.2 Channel raster to resource element mapping 35

5.4.2.3 Channel raster entries for each operating band 35

5.4.3 Synchronization raster 36

5.4.3.1 Synchronization raster and numbering 36

5.4.3.2 Synchronization raster to synchronization block resource element mapping 36

5.4.3.3 Synchronization raster entries for each operating band 36

5.4A Channel arrangement for CA 37

5.4A.1 Channel spacing for CA 37

5.5 Configurations 38

5.5A Configurations for CA 38

5.5A.1 Configurations for intra-band contiguous CA 38

5.5A.2 Configurations for intra-band non-contiguous CA 39

5.5A.3 Configurations for inter-band CA 43

5.5D Configurations for UL MIMO 43

6 Transmitter characteristics 44

6.1 General 44

6.2 Transmit power 47

6.2.1 UE maximum output power 47

6.2.1.0 General 47

6.2.1.1 UE maximum output power - EIRP and TRP 47

6.2.1.1.3.1 UE maximum output power for power class 1 47

6.2.1.1.3.2 UE maximum output power for power class 2 48

6.2.1.1.3.3 UE maximum output power for power class 3 49

6.2.1.1.3.4 UE maximum output power for power class 4 51

6.2.1.1.3.5 UE maximum output power for power class 5 52

6.2.1.1.3.6 53

6.2.1.1.3.7 UE maximum output power for power class 7 53

6.2.1.1\_1 UE maximum output power - EIRP and TRP (Rel16 and forward) 59

6.2.1.2 UE maximum output power - Spherical coverage 61

6.2.1.2\_1 UE maximum output power - Spherical coverage (Rel16 and forward) 67

6.2.2 UE maximum output power reduction 68

6.2.2.0 General 68

6.2.2.3.1 UE maximum output power reduction for power class 1 69

6.2.2.3.2 UE maximum output power reduction for power class 2 70

6.2.2.3.3 UE maximum output power reduction for power class 3 70

6.2.2.3.4 UE maximum output power reduction for power class 4 71

6.2.2.3.5 UE maximum output power reduction for power class 5 71

6.2.2.3.6 UE maximum output power reduction for power class 6 71

6.2.2.3.7 UE maximum output power reduction for power class 7 71

6.2.2\_1 UE maximum output power reduction enhancements 96

6.2.2\_1.0 General 96

6.2.3 UE maximum output power with additional requirements 107

6.2.3.3.1 General 107

6.2.3.3.2 Void 108

6.2.3.3.3 A-MPR for NS\_202 108

6.2.3.3.4 A-MPR for NS\_203 109

6.2.4 Configured transmitted power 116

6.2.4\_1 Configured transmitted power with Power Boost 117

6.2.5 UE Maximum Output Power – EIRP with UL Gaps 119

6.2A Transmit power for CA 123

6.2A.1 UE maximum output power for CA 123

6.2A.1.0 Minimum conformance requirements 123

6.2A.1.1 UE maximum output power - EIRP and TRP for CA 124

6.2A.1.1.1 UE maximum output power - EIRP and TRP for CA (2UL CA) 124

6.2A.1.1.2 UE maximum output power - EIRP and TRP for CA (3UL CA) 128

6.2A.1.1.3 UE maximum output power - EIRP and TRP for CA (4UL CA) 129

6.2A.1.1.4 UE maximum output power - EIRP and TRP for CA (5UL CA) 131

6.2A.1.1.5 UE maximum output power - EIRP and TRP for CA (6UL CA) 131

6.2A.1.1.6 UE maximum output power - EIRP and TRP for CA (7UL CA) 132

6.2A.1.1.7 UE maximum output power - EIRP and TRP for CA (8UL CA) 132

6.2A.1.2 UE maximum output power - Spherical coverage 132

6.2A.1.2.1 UE maximum output power - Spherical coverage for CA (2UL CA) 132

6.2A.1.2.2 UE maximum output power - Spherical coverage for CA (3UL CA) 136

6.2A.1.2.3 UE maximum output power - Spherical coverage for CA (4UL CA) 139

6.2A.1.2.4 UE maximum output power - Spherical coverage for CA (5UL CA) 142

6.2A.1.2.5 UE maximum output power - Spherical coverage for CA (6UL CA) 142

6.2A.1.2.6 UE maximum output power - Spherical coverage for CA (7UL CA) 142

6.2A.1.2.7 UE maximum output power - Spherical coverage for CA (8UL CA) 142

6.2A.2 UE maximum output power reduction for CA 143

6.2A.2.0 Minimum conformance requirements 143

6.2A.2.0.1 General 143

6.2A.2.0.2 Maximum output power reduction for power class 1 143

6.2A.2.0.3 Maximum output power reduction for power class 2 144

6.2A.2.0.4 Maximum output power reduction for power class 3 145

6.2A.2.0.5 Maximum output power reduction for power class 4 146

6.2A.2.1 UE maximum output power reduction for CA (2UL CA) 146

6.2A.2.2 UE maximum output power reduction for CA (3UL CA) 178

6.2A.2.3 UE maximum output power reduction for CA (4UL CA) 184

6.2A.2.4 UE maximum output power reduction for CA (5UL CA) 191

6.2A.2.5 UE maximum output power reduction for CA (6UL CA) 191

6.2A.2.6 UE maximum output power reduction for CA (7UL CA) 192

6.2A.2.7 UE maximum output power reduction for CA (8UL CA) 192

6.2A.3 UE maximum output power with additional requirements for CA 192

6.2A.3.0 Minimum conformance requirements 192

6.2A.3.0.1 General 192

6.2A.3.0.2 Void 193

6.2A.3.0.3 A-MPR for CA\_NS\_202 193

6.2A.3.0.4 A-MPR for CA\_NS\_203 193

6.2A.3.1 UE maximum output power with additional requirements for CA (2UL CA) 194

6.2A.3.2 UE maximum output power with additional requirements for CA (3UL CA) 199

6.2A.3.3 UE maximum output power with additional requirements for CA (4UL CA) 204

6.2A.3.4 UE maximum output power with additional requirements for CA (5UL CA) 210

6.2A.3.5 UE maximum output power with additional requirements for CA (6UL CA) 210

6.2A.3.6 UE maximum output power with additional requirements for CA (7UL CA) 210

6.2A.3.7 UE maximum output power with additional requirements for CA (8UL CA) 210

6.2A.4 Configured transmitted power for CA 210

6.2A.4.0 Minimum conformance requirements 210

6.2A.4.1 Configured transmitted power for CA (2UL CA) 211

6.2A.4.2 Configured transmitted power for CA (3UL CA) 212

6.2A.4.3 Configured transmitted power for CA (4UL CA) 212

6.2A.4.4 Configured transmitted power for CA (5UL CA) 212

6.2A.4.5 Configured transmitted power for CA (6UL CA) 212

6.2A.4.6 Configured transmitted power for CA (7UL CA) 212

6.2A.4.7 Configured transmitted power for CA (8UL CA) 212

6.2A.5 UE maximum output power - EIRP and TRP for CA (2UL CA) with UL Gaps 212

6.2D Transmit power for UL MIMO 215

6.2D.1 UE maximum output power for UL MIMO 215

6.2D.1.0 General 215

6.2D.1.1 UE maximum output power - EIRP and TRP for UL MIMO 215

6.2D.1.2 UE maximum output power - Spherical coverage for UL MIMO 224

6.2D.2 UE maximum output power reduction for UL MIMO 228

6.2D.2.3.1 UE maximum output power reduction for modulation / channel bandwidth for UL MIMO for power class 1 228

6.2D.2.3.2 UE maximum output power reduction for modulation / channel bandwidth for UL MIMO for power class 2 229

6.2D.2.3.3 UE maximum output power reduction for modulation / channel bandwidth for UL MIMO for power class 3 229

6.2D.2.3.4 UE maximum output power reduction for modulation / channel bandwidth for UL MIMO for power class 4 229

6.2D.2.3.5 UE maximum output power reduction for modulation / channel bandwidth for UL MIMO for power class 5 229

6.2D.3 UE maximum output power with additional requirements for UL MIMO 241

6.2D.4 Configured transmitted power for UL MIMO 250

6.3 Output power dynamics 250

6.3.1 Minimum output power 250

6.3.2 Transmit OFF power 255

6.3.3 Transmit ON/OFF time mask 257

6.3.3.1 General 257

6.3.3.2 General ON/OFF time mask 257

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 261

6.3.3.4 PRACH time mask 261

6.3.3.5 Void 265

6.3.3.6 SRS time mask 265

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 271

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 271

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 271

6.3.4 Power control 271

6.3.4.1 General 271

6.3.4.2 Absolute power tolerance 271

6.3.4.3 Relative power tolerance 276

6.3.4.4 Aggregate power tolerance 287

6.3A Output power dynamics for CA 292

6.3A.1 Minimum output power for CA 292

6.3A.1.0 Minimum conformance requirements 292

6.3A.1.1 Minimum output power for CA (2UL CA) 292

6.3A.1.2 Minimum output power for CA (3UL CA) 295

6.3A.1.3 Minimum output power for CA (4UL CA) 297

6.3A.1.4 Minimum output power for CA (5UL CA) 299

6.3A.1.5 Minimum output power for CA (6UL CA) 301

6.3A.1.6 Minimum output power for CA (7UL CA) 303

6.3A.1.7 Minimum output power for CA (8UL CA) 305

6.3A.2 Transmit OFF power for CA 307

6.3A.2.0 Minimum conformance requirements 307

6.3A.2.1 Void 308

6.3A.2.2 Void 308

6.3A.2.3 Void 308

6.3A.3 Transmit ON/OFF time mask for CA 308

6.3A.3.0 Minimum conformance requirements 308

6.3A.3.1 General ON/OFF time mask for CA 308

6.3A.3.1.1 General ON/OFF time mask for CA (2UL CA) 308

6.3A.3.1.2 General ON/OFF time mask for CA (3UL CA) 311

6.3A.3.1.3 General ON/OFF time mask for CA (4UL CA) 311

6.3A.3.1.4 General ON/OFF time mask for CA (5UL CA) 311

6.3A.3.1.5 General ON/OFF time mask for CA (6UL CA) 311

6.3A.3.1.6 General ON/OFF time mask for CA (7UL CA) 311

6.3A.3.1.7 General ON/OFF time mask for CA (8UL CA) 311

6.3A.4 Power control for CA 311

6.3A.4.1 General 311

6.3A.4.2 Absolute power tolerance for CA 312

6.3A.4.2.0 Minimum conformance requirements 312

6.3A.4.2.1 Absolute power tolerance for CA (2UL CA) 312

6.3A.4.2.2 Absolute power tolerance for CA (3UL CA) 316

6.3A.4.2.3 Absolute power tolerance for CA (4UL CA) 318

6.3A.4.2.4 Absolute power tolerance for CA (5UL CA) 320

6.3A.4.2.5 Absolute power tolerance for CA (6UL CA) 323

6.3A.4.2.6 Absolute power tolerance for CA (7UL CA) 325

6.3A.4.2.7 Absolute power tolerance for CA (8UL CA) 327

6.3A.4.3 Relative power tolerance for CA 330

6.3A.4.3.0 Minimum conformance requirements 330

6.3A.4.3.1 Relative power tolerance for CA (2UL CA) 330

6.3A.4.3.2 Relative power tolerance for CA (3UL CA) 330

6.3A.4.3.3 Relative power tolerance for CA (4UL CA) 330

6.3A.4.3.4 Relative power tolerance for CA (5UL CA) 330

6.3A.4.3.5 Relative power tolerance for CA (6UL CA) 330

6.3A.4.3.6 Relative power tolerance for CA (7UL CA) 330

6.3A.4.3.7 Relative power tolerance for CA (8UL CA) 330

6.3A.4.4 Aggregate power tolerance for CA 330

6.3A.4.4.0 Minimum conformance requirements 330

6.3A.4.4.1 Aggregate power tolerance for CA (2UL CA) 330

6.3A.4.4.2 Aggregate power tolerance for CA (3UL CA) 333

6.3A.4.4.3 Aggregate power tolerance for CA (4UL CA) 335

6.3A.4.4.4 Aggregate power tolerance for CA (5UL CA) 337

6.3A.4.4.5 Aggregate power tolerance for CA (6UL CA) 339

6.3A.4.4.6 Aggregate power tolerance for CA (7UL CA) 341

6.3A.4.4.7 Aggregate power tolerance for CA (8UL CA) 343

6.3D Output power dynamics for UL MIMO 345

6.3D.0 General 345

6.3D.1 Minimum output power for UL MIMO 345

6.3D.2 Transmit OFF power for UL MIMO 348

6.3D.3 Transmit ON/OFF time mask for UL MIMO 350

6.3D.3.1 General ON/OFF time mask for UL MIMO 350

6.3D.3.2 Void 353

6.3D.3.3 Void 353

6.3D.3.4 Void 353

6.4 Transmit signal quality 353

6.4.1 Frequency error 353

6.4.2 Transmit modulation quality 355

6.4.2.1 Error vector magnitude 356

6.4.2.1\_1 Error vector magnitude with Power Boost 363

6.4.2.2 Carrier leakage 365

6.4.2.3 In-band emissions 371

6.4.2.4 EVM equalizer spectrum flatness 383

6.4.2.5 EVM spectral flatness for pi/2 BPSK modulation 386

6.4.2.6 Phase continuity requirements for DMRS bundling 389

6.4A Transmit signal quality for CA 394

6.4A.1 Frequency error for CA 394

6.4A.1.0 Minimum conformance requirements 394

6.4A.1.1 Frequency error for CA (2UL CA) 394

6.4A.1.2 Frequency error for CA (3UL CA) 396

6.4A.1.3 Frequency error for CA (4UL CA) 397

6.4A.1.4 Frequency error for CA (5UL CA) 399

6.4A.1.5 Frequency error for CA (6UL CA) 399

6.4A.1.6 Frequency error for CA (7UL CA) 399

6.4A.1.7 Frequency error for CA (8UL CA) 399

6.4A.2 Transmit modulation quality for CA 399

6.4A.2.0 General 399

6.4A.2.1 Error vector magnitude for CA 400

6.4A.2.1.0 Minimum conformance requirements 400

6.4A.2.1.1 Error vector magnitude for CA (2UL CA) 400

6.4A.2.1.2 Error vector magnitude for CA (3UL CA) 403

6.4A.2.1.3 Error vector magnitude for CA (4UL CA) 405

6.4A.2.1.4 Error Vector magnitude for CA (5UL CA) 408

6.4A.2.1.5 Error Vector magnitude for CA (6UL CA) 411

6.4A.2.1.6 Error vector magnitude for CA (7UL CA) 414

6.4A.2.1.7 Error vector magnitude for CA (8UL CA) 417

6.4A.2.2 Carrier leakage for CA 421

6.4A.2.2.0 Minimum conformance requirements 421

6.4A.2.2.1 Carrier leakage for CA (2UL CA) 422

6.4A.2.2.2 Carrier leakage for CA (3UL CA) 425

6.4A.2.2.3 Carrier leakage for CA (4UL CA) 427

6.4A.2.2.4 Carrier leakage for CA (5UL CA) 428

6.4A.2.2.5 Carrier leakage for CA (6UL CA) 430

6.4A.2.2.6 Carrier leakage for CA (7UL CA) 431

6.4A.2.2.7 Carrier leakage for CA (8UL CA) 433

6.4A.2.3 In-band emissions for CA 434

6.4A.2.3.0 Minimum conformance requirements 434

6.4A.2.3.1 In-band emissions for CA (2UL CA) 437

6.4A.2.3.2 In-band emissions for CA (3UL CA) 442

6.4A.2.3.3 In-band emissions for CA (4UL CA) 447

6.4A.2.3.4 In-band emissions for CA (5UL CA) 451

6.4A.2.3.5 In-band emissions for CA (6UL CA) 455

6.4A.2.3.6 In-band emissions for CA (7UL CA) 460

6.4A.2.3.7 In-band emissions for CA (8UL CA) 465

6.4A.2.4 Void 471

6.4A.2.5 Void 471

6.4D Transmit signal quality for UL MIMO 471

6.4D.0 General 471

6.4D.1 Frequency error for UL MIMO 471

6.4D.2 Transmit signal quality for UL MIMO 473

6.4D.2.1 Error vector magnitude for UL MIMO 473

6.4D.2.2 Carrier leakage for UL MIMO 478

6.4D.2.3 In-band emissions for UL MIMO 483

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 493

6.4D.3 Time alignment error for UL MIMO 499

6.5 Output RF spectrum emissions 502

6.5.1 Occupied bandwidth 502

6.5.2 Out of band emission 504

6.5.2.1 Spectrum Emission Mask 505

6.5.2.1\_1 Spectrum Emission Mask with Power Boost 508

6.5.2.2 Void 509

6.5.2.3 Adjacent channel leakage ratio 509

6.5.3 Spurious emissions 515

6.5.3.1 Transmitter Spurious emissions 516

6.5.3.1\_1 Transmitter Spurious emissions with Power Boost 521

6.5.3.2 Spurious emission band UE co-existence 522

6.5.3.2\_1 Spurious emission band UE co-existence with Power Boost 526

6.5.3.3 Additional spurious emissions 528

6.5.3.3\_1 Additional spurious emissions with Power Boost 533

6.5A Output RF spectrum emissions for CA 534

6.5A.1 Occupied bandwidth for CA 534

6.5A.1.0 Minimum conformance requirements 534

6.5A.1.1 Occupied bandwidth for CA (2UL CA) 535

6.5A.1.2 Occupied bandwidth for CA (3UL CA) 538

6.5A.1.3 Occupied bandwidth for CA (4UL CA) 539

6.5A.1.4 Occupied bandwidth for CA (5UL CA) 540

6.5A.1.5 Occupied bandwidth for CA (6UL CA) 541

6.5A.1.6 Occupied bandwidth for CA (7UL CA) 542

6.5A.1.7 Occupied bandwidth for CA (8UL CA) 543

6.5A.2 Out of band emission for CA 544

6.5A.2.1 Spectrum Emission Mask for CA 544

6.5A.2.1.0 Minimum conformance requirements 544

6.5A.2.1.1 Spectrum Emission Mask for CA (2UL CA) 545

6.5A.2.1.2 Spectrum Emission Mask for CA (3UL CA) 550

6.5A.2.1.3 Spectrum Emission Mask for CA (4UL CA) 551

6.5A.2.1.4 Spectrum Emission Mask for CA (5UL CA) 552

6.5A.2.1.5 Spectrum Emission Mask for CA (6UL CA) 553

6.5A.2.1.6 Spectrum Emission Mask for CA (7UL CA) 554

6.5A.2.1.7 Spectrum Emission Mask for CA (8UL CA) 555

6.5A.2.2 Adjacent channel leakage ratio for CA 556

6.5A.2.2.0 Minimum conformance requirements 556

6.5A.2.2.1 Adjacent channel leakage ratio for CA (2UL CA) 557

6.5A.2.2.2 Adjacent channel leakage ratio for CA (3UL CA) 563

6.5A.2.2.3 Adjacent channel leakage ratio for CA (4UL CA) 564

6.5A.2.2.4 Adjacent channel leakage ratio for CA (5UL CA) 565

6.5A.2.2.5 Adjacent channel leakage ratio for CA (6UL CA) 566

6.5A.2.2.6 Adjacent channel leakage ratio for CA (7UL CA) 567

6.5A.2.2.7 Adjacent channel leakage ratio for CA (8UL CA) 568

6.5A.3 Spurious emissions for CA 569

6.5A.3.1 General spurious emissions for CA 569

6.5A.3.1.0 Minimum conformance requirements 569

6.5A.3.1.1 General spurious emissions for CA (2UL CA) 569

6.5A.3.1.2 General spurious emissions for CA (3UL CA) 574

6.5A.3.1.3 General spurious emissions for CA (4UL CA) 575

6.5A.3.1.4 General spurious emissions for CA (5UL CA) 575

6.5A.3.1.5 General spurious emissions for CA (6UL CA) 576

6.5A.3.1.6 General spurious emissions for CA (7UL CA) 577

6.5A.3.1.7 General spurious emissions for CA (8UL CA) 577

6.5A.3.2 Spurious emission band UE co-existence for UL CA 578

6.5A.3.2.0 Minimum conformance requirements 578

6.5A.3.2.1 Spurious emission band UE co-existence for CA (2UL CA) 578

6.5A.3.2.2 Spurious emission band UE co-existence for CA (3UL CA) 583

6.5A.3.2.3 Spurious emission band UE co-existence for CA (4UL CA) 584

6.5A.3.2.4 Spurious emission band UE co-existence for CA (5UL CA) 585

6.5A.3.2.5 Spurious emission band UE co-existence for CA (6UL CA) 585

6.5A.3.2.6 Spurious emission band UE co-existence for CA (7UL CA) 586

6.5A.3.2.7 Spurious emission band UE co-existence for CA (8UL CA) 586

6.5A.3.3 Additional spurious emissions for CA 587

6.5A.3.3.0 Minimum conformance requirements 587

6.5A.3.3.1 Additional spurious emissions for CA (2UL CA) 588

6.5A.3.3.2 Additional spurious emissions for CA (3UL CA) 593

6.5A.3.3.3 Additional spurious emissions for CA (4UL CA) 594

6.5A.3.3.4 Additional spurious emissions for CA (5UL CA) 594

6.5A.3.3.5 Additional spurious emissions for CA (6UL CA) 595

6.5A.3.3.6 Additional spurious emissions for CA (7UL CA) 595

6.5A.3.3.7 Additional spurious emissions for CA (8UL CA) 596

6.5D Output RF spectrum emissions for UL MIMO 597

6.5D.1 Occupied bandwidth for UL MIMO 597

6.5D.2 Out of band emission for UL MIMO 599

6.5D.2.1 Spectrum Emission Mask for UL MIMO 599

6.5D.2.2 Adjacent channel leakage ratio for UL MIMO 600

6.5D.3 Spurious emissions for UL MIMO 603

6.5D.3.1 Transmitter Spurious emissions for UL MIMO 603

6.5D.3.2 Spurious emission band UE co-existence for UL MIMO 604

6.5D.3.3 Additional spurious emissions for UL MIMO 605

6.6 Beam correspondence 606

6.6.0 General 606

6.6.1 Beam correspondence - EIRP 606

6.6.2 Enhanced Beam correspondence – EIRP 617

6.6A Beam correspondence for CA 622

7 Receiver characteristics 622

7.1 General 622

7.2 Diversity characteristics 622

7.3 Reference sensitivity 622

7.3.1 General 622

7.3.2 Reference sensitivity power level 622

7.3.2.3.1 Reference sensitivity power level for power class 1 623

7.3.2.3.2 Reference sensitivity power level for power class 2 624

7.3.2.3.3 Reference sensitivity power level for power class 3 624

7.3.2.3.4 Reference sensitivity power level for power class 4 625

7.3.2.3.5 Reference sensitivity power level for power class 5 626

7.3.2.3.7 Reference sensitivity power level for power class 7 626

7.3.4 EIS spherical coverage 632

7.3A Reference sensitivity for CA 639

7.3A.1 General 639

7.3A.2 Reference sensitivity power level for CA 639

7.3A.2.0 Minimum Conformance Requirements 639

7.3A.2.0.1 Intra-band contiguous CA 639

7.3A.2.0.2 Intra-band non-contiguous CA 640

7.3A.2.0.3 Inter-band CA 640

7.3A.2.1 Reference sensitivity power level for CA (2DL CA) 640

7.3A.2.2 Reference sensitivity power level for CA (3DL CA) 645

7.3A.2.3 Reference sensitivity power level for CA (4DL CA) 646

7.3A.2.4 Reference sensitivity power level for CA (5DL CA) 646

7.3A.2.5 Reference sensitivity power level for CA (6DL CA) 647

7.3A.2.6 Reference sensitivity power level for CA (7DL CA) 647

7.3A.2.7 Reference sensitivity power level for CA (8DL CA) 648

7.3A.3 EIS spherical coverage for DL CA 649

7.3A.3.0 Minimum Conformance Requirements 649

7.3A.3.0.1 Void 649

7.3A.3.0.2 Void 649

7.3A.3.0.3 EIS spherical coverage for inter-band CA 649

7.3A.3.1 EIS Spherical Coverage for Inter-band CA (2DL CA) 649

7.3A.3.2 EIS Spherical Coverage for Inter-band CA (3DL CA) 653

7.3A.3.3 EIS Spherical Coverage for Inter-band CA (4DL CA) 654

7.3D Reference sensitivity for UL MIMO 654

7.4 Maximum input level 654

7.4A Maximum input level for CA 657

7.4A.0 Minimum Conformance Requirements 657

7.4A.0.1 Maximum input level for Intra-band contiguous CA 657

7.4A.0.2 Maximum input level for Intra-band non-contiguous CA 658

7.4A.0.3 Maximum input level for inter-band CA 658

7.4A.1 Maximum input level for CA (2DL CA) 658

7.4A.2 Maximum input level for CA (3DL CA) 661

7.4A.3 Maximum input level for CA (4DL CA) 662

7.4A.4 Maximum input level for CA (5DL CA) 662

7.4A.5 Maximum input level for CA (6DL CA) 663

7.4A.6 Maximum input level for CA (7DL CA) 663

7.4A.7 Maximum input level for CA (8DL CA) 664

7.4D Maximum input level for UL MIMO 664

7.5 Adjacent channel selectivity 665

7.5A Adjacent channel selectivity for CA 671

7.5A.0 Minimum Conformance Requirements 671

7.5A.0.1 Adjacent channel selectivity for Intra-band contiguous CA 671

7.5A.0.2 Adjacent channel selectivity for Intra-band non-contiguous CA 672

7.5A.0.3 Adjacent channel selectivity for Inter-band CA 673

7.5A.1 Adjacent channel selectivity for CA (2DL CA) 673

7.5A.2 Adjacent channel selectivity for CA (3DL CA) 673

7.5A.3 Adjacent channel selectivity for CA (4DL CA) 673

7.5A.4 Adjacent channel selectivity for CA (5DL CA) 673

7.5A.5 Adjacent channel selectivity for CA (6DL CA) 673

7.5A.6 Adjacent channel selectivity for CA (7DL CA) 673

7.5A.7 Adjacent channel selectivity for CA (8DL CA) 673

7.5D Adjacent channel selectivity for UL MIMO 673

7.6 Blocking characteristics 674

7.6.1 General 674

7.6.2 In-band blocking 674

7.6.3 Void 680

7.6A Blocking characteristics for CA 680

7.6A.1 General 680

7.6A.2 In-band blocking for CA 680

7.6A.2.0 Minimum Conformance Requirements 680

7.6A.2.0.1 In-band blocking for Intra-band contiguous CA 680

7.6A.2.0.2 In-band blocking for Intra-band non-contiguous CA 681

7.6A.2.0.3 In-band blocking for Inter-band CA 682

7.6A.2.1 In-band blocking for CA (2DL CA) 682

7.6A.2.2 Void 685

7.6A.2.3 Void 685

7.6A.2.4 Void 685

7.6A.2.5 Void 685

7.6A.2.6 Void 685

7.6A.2.7 Void 685

7.6D Blocking characteristics for UL MIMO 685

7.7 Void 685

7.8 Void 685

7.9 Spurious emissions 685

7.10 Void 688

Annex A (normative): Measurement channels 689

A.1 General 689

A.2 UL reference measurement channels 689

A.2.1 General 689

A.2.2 Void 689

A.2.3 Reference measurement channels for TDD 690

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 691

A.2.3.2 DFT-s-OFDM QPSK 692

A.2.3.3 DFT-s-OFDM 16QAM 693

A.2.3.4 DFT-s-OFDM 64QAM 694

A.2.3.5 CP-OFDM QPSK 695

A.2.3.6 CP-OFDM 16QAM 696

A.2.3.7 CP-OFDM 64QAM 697

A.3 DL reference measurement channels 698

A.3.1 General 698

A.3.2 Void 700

A.3.3 DL reference measurement channels for TDD 700

A.3.3.1 General 700

A.3.3.2 FRC for receiver requirements for QPSK 701

A.3.3.3 FRC for receiver requirements for 16QAM 702

A.3.3.4 FRC for receiver requirements for 64QAM 703

A.3.3.5 FRC for receiver requirements for 256QAM 705

A.4 Void 706

A.5 OFDMA Channel Noise Generator (OCNG) 706

A.5.1 OCNG Patterns for FDD 706

A.5.2 OCNG Patterns for TDD 707

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 707

Annex B (normative): Propagation conditions 708

B.0 No interference 708

Annex C (normative): Downlink Physical Channels 709

C.0 Downlink signal levels 709

C.1 General 710

C.2 Setup 710

C.3 Connection 711

C.3.0 Measurement of Transmitter Characteristics 711

C.3.1 Measurement of Receiver Characteristics 712

Annex D (normative): Characteristics of the interfering signal 713

D.1 General 713

D.2 Interference signals 713

Annex E (normative): Global In-Channel TX-Test 714

E.1 General 714

E.2 Signals and results 714

E.2.1 Basic principle 714

E.2.2 Output signal of the TX under test 714

E.2.3 Reference signal 714

E.2.4 Measurement results 715

E.2.5 Measurement points 715

E.3 Signal processing 715

E.3.1 Pre FFT minimization process 715

E.3.2 Timing of the FFT window 716

E.3.3 Post FFT equalisation 717

E.4 Derivation of the results 718

E.4.1 EVM 718

E.4.2 Averaged EVM 718

E.4.3 In-band emissions measurement 719

E.4.4 EVM equalizer spectrum flatness 721

E.4.5 Frequency error and Carrier leakage 721

E.4.6 EVM of Demodulation reference symbols (EVMDMRS) 722

E.4.6.1 1st average for EVM DMRS 722

E.4.6.2 Final average for EVM DMRS 723

E.5 EVM and inband emissions for PUCCH 723

E.5.1 Basic principle 723

E.5.2 Output signal of the TX under test 723

E.5.3 Reference signal 723

E.5.4 Measurement results 723

E.5.5 Measurement points 724

E.5.6 Pre FFT minimization process 724

E.5.7 Timing of the FFT window 724

E.5.8 Post FFT equalisation 724

E.5.9 Derivation of the results 725

E.5.9.1 EVMPUCCH 725

E.5.9.2 Averaged EVMPUCCH 725

E.5.9.3 In-band emissions measurement 726

E.5.10 Modified signal under test 727

E.6 EVM for PRACH 729

E.6.1 Basic principle 729

E.6.2 Output signal of the TX under test 729

E.6.3 Reference signal 729

E.6.4 Measurement results 729

E.6.5 Measurement points 730

E.6.6 Pre FFT minimization process 730

E.6.7 Timing of the FFT window 730

E.6.8 Post FFT equalisation 731

E.6.9 Derivation of the results 731

E.6.9.1 EVMPRACH 731

E.6.9.2 Averaged EVMPRACH 732

E.6.10 Modified signal under test 732

E.6.11 Phase offset measurement for DMRS bundling 732

E.6.11.1 Measurement point 732

E.6.11.2 Symbols used 732

E.6.11.3 Modified test signal 732

E.6.11.4 Phase offset measurement 732

E.6.12 EVM for dual transmit polarizations 733

E.6.12.1 General 733

E.6.12.2 MIMO Equalization (UL MIMO transmission) 733

E.6.12.3 Maximum Ratio combining (Tx diversity transmission) 734

E.6.12.4 Layer processing 735

Annex F (normative): Measurement uncertainties and Test Tolerances 736

F.1 Acceptable uncertainty of Test System (normative) 736

F.1.0 General 736

F.1.1 Measurement of test environments 736

F.1.2 Measurement of transmitter 737

F.1.3 Measurement of receiver 757

F.2 Interpretation of measurement results (normative) 760

F.3 Test Tolerance and Derivation of Test Requirements (informative) 761

F.3.1 Measurement of test environments 761

F.3.2 Measurement of transmitter 761

F.3.3 Measurement of receiver 782

F.4 Uplink power window 785

F.4.1 Introduction 785

F.4.2 Setting the power window above a requirement 785

F.4.3 Setting the power window below a requirement 785

F.4.4 Setting the power window centred on a target value 785

F.8 FFS 786

F.9 FFS 786

F.10 FFS 786

Annex G (normative): Uplink Physical Channels 786

G.0 Uplink Signal Levels 786

G.1 General 786

G.2 Set-up 786

G.3 Connection 786

G.3.0 Measurement of Transmitter Characteristics 786

G.3.1 Measurement of Receiver Characteristics 786

Annex H (normative): Statistical Testing 787

H.1 General 787

H.2 Statistical testing of receiver characteristics 787

H.2.1 General 787

H.2.2 Mapping throughput to error ratio 787

H.2.3 Design of the test 788

H.2.4 Numerical definition of the pass fail limits 789

H.2.5 Pass fail decision rules 790

Annex I:Void 791

Annex J (normative): Test applicability per permitted test method 792

Annex K (normative): EIRP, TRP, and EIS measurement procedures 793

K.1 Direct far field (DFF) 793

K.1.1 TX beam peak direction search 793

K.1.2 RX beam peak direction search 795

K.1.3 Peak EIRP measurement procedure 797

K.1.4 Peak EIS measurement procedure 798

K.1.5 EIRP spherical coverage 798

K.1.5.0 Tx Spherical Coverage Method 798

K.1.5.1 Tx Fast Spherical Coverage Method 799

K.1.5.1.1 Introduction 799

K.1.5.1.2 Description 799

K.1.6 EIS spherical coverage 799

K.1.6.0 Rx Spherical Coverage Method 799

K.1.6.1 Rx Fast Spherical Coverage Method 800

K.1.6.1.1 Introduction 800

K.1.6.1.2 Description 800

K.1.7 TRP measurement procedure 800

K.1.8 Blocking measurement procedure 801

K.1.9 Beam Correspondence tolerance procedure 801

K.1.11 RSRP(B) based RX beam peak search 802

K.1.11.1 Test procedure 802

K.1.12 Enhanced test method for EIRP measurements 803

K.1.12.1 Applicability of TPMI side condition method 804

K.1.12.2 TPMI side condition method Measurement uncertainties impact 804

K.2 Direct far field (DFF) simplification 804

K.2.1 TX beam peak direction search 804

K.2.2 RX beam peak direction search 804

K.2.3 Peak EIRP measurement procedure 804

K.2.4 Peak EIS measurement procedure 804

K.2.5 EIRP spherical coverage 804

K.2.6 EIS spherical coverage 805

K.2.7 TRP measurement procedure 805

K.2.8 Blocking measurement procedure 805

K.3 Indirect far field (IFF) 805

K.3.1 TX beam peak direction search 805

K.3.2 RX beam peak direction search 805

K.3.3 Peak EIRP measurement procedure 805

K.3.4 Peak EIS measurement procedure 805

K.3.5 EIRP spherical coverage 805

K.3.6 EIS spherical coverage 805

K.3.7 TRP measurement procedure 805

K.3.8 Blocking measurement procedure 805

K.4 Near field to far field transform (NFTF) 806

K.4.1 TX beam peak direction search 806

K.4.2 RX beam peak direction search 806

K.4.3 Peak EIRP measurement procedure 806

K.4.4 Peak EIS measurement procedure 806

K.4.5 EIRP spherical coverage 806

K.4.6 EIS spherical coverage 806

K.4.7 TRP measurement procedure 806

K.4.8 Blocking measurement procedure 807

Annex L (normative): Void 808

Annex M:(normative) Measurement grids 808

M.1 Grid Types 808

M.2 Beam Peak Search Grid 810

M.2.1 UE Power classes 810

M.2.1.1 Power class 1 devices 810

M.2.1.2 Power class 2 devices 811

M.2.1.3 Power class 3 devices 811

M.2.1.4 Power class 4 devices 811

M.2.1.5 Power class 5 devices 811

M.2.2 Coarse and fine measurement grids 812

M.3 Spherical Coverage Grid 815

M.3.1 EIRP spherical coverage 815

M.3.1.1 UE Power classes 815

M.3.1.1.1 Power class 1 devices 815

M.3.1.1.2 Power class 2 devices 816

M.3.1.1.3 Power class 3 devices 816

M.3.1.1.4 Power class 4 devices 817

M.3.1.1.5 Power class 5 devices 817

M.3.2 EIS spherical coverage 817

M.3.2.1 UE Power classes 817

M.3.2.1.1 Power class 1 devices 817

M.3.2.1.2 Power class 2 devices 818

M.3.2.1.3 Power class 3 devices 818

M.3.2.1.4 Power class 4 devices 819

M.3.2.1.5 Power class 5 devices 819

M.4 TRP Measurement Grid 819

M.4.1 UE Power Classes 820

M.4.1.1 Power class 1 devices 820

M.4.1.2 Power class 2 devices 820

M.4.1.3 Power class 3 devices 820

M.4.1.4 Power class 4 devices 822

M.4.1.5 Power class 5 devices 822

M.4.2 TRP Integration for Constant Step Size Grid Type 822

M.4.2.1 TRP Integration using Weights 823

M.4.3 TRP Integration for Constant Density Grid Types 824

M.4.4 Interpolation at or near the Pole 825

M.4.5 TRP Grids for Spurious Emissions 825

Annex N (normative): UE coordinate system 828

N.1 Reference coordinate system 828

N.2 Test conditions and angle definitions 829

N.3 DUT positioning guidelines 838

Annex O: Quality of the quiet zone validation 840

O.1 General 840

O.2 Procedure to characterize the quality of the quiet zone for in-band/OOB for the permitted far field methods 840

O.2.1 Equipment used 841

O.2.2 Test frequencies 842

O.2.3 Reference measurements 843

O.2.4 Size of the quiet zone 843

O.2.5 Reference AUT positions 843

O.2.5.1 Distributed-axes system 844

O.2.5.2 Combined-axes system 845

O.2.6 Reference AUT orientations 846

O.2.6.1 Distributed-axes system 846

O.2.6.2 Combined-axes system 848

O.2.7 Quality of quiet zone measurement uncertainty calculations for TRP 849

O.2.8 Quality of quiet zone measurement uncertainty for EIRP/EIS 849

O.3 Procedure to characterize the spurious emissions quality of the quiet zone for the permitted far field methods 850

O.3.1 Equipment used 850

O.3.2 Test frequencies 850

O.3.3 Reference measurements 851

O.3.4 Size of the quiet zone 851

O.3.5 Reference AUT positions 851

O.3.5.1 Distributed-axes system 851

O.3.5.2 Combined-axes system 851

O.3.6 Reference AUT orientations 851

O.3.6.1 Distributed-axes system 851

O.3.6.2 Combined-axes system 853

O.3.7 Quality of quiet zone measurement uncertainty calculations for TRP 853

Annex P (normative): Modified MPR behaviour 854

P.1 Indication of modified MPR behaviour 854

Annex Q (normative): 854

Q.0 General 854

Q.1 Measurement Point 855

Q.2 Relative Phase Error Measurement 855

Q.2.1 Symbols used 855

Q.2.2 CFO (carrier frequency offset) correction 855

Q.2.3 Steps of the measurement method 855

Annex R (informative): Change history 857