|  |  |
| --- | --- |
| 3GPP TS 38.521-4 V18.2.0 (2024-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) conformance specification;  Radio transmission and reception;  Part 4: Performance requirements  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 20

1 Scope 21

2 References 21

3 Definition of terms, symbols and abbreviations 22

3.1 Terms 22

3.2 Symbols 23

3.3 Abbreviations 23

4 General 24

4.1 Relationship between minimum requirements and test requirements 24

4.2 Applicability of minimum requirements 25

4.3 Specification suffix information 25

4.4 Conducted requirements 25

4.4.0 Introduction 25

4.4.1 Reference point 26

4.4.2 SNR definition 26

4.4.3 Noc 26

4.4.3.1 Introduction 26

4.4.3.2 Noc for NR operating bands in FR1 26

4.4.3.2.1 Derivation of Noc values for NR operating bands in FR1 26

4.4.4 Es 27

4.4.4.1 Introduction 27

4.4.4.2 Es for NR operating bands in FR1 27

4.4.4.2.1 Derivation of Es values for NR operating bands in FR1 27

4.5 Radiated requirements 28

4.5.0 Introduction 28

4.5.1 Reference point 28

4.5.2 SNR definition 28

4.5.3 Noc 29

4.5.3.1 Introduction 29

4.5.3.2 Noc for NR operating bands in FR2 29

4.5.3.3 Derivation of Noc values for NR operating bands in FR2 29

4.5.4 Angle of arrival 30

4.5.5 Es 30

4.6 Test coverage across 5G NR connectivity options 30

5 Demodulation performance requirements (Conducted requirements) 31

5.1 General 31

5.1.1 Applicability of requirements 31

5.1.1.1 General 31

5.1.1.2 Applicability of requirements for different number of RX antenna ports 31

5.1.1.3 Applicability of requirements for optional UE features 31

5.1.1.4 Applicability of requirements for mandatory UE features with capability signalling 35

5.1.1.5 Applicability of CA requirements 39

5.1.1.5.1 Definition of CA capability 39

5.1.1.5.2 Applicability and test rules for different CA configurations and bandwidth combination sets 39

5.1.1.5.3 Applicability rule and antenna connection for CA tests with 4 RX 41

5.1.1.5.4 Applicability of different requirements for HST 41

5.1.1.6 Applicability and test rules for PDSCH performance requirements with power imbalance for intra-band contiguous CA 44

5.1.1.7 Applicability of different requirements for HST 45

5.1.1.8 Applicability of different requirements with Multi-TRxP 45

5.1.1.9 Applicability of requirements for PDSCH on bands with shared spectrum access 46

5.1.1.10 Applicability of requirements for PDSCH with inter cell interference 46

5.1.1.11 Applicability of requirements for RedCap 46

5.2 PDSCH demodulation requirements 47

5.2.1 1RX requirements 51

5.2.1.1 FDD 51

5.2.1.1.1 1Rx FDD FR1 PDSCH performance for RedCap 51

5.2.1.2 TDD 54

5.2.1.2.1 1Rx TDD FR1 PDSCH performance for RedCap 54

5.2.2 2RX requirements 57

5.2.2.1 FDD 57

5.2.2.1.1 2Rx FDD FR1 PDSCH mapping Type A performance 57

5.2.2.1.1\_1 2Rx FDD FR1 PDSCH mapping Type A performance - 2x2 MIMO with baseline receiver for both SA and NSA 59

5.2.2.1.1\_2 2Rx FDD FR1 PDSCH mapping Type A performance - 2x2 MIMO with enhanced receiver type 1 for both SA and NSA 63

5.2.2.1.1\_3 2Rx FDD FR1 PDSCH mapping Type A performance – 2x2 MIMO with baseline receiver for DL1024QAM for both SA and NSA 64

5.2.2.1.2 2Rx FDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance 66

5.2.2.1.2\_1 2Rx FDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance - 2x2 MIMO with baseline receiver for both SA and NSA 67

5.2.2.1.3 2Rx FDD FR1 PDSCH mapping Type B performance 69

5.2.2.1.3\_1 2Rx FDD FR1 PDSCH mapping Type B performance - 2x2 MIMO with baseline receiver for both SA and NSA 70

5.2.2.1.4 2Rx FDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance 72

5.2.2.1.4\_1 2Rx FDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance - 4x2 MIMO with baseline receiver for both SA and NSA 73

5.2.2.1.5 2Rx FDD FR1 PDSCH 0.001% BLER performance 78

5.2.2.1.5\_1 2Rx FDD FR1 PDSCH 0.001% BLER performance - 1x2 MIMO with baseline receiver for both SA and NSA 79

5.2.2.1.6 2Rx FDD FR1 PDSCH repetitions over multiple slots performance 80

5.2.2.1.6\_1 2Rx FDD FR1 PDSCH repetitions over multiple slots performance - 2x2 MIMO with baseline receiver for both SA and NSA 81

5.2.2.1.7 2Rx FDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance 83

5.2.2.1.7\_1 2Rx FDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance - 2x2 MIMO with baseline receiver for both SA and NSA 84

5.2.2.1.8 2Rx FDD FR1 PDSCH pre-emption performance 86

5.2.2.1.8\_1 2Rx FDD FR1 PDSCH pre-emption performance - 2x2 MIMO with baseline receiver for both SA and NSA 87

5.2.2.1.9 2Rx FDD FR1 HST-SFN performance 90

5.2.2.1.9\_1 2Rx FDD FR1 HST-SFN performance - 2x2 MIMO with baseline receiver for both SA and NSA 91

5.2.2.1.10 2Rx FDD FR1 HST DPS performance 93

5.2.2.1.10\_1 2Rx FDD FR1 HST-DPS performance - 2x2 MIMO with baseline receiver for both SA and NSA 96

5.2.2.1.11 2Rx FDD FR1 PDSCH Single-DCI based SDM scheme performance 102

5.2.2.1.11\_1 2Rx FDD FR1 PDSCH Single-DCI based SDM scheme performance - 2x2 MIMO for both SA and NSA 104

5.2.2.1.12 2Rx FDD FR1 PDSCH Multi-DCI based transmission scheme performance 108

5.2.2.1.12\_1 2Rx FDD FR1 PDSCH Multiple-DCI based transmission scheme performance - 2x2 MIMO for both SA and NSA 109

5.2.2.1.13 2Rx FDD FR1 PDSCH Single-DCI based FDM scheme A performance 114

5.2.2.1.13\_1 2Rx FDD FR1 PDSCH Single-DCI based FDM scheme A performance - 2x2 MIMO for both SA and NSA 115

5.2.2.1.14 2Rx FDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance 119

5.2.2.1.14\_1 2Rx FDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance - 2x2 MIMO for both SA and NSA 120

5.2.2.1.15 2Rx FDD FR1 PDSCH with inter-cell interference 125

5.2.2.1.15\_1 2Rx FDD FR1 PDSCH with inter-cell interference performance - 2x2 MIMO for both SA and NSA 127

5.2.2.1.16 2Rx FDD FR1 for PDSCH with intra-cell inter user interference 130

5.2.2.1.16\_1 2Rx FDD FR1 for PDSCH with intra cell inter user interference performance – 2x2 MIMO for both NSA and SA 131

5.2.2.1.17 2Rx FDD FR1 PDSCH performance for RedCap 133

5.2.2.1.18 2Rx FDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario 137

5.2.2.1.18\_1 2Rx FDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario – 2x2 MIMO for both NSA and SA 139

5.2.2.1.19 2Rx FDD FR1 for PDSCH with inter cell CRS interference 140

5.2.2.1.19\_1 2Rx FDD FR1 for PDSCH with inter cell CRS interference scenario – 4x2 MIMO for both NSA and SA 143

5.2.2.1.20 2Rx FDD FR1 PDSCH HST-SFN Scheme A performance - 2x2 MIMO for both SA and NSA 145

5.2.2.1.21 2Rx FDD FR1 PDSCH HST-SFN Scheme B performance - 2x2 MIMO for both SA and NSA 154

5.2.2.2 TDD 157

5.2.2.2.1 2Rx TDD FR1 PDSCH mapping Type A performance 157

5.2.2.2.1\_1 2Rx TDD FR1 PDSCH mapping Type A performance - 2x2 MIMO with baseline receiver for both SA and NSA 159

5.2.2.2.1\_2 2Rx TDD FR1 PDSCH mapping Type A performance - 2x2 MIMO with enhanced receiver type 1 for both SA and NSA 166

5.2.2.2.1\_3 2Rx TDD FR1 PDSCH mapping Type A performance - 2x2 MIMO with baseline receiver for DL1024QAM for both SA and NSA 166

5.2.2.2.2 2Rx TDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance 168

5.2.2.2.2\_1 2Rx TDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance - 2x2 MIMO with baseline receiver for both SA and NSA 168

5.2.2.2.3 2Rx TDD FR1 PDSCH mapping Type B performance 172

5.2.2.2.3\_1 2Rx TDD FR1 PDSCH mapping Type B performance - 2x2 MIMO with baseline receiver for both SA and NSA 173

5.2.2.2.4 2Rx TDD FR1 PDSCH mapping Type A and LTE-NR coexistence performance 175

5.2.2.2.4\_1 2Rx TDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance - 4x2 MIMO with baseline receiver for both SA and NSA 176

5.2.2.2.5 2Rx TDD FR1 PDSCH 0.001% BLER performance 181

5.2.2.2.5\_1 2Rx TDD FR1 PDSCH 0.001% BLER performance - 1x2 MIMO with baseline receiver for both SA and NSA 182

5.2.2.2.6 2Rx TDD FR1 PDSCH repetitions over multiple slots performance 184

5.2.2.2.6\_1 2Rx TDD FR1 PDSCH repetitions over multiple slots performance - 2x2 MIMO with baseline receiver for both SA and NSA 185

5.2.2.2.7 2Rx TDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance 186

5.2.2.2.7\_1 2Rx TDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance - 2x2 MIMO with baseline receiver for both SA and NSA 187

5.2.2.2.8 2Rx TDD FR1 PDSCH pre-emption performance 189

5.2.2.2.8\_1 2Rx TDD FR1 PDSCH pre-emption performance - 2x2 MIMO with baseline receiver for both SA and NSA 190

5.2.2.2.9 2Rx TDD FR1 HST-SFN performance 192

5.2.2.2.9\_1 2Rx TDD FR1 HST-SFN performance - 2x2 MIMO with baseline receiver for both SA and NSA 193

5.2.2.2.10 2Rx TDD FR1 HST DPS performance 195

5.2.2.2.10\_1 2Rx TDD FR1 HST-DPS performance - 2x2 MIMO with baseline receiver for both SA and NSA 198

5.2.2.2.11 2Rx TDD FR1 PDSCH Single-DCI based SDM scheme performance 204

5.2.2.2.11\_1 2Rx TDD FR1 PDSCH Single-DCI based SDM scheme performance - 2x2 MIMO for both SA and NSA 206

5.2.2.2.12 2Rx TDD FR1 PDSCH Multi-DCI based transmission scheme performance 210

5.2.2.2.12\_1 2Rx TDD FR1 PDSCH Multiple-DCI based transmission scheme performance - 2x2 MIMO for both SA and NSA 211

5.2.2.2.13 2Rx TDD FR1 PDSCH Single-DCI based FDM scheme A performance 212

5.2.2.2.13\_1 2Rx TDD FR1 PDSCH Single-DCI based FDM scheme A performance - 2x2 MIMO for both SA and NSA 214

5.2.2.2.14 2Rx TDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance 215

5.2.2.2.14\_1 2Rx TDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance - 2x2 MIMO for both SA and NSA 216

5.2.2.2.15 2Rx TDD FR1 PDSCH mapping type A performance on band with shared spectrum access 217

5.2.2.2.15\_1 2Rx TDD FR1 PDSCH mapping type A performance on band with shared spectrum access – 2x2 MIMO for both NSA and SA 219

5.2.2.2.16 2Rx TDD FR1 for PDSCH with inter-cell interference performance 221

5.2.2.2.17 2Rx TDD FR1 for PDSCH with intra-cell inter user interference 226

5.2.2.2.17\_1 2Rx TDD FR1 for PDSCH with intra cell inter user interference performance – 2x2 MIMO for both NSA and SA 227

5.2.2.2.18 2Rx TDD FR1 PDSCH performance for RedCap 229

5.2.2.2.19 2Rx TDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario 232

5.2.2.2.19\_1 2Rx TDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario – 4x2 MIMO for both NSA and SA 234

5.2.2.2.20 2Rx TDD FR1 for PDSCH with inter cell CRS interference 236

5.2.2.2.20\_1 2Rx TDD FR1 for PDSCH with inter cell CRS interference scenario – 4x2 MIMO for both NSA and SA 238

5.2.2.2.21 2Rx TDD FR1 PDSCH HST-SFN Scheme A performance - 2x2 MIMO for both SA and NSA 240

5.2.2.2.22 2Rx TDD FR1 PDSCH HST-SFN Scheme B performance - 2x2 MIMO for both SA and NSA 250

5.2.3 4RX requirements 253

5.2.3.1 FDD 253

5.2.3.1.1 4Rx FDD FR1 PDSCH mapping Type A performance 253

5.2.3.1.1\_1 4Rx FDD FR1 PDSCH mapping Type A performance - 2x4 MIMO with baseline receiver for both SA and NSA 256

5.2.3.1.1\_2 4Rx FDD FR1 PDSCH mapping Type A performance - 4x4 MIMO with baseline receiver for both SA and NSA 259

5.2.3.1.1\_3 FFS 260

5.2.3.1.1\_4 4Rx FDD FR1 PDSCH mapping Type A performance - 4x4 MIMO with enhanced receiver type 1 for both SA and NSA 260

5.2.3.1.1\_5 4Rx FDD FR1 PDSCH mapping Type A performance - 2x4 MIMO with baseline receiver for DL1024QAM for both SA and NSA 261

5.2.3.1.1\_5.1 Test purpose 261

5.2.3.1.2 4Rx FDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance 262

5.2.3.1.2\_1 4Rx FDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance - 4x4 MIMO with baseline receiver for both SA and NSA 263

5.2.3.1.3 4Rx FDD FR1 PDSCH mapping Type B performance 266

5.2.3.1.3\_1 4Rx FDD FR1 PDSCH mapping Type B performance - 2x4 MIMO with baseline receiver for both SA and NSA 267

5.2.3.1.4 4Rx FDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance 269

5.2.3.1.4\_1 4Rx FDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance - 4x4 MIMO with baseline receiver for both SA and NSA 270

5.2.3.1.5 4Rx FDD FR1 PDSCH 0.001% BLER performance 271

5.2.3.1.5\_1 4Rx FDD FR1 PDSCH 0.001% BLER performance - 1x4 MIMO with baseline receiver for both SA and NSA 272

5.2.3.1.6 4Rx FDD FR1 PDSCH repetitions over multiple slots performance 273

5.2.3.1.6\_1 4Rx FDD FR1 PDSCH repetitions over multiple slots performance - 2x4 MIMO with baseline receiver for both SA and NSA 274

5.2.3.1.7 4Rx FDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance 276

5.2.3.1.7\_1 4Rx FDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance - 2x4 MIMO with baseline receiver for both SA and NSA 277

5.2.3.1.8 4Rx FDD FR1 PDSCH pre-emption performance 279

5.2.3.1.8\_1 4Rx FDD FR1 PDSCH pre-emption performance - 2x4 MIMO with baseline receiver for both SA and NSA 280

5.2.3.1.9 4Rx FDD FR1 HST-SFN performance 282

5.2.3.1.9\_1 4Rx FDD FR1 HST-SFN performance - 2x4 MIMO with baseline receiver for both SA and NSA 283

5.2.3.1.10 4Rx FDD FR1 HST DPS performance 285

5.2.3.1.10\_1 4Rx FDD FR1 HST-DPS performance - 2x4 MIMO with baseline receiver for both SA and NSA 288

5.2.3.1.11 4Rx FDD FR1 PDSCH Single-DCI based SDM scheme performance 294

5.2.3.1.11\_1 4Rx FDD FR1 PDSCH Single-DCI based SDM scheme performance - 2x4 MIMO for both SA and NSA 296

5.2.3.1.12 4Rx FDD FR1 PDSCH Multi-DCI based transmission scheme performance 300

5.2.3.1.12\_1 4Rx FDD FR1 PDSCH Multiple-DCI based transmission scheme performance - 2x4 MIMO for both SA and NSA 302

5.2.3.1.13 4Rx FDD FR1 PDSCH Single-DCI based FDM scheme A performance 306

5.2.3.1.13\_1 4Rx FDD FR1 PDSCH Single-DCI based FDM scheme A performance - 2x4 MIMO for both SA and NSA 307

5.2.3.1.14 4Rx FDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance 311

5.2.3.1.14\_1 4Rx FDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance - 2x4 MIMO for both SA and NSA 312

5.2.3.1.15 4Rx FDD FR1 PDSCH with inter-cell interference 317

5.2.3.1.15\_1 4Rx FDD FR1 PDSCH with inter-cell interference performance - 2x4 MIMO for both SA and NSA 318

5.2.3.1.16 4Rx FDD FR1 for PDSCH with intra-cell inter-user interference 321

5.2.3.1.16\_1 4Rx FDD FR1 for PDSCH with intra cell inter user interference performance – 2x4 MIMO for both NSA and SA 322

5.2.3.1.16\_2 4Rx FDD FR1 for PDSCH with intra cell inter user interference performance – 4x4 MIMO for both NSA and SA 324

5.2.3.1.17 4Rx FDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario 325

5.2.3.1.17\_1 4Rx FDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario – 2x4 MIMO for both NSA and SA 327

5.2.3.1.18 4Rx FDD FR1 for PDSCH with inter cell CRS interference 328

5.2.3.1.18\_1 4Rx FDD FR1 for PDSCH with inter cell CRS interference scenario – 4x4 MIMO for both NSA and SA 331

5.2.3.1.19 4Rx FDD FR1 PDSCH HST-SFN Scheme A performance - 2x4 MIMO for both SA and NSA 333

5.2.3.1.20 4Rx FDD FR1 PDSCH HST-SFN Scheme B performance - 2x4 MIMO for both SA and NSA 342

5.2.3.2 TDD 345

5.2.3.2.1 4Rx TDD FR1 PDSCH mapping Type A performance 345

5.2.3.2.1\_1 4Rx TDD FR1 PDSCH mapping Type A performance - 2x4 MIMO with baseline receiver for both SA and NSA 348

5.2.3.2.1\_2 4Rx TDD FR1 PDSCH mapping Type A performance - 4x4 MIMO with baseline receiver for both SA and NSA 355

5.2.3.2.1\_3 4Rx TDD FR1 PDSCH mapping Type A performance - 2x4 MIMO with enhanced receiver type 1 for both SA and NSA 356

5.2.3.2.1\_4 4Rx TDD FR1 PDSCH mapping Type A performance - 4x4 MIMO with enhanced receiver type 1 for both SA and NSA 356

5.2.3.2.1\_5 4Rx TDD FR1 PDSCH mapping Type A performance - 2x4 MIMO with baseline receiver for DL1024QAM for both SA and NSA 357

5.2.3.2.1\_5.1 Test purpose 357

5.2.3.2.2 4Rx TDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance 359

5.2.3.2.2\_1 4Rx TDD FR1 PDSCH mapping Type A and CSI-RS overlapped with PDSCH performance - 2x4 MIMO with baseline receiver for both SA and NSA 360

5.2.3.2.3 4Rx TDD FR1 PDSCH mapping Type B performance 362

5.2.3.2.3\_1 4Rx TDD FR1 PDSCH mapping Type B performance - 2x4 MIMO with baseline receiver for both SA and NSA 363

5.2.3.2.4 4Rx TDD FR1 PDSCH mapping Type A performance 365

5.2.3.2.4\_1 4Rx TDD FR1 PDSCH Mapping Type A and LTE-NR coexistence performance - 4x4 MIMO with baseline receiver for both SA and NSA 366

5.2.3.2.5 4Rx TDD FR1 PDSCH 0.001% BLER performance 367

5.2.3.2.5\_1 4Rx TDD FR1 PDSCH 0.001% BLER performance - 1x4 MIMO with baseline receiver for both SA and NSA 368

5.2.3.2.6 4Rx TDD FR1 PDSCH repetitions over multiple slots performance 370

5.2.3.2.6\_1 4Rx TDD FR1 PDSCH repetitions over multiple slots performance - 2x4 MIMO with baseline receiver for both SA and NSA 371

5.2.3.2.7 4Rx TDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance 373

5.2.3.2.7\_1 4Rx TDD FR1 PDSCH Mapping Type B and UE processing capability 2 performance - 2x4 MIMO with baseline receiver for both SA and NSA 374

5.2.3.2.8 4Rx TDD FR1 PDSCH pre-emption performance 376

5.2.3.2.8\_1 4Rx TDD FR1 PDSCH pre-emption performance - 2x4 MIMO with baseline receiver for both SA and NSA 377

5.2.3.2.9 4Rx TDD FR1 HST-SFN performance 378

5.2.3.2.9\_1 4Rx TDD FR1 HST-SFN performance - 2x4 MIMO with baseline receiver for both SA and NSA 379

5.2.3.2.10 4Rx TDD FR1 HST DPS performance 381

5.2.3.2.10\_1 4Rx TDD FR1 HST DPS performance - 2x4 MIMO with baseline receiver for both SA and NSA 384

5.2.3.2.11 4Rx TDD FR1 PDSCH Single-DCI based SDM scheme performance 389

5.2.3.2.11\_1 4Rx TDD FR1 PDSCH Single-DCI based SDM scheme performance - 2x4 MIMO for both SA and NSA 391

5.2.3.2.12 4Rx TDD FR1 PDSCH Multi-DCI based transmission scheme performance 395

5.2.3.2.12\_1 4Rx TDD FR1 PDSCH Multiple-DCI based transmission scheme performance - 2x4 MIMO for both SA and NSA 396

5.2.3.2.13 4Rx TDD FR1 PDSCH Single-DCI based FDM scheme A performance 397

5.2.3.2.13\_1 4Rx TDD FR1 PDSCH Single-DCI based FDM scheme A performance - 2x4 MIMO for both SA and NSA 399

5.2.3.2.14 4Rx TDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance 400

5.2.3.2.14\_1 4Rx TDD FR1 PDSCH Single-DCI based Inter-slot TDM scheme performance - 2x4 MIMO for both SA and NSA 402

5.2.3.2.15 4Rx TDD FR1 PDSCH mapping type A performance on band with shared spectrum access 402

5.2.3.2.15\_1 4Rx TDD FR1 PDSCH mapping type A performance on band with shared spectrum access – 2x4 MIMO for both NSA and SA 404

5.2.3.2.16 4Rx TDD FR1 for PDSCH with inter-cell interference performance 405

5.2.3.2.17 4Rx TDD FR1 for PDSCH with intra-cell inter-user interference 410

5.2.3.2.17\_1 4Rx TDD FR1 for PDSCH with intra cell inter user interference performance – 2x4 MIMO for both NSA and SA 411

5.2.3.2.17\_2 4Rx TDD FR1 for PDSCH with intra cell inter user interference performance – 4x4 MIMO for both NSA and SA 413

5.2.3.2.18 4Rx TDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario 414

5.2.3.2.18\_1 4Rx TDD FR1 for PDSCH CRS interference mitigation under NR-LTE coexistence scenario – 4x4 MIMO for both NSA and SA 416

5.2.3.2.19 4Rx TDD FR1 for PDSCH with inter cell CRS interference 418

5.2.3.2.19\_1 4Rx TDD FR1 for PDSCH with inter cell CRS interference scenario – 4x4 MIMO for both NSA and SA 420

5.2.3.2.20 4Rx TDD FR1 PDSCH HST-SFN Scheme A performance - 2x4 MIMO for both SA and NSA 422

5.2.3.2.21 4Rx TDD FR1 PDSCH HST-SFN Scheme B performance - 2x4 MIMO for both SA and NSA 432

5.2A PDSCH demodulation requirements for CA 437

5.2A.1 1RX requirements (Void) 438

5.2A.2 2RX requirements 438

5.2A.2.1 Requirements for 2RX normal PDSCH 438

5.2A.2.1.0 Minimum conformance requirements for 2RX normal PDSCH 438

5.2A.2.1.1 2Rx Normal PDSCH Demodulation Performance for CA (2DL CA) for both SA and NSA 440

5.2A.2.1.2 2Rx Normal PDSCH Demodulation Performance for CA (3DL CA) for both SA and NSA 443

5.2A.2.1.3 2Rx Normal PDSCH Demodulation Performance for CA (4DL CA) for both SA and NSA 444

5.2A.2.2 Requirements for 2RX PDSCH carrier aggregation with power imbalance 445

5.2A.2.2.0 Minimum conformance requirements for 2RX PDSCH CA with power imbalance 445

5.2A.2.2.1 2Rx PDSCH Demodulation Performance for CA with power imbalance (2DL CA) 446

5.2A.2.2.2 Void 448

5.2A.2.2.3 Void 448

5.2A.2.3 2Rx TDD FR1 PDSCH mapping type A performance of SCell on band with shared spectrum access 448

5.2A.2.4 Requirements for 2RX HST-SFN CA PDSCH 450

5.2A.2.4.0 Minimum conformance requirements for 2RX HST-SFN CA PDSCH 450

5.2A.2.4.1 2Rx PDSCH Demodulation Performance for HST-SFN CA 453

5.2A.2.5 Requirements for 2RX HST-DPS CA PDSCH 457

5.2A.2.5.0 Minimum conformance requirements for 2RX HST-DPS CA PDSCH 457

5.2A.2.5.1 2RX PDSCH Demodulation Performance for HST-DPS CA 462

5.2A.3 4RX requirements 470

5.2A.3.1 Requirements for 4RX normal PDSCH 470

5.2A.3.1.0 Minimum conformance requirements for 4RX normal PDSCH 470

5.2A.3.1.1 4Rx Normal PDSCH Demodulation Performance for CA (2DL CA) 472

5.2A.3.1.2 4Rx Normal PDSCH Demodulation Performance for CA (3DL CA) 475

5.2A.3.1.3 4Rx Normal PDSCH Demodulation Performance for CA (4DL CA) 476

5.2A.3.2 Requirements for 4RX PDSCH carrier aggregation with power imbalance 476

5.2A.3.2.0 Minimum requirements for carrier aggregation with power imbalance 476

5.2A.3.2.1 4Rx PDSCH Demodulation Performance for CA with power imbalance (2DL CA) 478

5.2A.3.3 4Rx TDD FR1 PDSCH mapping type A performance of SCell on band with shared spectrum access 479

5.2A.3.4 Requirements for 4RX HST-SFN CA PDSCH 481

5.2A.3.4.0 Minimum conformance requirements for 4RX HST-SFN CA PDSCH 481

5.2A.3.4.1 4RX PDSCH Demodulation Performance for HST-SFN CA 484

5.2A.3.5 Requirements for 4RX HST-DPS CA PDSCH 487

5.2A.3.5.0 Minimum conformance requirements for 4RX HST-DPS CA PDSCH 487

5.2A.3.5.1 4RX PDSCH Demodulation Performance for HST-DPS CA 493

5.2A.3A 2Rx-4RX requirements 501

5.2A.3A.1 Requirements for 2Rx-4RX normal PDSCH 501

5.2A.3A.1.0 Minimum conformance requirements for 2Rx-4RX normal PDSCH 501

5.2A.3A.1.1 2Rx-4Rx Normal PDSCH Demodulation Performance for CA (2DL CA) 501

5.2A.3A.1.2 2Rx-4Rx Normal PDSCH Demodulation Performance for CA (3DL CA) 505

5.2A.3A.1.3 2Rx-4Rx Normal PDSCH Demodulation Performance for CA (4DL CA) 506

5.3 PDCCH demodulation requirements 506

5.3.1 1RX requirements 508

5.3.1.1 FDD 508

5.3.1.1.1 1Rx FDD FR1 PDCCH performance for RedCap 508

5.3.1.2 TDD 510

5.3.1.2.1 1Rx TDD FR1 PDCCH performance for RedCap 511

5.3.2 2RX requirements 513

5.3.2.1 FDD 513

5.3.2.1.1 2Rx FDD FR1 PDCCH 1 Tx antenna performance for both SA and NSA 513

5.3.2.1.2 2Rx FDD FR1 PDCCH 2 Tx antenna performance for both SA and NSA 516

5.3.2.1.3 2Rx FDD FR1 PDCCH 1 Tx antenna performance for power saving 519

5.3.2.1.4 2Rx FDD FR1 PDCCH performance for RedCap 525

5.3.2.1.5 2RX FDD Minimum requirements for PDCCH with intra-slot repetition 527

5.3.2.2 TDD 531

5.3.2.2.1 2Rx TDD FR1 PDCCH 1 Tx antenna performance for both SA and NSA 531

5.3.2.2.2 2Rx TDD FR1 PDCCH 2 Tx antenna performance for both SA and NSA 535

5.3.2.2.3 2Rx TDD FR1 PDCCH 1 Tx antenna performance for power saving 537

5.3.2.2.4 2Rx TDD FR1 PDCCH performance for RedCap 543

5.3.2.2.5 2RX TDD Minimum requirements for PDCCH with intra-slot repetition 545

5.3.3 4RX requirements 549

5.3.3.1 FDD 549

5.3.3.1.1 4Rx FDD FR1 PDCCH 1 Tx antenna performance for both SA and NSA 549

5.3.3.1.2 4Rx FDD FR1 PDCCH 2 Tx antenna performance for both SA and NSA 552

5.3.3.1.3 4Rx FDD FR1 PDCCH 1 Tx antenna performance for power saving 555

5.3.3.1.4 4RX FDD Minimum requirements for PDCCH with intra-slot repetition 561

5.3.3.2 TDD 565

5.3.3.2.1 4Rx TDD FR1 PDCCH 1 Tx antenna performance for both SA and NSA 565

5.3.3.2.2 4Rx TDD FR1 PDCCH 2 Tx antenna performance for both SA and NSA 568

5.3.3.2.3 4Rx TDD FR1 PDCCH 1 Tx antenna performance for power saving 571

5.3.3.2.4 4RX TDD Minimum requirements for PDCCH with intra-slot repetition 577

5.4 PBCH demodulation requirements 581

5.5 Sustained downlink data rate provided by lower layers 581

5.5.1 FR1 Sustained downlink data rate performance for single carrier 581

5.5.2 FR1 Sustained downlink data rate performance for single carrier with DL1024QAM 589

5.5.3 FR1 Sustained downlink data rate performance for RedCap 591

5.5A.1 FR1 Sustained downlink data rate performance for carrier aggregation 592

5.5A.1.1 FR1 SDR performance for CA (2DL CA) 592

5.5A.1.2 FR1 SDR performance for CA (3DL CA) 600

5.5A.1.2.1 Test Purpose 600

5.5A.1.2.2 Test applicability 600

5.5A.1.2.3 Minimum conformance requirements 600

5.5A.1.2.4 Test description 600

5.5A.1.2.5 Test requirement 600

5.5A.1.3 FR1 SDR performance for CA (4DL CA) 600

5.5A.1.3.1 Test Purpose 600

5.5A.1.3.2 Test applicability 600

5.5A.1.3.3 Minimum conformance requirements 601

5.5A.1.3.4 Test description 601

5.5A.1.3.5 Test requirement 601

5.5A.1.4 FR1 SDR performance for CA (5DL CA) 601

5.5A.1.4.1 Test Purpose 601

5.5A.1.4.2 Test applicability 601

5.5A.1.4.3 Minimum conformance requirements 601

5.5A.1.4.4 Test description 601

5.5A.1.4.5 Test requirement 601

6 CSI reporting requirements (Conducted requirements) 602

6.1 General 602

6.1.1 Applicability of requirements 602

6.1.1.1 General 602

6.1.1.2 Applicability of requirements for different number of RX antenna ports 602

6.1.1.3 Applicability of requirements for optional UE features 602

6.1.1.4 Applicability of requirements for mandatory UE features with capability signalling 603

6.1.1.5 Applicability of Channel Quality Indicator (CQI) reporting requirements for CA 604

6.1.1.5.1 Applicability and test rules for different duplex modes and SCS combinations 604

6.1.1.5.2 Applicability and test rules for different CA configurations and bandwidth combination sets 604

6.1.1.5.3 Test coverage for different number of component carriers 605

6.1.1.5.4 Applicability rule and antenna connection for CA tests with 4 RX 605

6.1.1.6 Applicability of requirements for RedCap 605

6.1.2 Common test parameters 605

6.2 Reporting of Channel Quality Indicator (CQI) 608

6.2.1 1RX requirements 608

6.2.1.1 FDD 608

6.2.1.1.1 CQI reporting definition under AWGN conditions 608

6.2.1.1.1.1 1Rx FDD FR1 periodic CQI reporting under AWGN conditions for RedCap 608

6.2.1.1.2 CQI reporting under fading conditions 612

6.2.1.1.2.1 1Rx FDD FR1 periodic wideband CQI reporting under fading conditions for RedCap 612

6.2.1.2 TDD 617

6.2.1.2.1 CQI reporting definition under AWGN conditions 617

6.2.1.2.1.1 1Rx TDD FR1 periodic CQI reporting under AWGN conditions for RedCap 617

6.2.1.2.2 CQI reporting definition under fading conditions 620

6.2.1.2.2.1 1Rx TDD FR1 periodic wideband CQI reporting under fading conditions for RedCap 620

6.2.2 2RX requirements 627

6.2.2.1 FDD 627

6.2.2.1.1 CQI reporting definition under AWGN conditions 627

6.2.2.1.1.1 2Rx FDD FR1 periodic CQI reporting under AWGN conditions for both SA and NSA 627

6.2.2.1.1.2 2Rx FDD FR1 periodic CQI reporting with Table 3 under AWGN conditions for both SA and NSA 630

6.2.2.1.1.3 2Rx FDD FR1 periodic CQI reporting with Table 4 under AWGN conditions for both SA and NSA 635

6.2.2.1.1.4 2Rx FDD FR1 periodic CQI reporting under AWGN conditions for RedCap 638

6.2.2.1.2 CQI reporting under fading conditions 641

6.2.2.1.2.1 2Rx FDD FR1 periodic wideband CQI reporting under fading conditions for both SA and NSA 641

6.2.2.1.2.2 2Rx FDD FR1 aperiodic subband CQI reporting under fading conditions for both SA and NSA 647

6.2.2.1.2.3 2Rx FDD FR1 Wideband CQI reporting with inter-cell intereference 652

6.2.2.1.2.4 2Rx FDD FR1 periodic wideband CQI reporting under fading conditions for RedCap 655

6.2.2.2 TDD 658

6.2.2.2.1 CQI Reporting definition under AWGN conditions 658

6.2.2.2.1.1 2Rx TDD FR1 periodic CQI reporting under AWGN conditions for both SA and NSA 658

6.2.2.2.1.2 2Rx TDD FR1 periodic CQI reporting with Table 3 under AWGN conditions for both SA and NSA 661

6.2.2.2.1.3 2Rx TDD FR1 CQI reporting for PCell on band with shared spectrum access under AWGN conditions for both SA and NSA 666

6.2.2.2.1.4 2Rx TDD FR1 periodic CQI reporting with Table 4 under AWGN conditions for both SA and NSA 670

6.2.2.2.1.5 2Rx TDD FR1 periodic CQI reporting under AWGN conditions for RedCap 673

6.2.2.2.2 CQI reporting under fading conditions 677

6.2.2.2.2.1 2Rx TDD FR1 periodic wideband CQI reporting under fading conditions for both SA and NSA 677

6.2.2.2.2.2 2Rx TDD FR1 aperiodic subband CQI reporting under fading conditions for both SA and NSA 681

6.2.2.2.2.3 2Rx FDD FR1 Wideband CQI reporting with inter-cell interference 685

6.2.2.2.2.4 2Rx TDD FR1 periodic wideband CQI reporting under fading conditions for RedCap 688

6.2.3 4RX requirements 692

6.2.3.1 FDD 692

6.2.3.1.1 CQI reporting definition under AWGN conditions 692

6.2.3.1.1.1 4Rx FDD FR1 periodic CQI reporting under AWGN conditions for both SA and NSA 693

6.2.3.1.1.2 4Rx FDD FR1 periodic CQI reporting with Table 3 under AWGN conditions for both SA and NSA 696

6.2.3.1.1.3 4Rx FDD FR1 periodic CQI reporting with Table 4 under AWGN conditions for both SA and NSA 699

6.2.3.1.2 CQI reporting definition under fading conditions 702

6.2.3.1.2.1 4Rx FDD FR1 periodic wideband CQI reporting under fading conditions for both SA and NSA 702

6.2.3.1.2.2 4Rx FDD FR1 aperiodic subband CQI reporting under fading conditions for both SA and NSA 706

6.2.3.1.2.3 4Rx FDD FR1 Wideband CQI reporting with inter-cell interference 708

6.2.3.2 TDD 711

6.2.3.2.1 CQI reporting definition under AWGN conditions 711

6.2.3.2.1.1 4Rx TDD FR1 periodic CQI reporting under AWGN conditions for both SA and NSA 712

6.2.3.2.1.2 4Rx TDD FR1 periodic CQI reporting with Table 3 under AWGN conditions for both SA and NSA 715

6.2.3.2.1.3 4Rx TDD FR1 CQI reporting for PCell on band with shared spectrum access under AWGN conditions for both SA and NSA 718

6.2.3.2.1.4 4Rx TDD FR1 periodic CQI reporting with Table 4 under AWGN conditions for both SA and NSA 722

6.2.3.2.2 CQI reporting under fading conditions 725

6.2.3.2.2.1 4Rx TDD FR1 periodic wideband CQI reporting under fading conditions for both SA and NSA 725

6.2.3.2.2.2 4Rx TDD FR1 aperiodic subband CQI reporting under fading conditions for both SA and NSA 729

6.2.3.2.2.3 4Rx FDD FR1 Wideband CQI reporting with inter-cell interference 732

6.2A Reporting of Channel Quality Indicator (CQI) for CA 734

6.2A.1 General 734

6.2A.2 1RX requirements 735

6.2A.3 2RX and 4RX requirements 735

6.2A.3.1 CQI reporting definition under AWGN conditions 735

6.2A.3.1.0 Minimum requirement for periodic CQI reporting 735

6.2A.3.1.1 CQI reporting accuracy under AWGN conditions for CA (2DL CA) 738

6.2A.3.1.2 CQI reporting accuracy under AWGN conditions for CA (3DL CA) 743

6.2A.3.1.3 CQI reporting accuracy under AWGN conditions for CA (4DL CA) 744

6.3 Reporting of Precoding Matrix Indicator (PMI) 745

6.3.0 General 745

6.3.1 1RX requirements 745

6.3.1.1 FDD 745

6.3.1.1.1 1Rx FDD Single PMI with 4TX TypeI-SinglePanel Codebook for RedCap 745

6.3.1.2 TDD 750

6.3.1.2.1 1Rx TDD Single PMI with 4TX TypeI-SinglePanel Codebook for RedCap 750

6.3.2 2RX requirements 754

6.3.2.1 FDD 754

6.3.2.1.1 2Rx FDD FR1 Single PMI with 4TX TypeI-SinglePanel codebook for both SA and NSA 754

6.3.2.1.2 2Rx FDD FR1 Single PMI with 8TX TypeI-SinglePanel codebook for both SA and NSA 760

6.3.2.1.3 2Rx FDD FR1 Multiple PMI with 16Tx Type I – SinglePanel Codebook for both SA and NSA 765

6.3.2.1.4 2Rx FDD FR1 Single PMI with 32Tx Type1 - SinglePanel codebook for both SA and NSA 769

6.3.2.1.5 2Rx FDD FR1 Multiple PMI with 16Tx TypeII codebook for both SA and NSA 773

6.3.2.1.6 2Rx FDD FR1 Multiple PMI with 16Tx Enhanced TypeII codebook for both SA and NSA 777

6.3.2.1.7 2Rx FDD FR1 Single PMI with 8TX TypeI-SinglePanel codebook for both SA and NSA 781

6.3.2.2 TDD 789

6.3.2.2.1 2Rx TDD FR1 Single PMI with 4TX TypeI-SinglePanel codebook for both SA and NSA 789

6.3.2.2.2 2Rx TDD FR1 Single PMI with 8TX TypeI-SinglePanel codebook for both SA and NSA 794

6.3.2.2.3 2Rx TDD FR1 Multiple PMI with 16Tx Type1 - SinglePanel codebook for both SA and NSA 799

6.3.2.2.4 2Rx TDD FR1 Single PMI with 32Tx Type1 - SinglePanel codebook for both SA and NSA 804

6.3.2.2.5 2Rx TDD FR1 Multiple PMI with 16Tx TypeII codebook for both SA and NSA 809

6.3.2.2.6 2Rx TDD FR1 Multiple PMI with 16Tx Enhanced TypeII codebook for both SA and NSA 813

6.3.2.2.7 2Rx TDD Single PMI with 4TX TypeI-SinglePanel Codebook for RedCap 817

6.3.2.2.8 Single PMI with 8 ports TypeI-SinglePanel Codebook for Single-DCI based transmission scheme 822

6.3.3 4RX requirements 830

6.3.3.1 FDD 830

6.3.3.1.1 4Rx FDD FR1 Single PMI with 4TX TypeI-SinglePanel codebook for both SA and NSA 830

6.3.3.1.2 4Rx FDD FR1 Single PMI with 8TX TypeI-SinglePanel codebook for both SA and NSA 836

6.3.3.1.3 4Rx FDD FR1 Multiple PMI with 16Tx Type I – SinglePanel Codebook for both SA and NSA 841

6.3.3.1.4 4Rx FDD FR1 Single PMI with 32Tx Type1 - SinglePanel codebook for both SA and NSA 845

6.3.3.1.5 4Rx FDD FR1 Multiple PMI with 16Tx TypeII codebook for both SA and NSA 849

6.3.3.1.6 4Rx FDD FR1 Multiple PMI with 16Tx Enhanced TypeII codebook for both SA and NSA 853

6.3.3.1.7 Single PMI with 8 ports TypeI-SinglePanel Codebook for Single-DCI based transmission scheme 857

6.3.3.2 TDD 865

6.3.3.2.1 4Rx TDD FR1 Single PMI with 4TX TypeI-SinglePanel codebook for both SA and NSA 865

6.3.3.2.2 4Rx TDD FR1 Single PMI with 8TX TypeI-SinglePanel codebook for both SA and NSA 871

6.3.3.2.3 4Rx TDD FR1 Multiple PMI with 16Tx Type1 - SinglePanel codebook for both SA and NSA 876

6.3.3.2.4 4Rx TDD FR1 Single PMI with 32Tx Type1 - SinglePanel codebook for both SA and NSA 881

6.3.3.2.5 4Rx TDD FR1 Multiple PMI with 16Tx TypeII codebook for both SA and NSA 886

6.3.3.2.6 4Rx TDD FR1 Multiple PMI with 16Tx Enhanced TypeII codebook for both SA and NSA 890

6.3.3.2.7 Single PMI with 8 ports TypeI-SinglePanel Codebook for Single-DCI based transmission scheme 894

6.4 Reporting of Rank Indicator (RI) 903

6.4.1 1RX requirements (Void) 903

6.4.2 2RX requirements 903

6.4.2.1 FDD 903

6.4.2.1\_1 2Rx FDD FR1 RI reporting for both SA and NSA 903

6.4.2.1.1 2Rx FDD FR1 RI reporting for RedCap 907

6.4.2.2 TDD 912

6.4.2.2\_1 2Rx TDD FR1 RI reporting for both SA and NSA 912

6.4.2.2.1 2Rx TDD FR1 RI reporting for RedCap 918

6.4.3 4RX requirements 922

6.4.3.1 FDD 922

6.4.3.1\_1 4Rx FDD FR1 RI reporting for both SA and NSA 922

6.4.3.2 TDD 928

6.4.3.2\_1 4Rx TDD FR1 RI reporting for both SA and NSA 928

7 Demodulation performance requirements (Radiated requirements) 933

7.1 General 933

7.1.1 Applicability of requirements 933

7.1.1.1 General 933

7.1.1.2 Applicability of requirements for different number of RX antenna ports 933

7.1.1.3 Applicability of requirements for optional UE features 933

7.1.1.4 Applicability of requirements for mandatory UE features with capability signaling 934

7.1.1.5 Applicability of CA requirements 934

7.1.1.5.1 Definition of CA capability 934

7.1.1.5.2 Applicability and test rules for different CA configurations and bandwidth combination sets 935

7.1.1.6 FFS 935

7.1.1.7 Applicability of requirements for RedCap 935

7.1.1\_1 Applicability of test requirements due to maximum achievable SNR 936

7.2 PDSCH demodulation requirements 938

7.2.1 1RX requirements (Void) 941

7.2.2 2RX requirements 941

7.2.2.1 FDD (Void) 941

7.2.2.2 TDD 941

7.2.2.2.1 2Rx TDD FR2 PDSCH mapping Type A performance 941

7.2.2.2.1\_1 2Rx TDD FR2 PDSCH mapping Type A performance - 2x2 MIMO with baseline receiver for SA and NSA 943

7.2.2.2.1\_2 2Rx TDD FR2 PDSCH mapping Type A performance - 2x2 MIMO with enhanced type 1 receiver for SA and NSA 947

7.2.2.2.1\_3 2Rx TDD FR2 PDSCH mapping Type A performance - 2x2 MIMO with 256QAM for SA and NSA (Rel-16 and forward) 948

7.2.2.2.2 2Rx TDD FR2 PDSCH repetitions over multiple slots 950

7.2.2.2.2\_1 2Rx TDD FR2 PDSCH repetitions over multiple slots - 2x2 MIMO with baseline receiver for SA and NSA 951

7.2.2.2.3 2Rx TDD FR2 PDSCH Mapping Type B 953

7.2.2.2.3\_1 2Rx TDD FR2 PDSCH mapping Type B performance - 2x2 MIMO with baseline receiver for SA and NSA 954

7.2A PDSCH demodulation requirements for CA 955

7.2A.1 1RX requirements (Void) 956

7.2A.2 2RX requirements 956

7.2A.2.1 2Rx TDD FR2 CA requirements for normal PDSCH Demodulation Performance for both SA and NSA (2DLCA) 957

7.2A.2.2 2Rx TDD FR2 CA requirements for normal PDSCH Demodulation Performance for both SA and NSA (3DLCA) 958

7.2A.2.3 2Rx TDD FR2 CA requirements for normal PDSCH Demodulation Performance for both SA and NSA (4DLCA) 959

7.3 PDCCH demodulation requirements 960

7.3.1 1RX requirements 962

7.3.2 2RX requirements 962

7.3.2.1 FDD 962

7.3.2.2 TDD 962

7.3.2.2.1 2Rx TDD FR2 PDCCH 1 Tx antenna performance for both SA and NSA 962

7.3.2.2.2 2Rx TDD FR2 PDCCH 2 Tx antenna performance for both SA and NSA 965

7.3.2.2.3 2Rx TDD FR2 PDCCH 1 Tx antenna performance for power saving 968

7.4 PBCH demodulation requirements 973

7.5 Sustained downlink data rate provided by lower layers 973

7.5.1 FR2 Sustained downlink data rate performance for single carrier 973

7.5.2 FR2 Sustained downlink data rate performance for RedCap 980

7.5A.1 FR2 Sustained downlink data rate performance for carrier aggregation 981

7.5A.1.1 FR2 SDR performance for CA (2DL CA) 981

7.5A.1.2 FR2 SDR performance for CA (3DL CA) 984

7.5A.1.3 FR2 SDR performance for CA (4DL CA) 985

7.5A.1.4 FR2 SDR performance for CA (5DL CA) 985

7.5A.1.5 FR2 SDR performance for CA (6DL CA) 985

7.5A.1.6 FR2 SDR performance for CA (7DL CA) 986

7.5A.1.7 FR2 SDR performance for CA (8DL CA) 986

8 CSI reporting requirements (Radiated requirements) 987

8.1 General 987

8.1.1 Applicability of requirements 987

8.1.1.1 General 987

8.1.1.2 Applicability of requirements for different number of RX antenna ports 987

8.1.1.3 Applicability of requirements for optional UE features 987

8.1.1.4 Applicability of requirements for mandatory UE features with capability signalling 988

8.1.1.5 Applicability of Channel Quality Indicator (CQI) reporting requirements for CA 988

8.1.1.5.1 Applicability and test rules for different CA configurations and bandwidth combination sets 988

8.1.1.5.2 Test coverage for different number of component carriers 988

8.1.1.6 Applicability of requirements for RedCap 988

8.1.1\_1 Applicability of test requirements due to maximum achievable SNR 988

8.1.2 Common test parameters 989

8.2 Reporting of Channel Quality Indicator (CQI) 992

8.2.1 1RX requirements 992

8.2.2 2RX requirements 992

8.2.2.1 FDD 992

8.2.2.2 TDD 992

8.2.2.2.1 CQI reporting under AWGN conditions 992

8.2.2.2.1.1 2Rx TDD FR2 periodic wideband CQI reporting under AWGN performance for both SA and NSA 992

8.2.2.2.2 CQI reporting under fading conditions 996

8.2.2.2.2.1 2Rx TDD FR2 aperiodic wideband CQI reporting under fading performance for both SA and NSA 996

8.2.2.2.2.1\_1 2Rx TDD FR2 aperiodic CQI wideband reporting under fading performance for both SA and NSA – 256QAM (Rel-16 and forward) 1003

8.2A Reporting of Channel Quality Indicator (CQI) for CA 1007

8.2A.1 General 1007

8.2A.2 1RX requirements 1007

8.2A.3 2RX requirements 1007

8.2A.3.1 CQI reporting definition under AWGN conditions 1007

8.2A.3.1.0 Minimum requirement for periodic CQI reporting 1007

8.2A.3.1.1 2Rx CQI reporting accuracy under AWGN conditions for CA (2DL CA) 1009

8.2A.3.1.2 2Rx CQI reporting accuracy under AWGN conditions for CA (3DL CA) 1011

8.2A.3.1.3 2Rx CQI reporting accuracy under AWGN conditions for CA (4DL CA) 1012

8.3 Reporting of Precoding Matrix Indicator (PMI) 1013

8.3.0 General 1013

8.3.1 1RX requirements (Void) 1013

8.3.2 2RX requirements 1013

8.3.2.1 FDD 1013

8.3.2.2 TDD 1013

8.3.2.2.1 2Rx TDD FR2 Single PMI with 2TX TypeI-SinglePanel codebook for both SA and NSA 1013

8.4 Reporting of Rank Indicator (RI) 1019

8.4.1 1RX requirements 1019

8.4.2 2RX requirements 1019

8.4.2.1 FDD 1019

8.4.2.2 TDD 1019

8.4.2.2.1 2Rx TDD FR2 RI reporting for both SA and NSA 1019

9 Demodulation performance requirements for interworking 1025

9.1 General 1025

9.1.1 Applicability of requirements 1025

9.1.1.1 Applicability of requirements for optional UE features 1026

9.1.1.2 Applicability of requirements for mandatory UE features with capability signalling 1026

9.1.2 E-UTRA Cell setup 1026

9.1.2.1 FDD 1026

9.1.2.2 TDD 1027

9.2 Void 1028

9.2A PDSCH Demodulation for CA 1028

9.2A.1 NR CA between FR1 and FR2 1028

9.2B PDSCH Demodulation for DC 1029

9.2B.1 EN-DC 1029

9.2B.1.1 EN-DC within FR1 1029

9.2B.1.2 EN-DC including FR2 NR carrier only 1029

9.2B.1.3 EN-DC including FR1 and FR2 NR carriers 1029

9.2B.2 NR DC between FR1 and FR2 1029

9.3 Void 1029

9.3A PDCCH Demodulation for CA 1029

9.3A.1 NR CA between FR1 and FR2 1029

9.3B PDCCH Demodulation for DC 1029

9.3B.1 EN-DC 1029

9.3B.1.1 EN-DC within FR1 1029

9.3B.1.2 EN-DC including FR2 NR carrier only 1030

9.3B.1.3 EN-DC including FR1 and FR2 NR carriers 1030

9.3B.2 NR DC between FR1 and FR2 1030

9.4 Void 1030

9.4A SDR test for CA 1030

9.4A.1 Sustained downlink data rate performance for NR CA between FR1 and FR2 1030

9.4B SDR test for DC 1030

9.4B.1 EN-DC 1030

9.4B.1.1 Sustained downlink data rate performance for EN-DC within FR1 1030

9.4B.1.1\_1 Sustained downlink data rate performance for EN-DC within FR1 (2 NR CCs) 1043

9.4B.1.1\_2 Sustained downlink data rate performance for EN-DC within FR1 (3 NR CCs) 1043

9.4B.1.1\_3 Sustained downlink data rate performance for EN-DC within FR1 (4 NR CCs) 1044

9.4B.1.2 Sustained downlink data rate performance for EN-DC including FR2 NR carrier 1044

9.4B.1.2\_1 Sustained downlink data rate performance for EN-DC including FR2 (2 NR CCs) 1055

9.4B.1.2\_2 Sustained downlink data rate performance for EN-DC including FR2 (3 NR CCs) 1056

9.4B.1.2\_3 Sustained downlink data rate performance for EN-DC including FR2 (4 NR CCs) 1056

9.4B.2 NR DC between FR1 and FR2 1057

9.4B.2.1 Sustained downlink data rate performance for NR DC between FR1 and FR2 1057

9.4B.3 NE-DC 1057

9.4B.3.1 Sustained downlink data rate performance for NE-DC within FR1 1057

10 CSI reporting requirements for interworking 1057

10.1 General 1057

10.1.1 Applicability of requirements 1057

10.1.1.1 Applicability of requirements for optional UE features 1058

10.1.1.2 Applicability of requirements for mandatory UE features with capability signalling 1058

10.2 Void 1058

10.2A Reporting of Channel Quality Indicator (CQI) for CA 1058

10.2B Reporting of Channel Quality Indicator (CQI) for DC 1058

10.2B.1 EN-DC 1058

10.2B.1.1 EN-DC within FR1 1058

10.2B.1.2 EN-DC including FR2 NR carrier 1058

10.2B.1.3 EN-DC including FR1 and FR2 NR carriers 1059

10.2B.2 NR DC between FR1 and FR2 1059

10.3A Reporting of Precoding Matrix Indicator (PMI) for CA 1059

10.3B Reporting of Precoding Matrix Indicator (PMI) for DC 1059

10.3B.1 EN-DC 1059

10.3B.1.1 EN-DC within FR1 1059

10.3B.1.2 EN-DC including FR2 NR carrier 1059

10.3B.1.3 EN-DC including FR1 and FR2 NR carriers 1059

10.3B.2 NR DC between FR1 and FR2 1059

10.4A Reporting of Rank Indicator (RI) for CA 1060

10.4B Reporting of Rank Indicator (RI) for DC 1060

10.4B.1 EN-DC 1060

10.4B.1.1 EN-DC within FR1 1060

10.4B.1.2 EN-DC including FR2 NR carrier 1060

10.4B.1.3 EN-DC including FR1 and FR2 NR carriers 1060

10.4B.2 NR DC between FR1 and FR2 1060

11 V2X requirements 1060

11.1 Demodulation performance requirements (Conducted requirements) 1061

11.1.1 General 1061

11.1.1.1 Applicability of requirements 1061

11.1.1.1.1 General 1061

11.1.1.1.2 Applicability of requirements for mandatory UE V2X features with capability signalling 1061

11.1.1.2 Common test parameters 1061

11.1.2 PSSCH demodulation requirements 1062

11.1.2.1 2Rx requirements 1062

11.1.2.1.1 2Rx FR1 PSSCH performance 1062

11.1.3 PSCCH demodulation requirements 1065

11.1.3.1 2Rx requirements 1065

11.1.3.1.1 2Rx FR1 PSCCH performance 1065

11.1.4 PSBCH demodulation requirements 1067

11.1.4.1 2Rx requirements 1067

11.1.4.1.1 2Rx FR1 PSBCH performance 1067

11.1.5 PSFCH demodulation requirements 1067

11.1.5.1 2Rx requirements 1067

11.1.5.1.1 2Rx FR1 PSFCH performance 1067

11.1.6 Power imbalance performance with two links 1070

11.1.6.1 2Rx requirements 1070

11.1.6.1.1 2Rx FR1 Power imbalance performance 1070

11.1.7 HARQ buffer soft combining 1073

11.1.7.1 2Rx requirements 1073

11.1.7.1.1 2Rx FR1 HARQ buffer soft combining performance 1073

11.1.8 PSCCH decoding capability test 1076

11.1.8.1 2Rx requirements 1076

11.1.8.1.1 2Rx FR1 PSCCH decoding capability 1076

11.1.9 PSFCH decoding capability Test 1079

11.1.9.1 2Rx requirements 1079

11.1.9.1.1 2Rx FR1 PSFCH decoding capability 1079

Annex A (normative): Measurement channels 1082

A.1 General 1082

A.1.1 Throughput definition 1082

A.1.2 TDD UL-DL configurations for FR1 1082

A.1.3 TDD UL-DL configurations for FR2 1086

A.2 UL Reference measurement channels 1088

A.2.1 General 1088

A.2.2 Reference measurement channels for FDD 1089

A.2.2.1 RMC for Sustained downlink data rate 1089

A.2.2.1.1 CP-OFDM 64QAM 1089

A.2.3 Reference measurement channels for TDD 1091

A.2.3.1 RMC for Sustained downlink data rate 1091

A.2.3.1.1 CP-OFDM 16QAM 1091

A.3 DL reference measurement channels 1093

A.3.1 General 1093

A.3.2 Reference measurement channels for PDSCH performance requirements 1093

A.3.2.1 FDD 1094

A.3.2.1.1 Reference measurement channels for SCS 15 kHz FR1 1094

A.3.2.1.2 Reference measurement channels for SCS 30 kHz FR1 1113

A.3.2.1.3 Reference measurement channels for SCS 60 kHz FR1 1114

A.3.2.1.4 Reference measurement channels for E-UTRA 1114

A.3.2.1.5 Reference measurement channels for Intra-cell Inter-UE interference scenario 1120

A.3.2.2 TDD 1121

A.3.2.2.1 Reference measurement channels for SCS 15 kHz FR1 1121

A.3.2.2.2 Reference measurement channels for SCS 30 kHz FR1 1127

A.3.2.2.3 Reference measurement channels for SCS 60 kHz FR1 1168

A.3.2.2.4 Reference measurement channels for SCS 60 kHz FR2 1168

A.3.2.2.5 Reference measurement channels for SCS 120 kHz FR2 1170

A.3.2.2.6 Reference measurement channels for E-UTRA 1180

A.3.2.2.7 Reference measurement channels for Intra-cell Inter-UE interference scenario 1186

A.3.2.3 HD-FDD 1187

A.3.2.3.1 Reference measurement channels for SCS 15 kHz FR1 1187

A.3.2\_1 Reference measurement channels for Sustained downlink data rate performance requirements 1190

A.3.2\_1.1 FDD 1190

A.3.2\_1.1.1 Reference measurement channels for SCS 15 kHz FR1 1190

A.3.2\_1.2 TDD 1193

A.3.2\_1.2.1 Reference measurement channels for SCS 30 kHz FR1 1193

A.3.2\_1.2.2 Reference measurement channels for SCS 120 kHz FR2 1196

A.3.3 Reference measurement channels for PDCCH performance requirements 1198

A.3.3.1 FDD 1198

A.3.3.1.1 Reference measurement channels for SCS 15 kHz FR1 1198

A.3.3.1.2 Reference measurement channels for SCS 30 kHz FR1 1199

A.3.3.2 TDD 1200

A.3.3.2.1 Reference measurement channels for SCS 15 kHz FR1 1200

A.3.3.2.2 Reference measurement channels for SCS 30 kHz FR1 1201

A.3.3.2.3 Reference measurement channels for SCS 60 kHz FR1 1203

A.3.3.2.4 Reference measurement channels for SCS 60 kHz FR2 1203

A.3.3.2.5 Reference measurement channels for SCS 120 kHz FR2 1203

A.3.4 Reference measurement channels for PBCH demodulation requirements 1205

A.3.4.1 Reference measurement channels for FR1 1205

A.3.4.2 Reference measurement channels for FR2 1205

A.4 CSI reference measurement channels 1205

A.5 OFDMA Channel Noise Generator (OCNG) 1211

A.5.1 OCNG Patterns for FDD 1211

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 1211

A.5.2 OCNG Patterns for TDD 1211

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 1211

A.6 SL reference measurement channels 1212

A.6.1 General 1212

A.6.2 Reference measurement channels for PSSCH performance requirements 1212

A.6.2.1 Reference measurement channels for SCS 15 kHz FR1 1212

A.6.2.2 Reference measurement channels for SCS 30 kHz FR1 1212

A.6.3 Reference measurement channels for PSCCH performance requirements 1212

A.6.3.1 Reference measurement channels for SCS 15 kHz FR1 1212

A.6.3.2 Reference measurement channels for SCS 30 kHz FR1 1213

A.6.4 Reference measurement for PSBCH performance requirements 1213

A.6.4.1 Reference measurement channels for SCS 15 kHz FR1 1213

A.6.4.2 Reference measurement channels for SCS 30 kHz FR1 1213

Annex B (normative): Propagation conditions 1213

B.0 No interference 1213

B.1 Static propagation condition 1214

B.1.0 UE Receiver with 1Rx 1214

B.1.1 UE Receiver with 2Rx 1214

B.1.2 UE Receiver with 4Rx 1214

B.2 Multi-path fading propagation conditions 1215

B.2.1 Delay profiles 1215

B.2.1.1 Delay profiles for FR1 1216

B.2.1.2 Delay profiles for FR2 1218

B.2.2 Combinations of channel model parameters 1219

B.2.3 MIMO Channel Correlation Matrices 1219

B.2.3.1 MIMO Correlation Matrices using Uniform Linear Array (ULA) 1220

B.2.3.1.1 Definition of MIMO Correlation Matrices 1220

B.2.3.1.2 MIMO Correlation Matrices at High, Medium and Low Level 1222

B.2.3.2 MIMO Correlation Matrices using Cross Polarized Antennas (X-pol) 1226

B.2.3.2.1 Definition of MIMO Correlation Matrices using cross polarized antennas 1226

B.2.3.2.2 MIMO Correlation Matrices using cross polarized antennas 1228

B.2.3.2.3 Beam steering approach 1231

B.2.3.2.3A Beam steering approach with dual cluster beams 1232

B.2.4 Two-tap propagation conditions for CQI tests 1233

B.3 High Speed Train Scenario 1234

B.3.1 Single Tap Channel Profile 1234

B.3.2 HST-SFN Channel Profile 1237

B.3.3 HST-DPS Channel Profile 1240

B.3.4 FFS 1244

B.3.5 HST-SFN Scheme A Channel Profile 1244

B.3.6 HST-SFN Scheme B Channel Profile 1247

B.4 Physical signals, channels mapping and precoding 1250

B.4.1 General 1250

B.4.2 Beamforming for MU-MIMO 1251

B.5 Downlink Transmission Model for requirements on bands with shared spectrum access 1251

B.5.1 Downlink Transmission Model for bands with shared spectrum access 1251

B.6 Interference model for PDSCH requirements with intercell interference 1252

B.6.1 Interference to Noise ratio (INR) 1252

B.6.2 Interference model for PDSCH requirements 1252

B.7 Interference model for PDSCH requirements with LTE-NR spectrum sharing 1253

Annex C (normative): Downlink physical channels 1254

C.0 Downlink signal levels 1254

C.0.1 FR1 Downlink Signal Levels (Conducted) 1254

C.0.2 FR2 Downlink Signal Levels (Radiated) 1254

C.1 Setup 1255

C.1.1 FR1 Setup 1255

C.1.2 FR2 Setup 1257

C.2 Connection 1259

C.2.1 FR1 Measurement of Performance Characteristics 1259

C.2.2 FR2 Measurement of Performance Characteristics 1259

Annex D (normative): E-UTRA link setup config for NSA testing 1260

D.0 General 1260

D.1 E-UTRA test parameters 1260

D.2 E-UTRA configuration 1262

D.3 E-UTRA link common physical channel setup 1263

D.4 E-UTRA power level 1263

D.4.1 E-UTRA power level (conducted) 1263

D.4.2 E-UTRA power level (radiated) 1263

Annex E (normative): Environmental conditions 1264

Annex F (normative): Measurement uncertainties and test tolerances 1264

F.1 Measurement uncertainties and test tolerances for FR1 1264

F.1.1 Acceptable uncertainty of test system (normative) 1264

F.1.1.1 Measurement of test environments 1264

F.1.1.2 Measurement of Demod Performance requirements 1264

F.1.1.3 Measurement of Channel State Information reporting 1279

F.1.2 Interpretation of measurement results (normative) 1283

F.1.3 Test Tolerance and Derivation of Test Requirements (informative) 1283

F.1.3.1 Measurement of test environments 1284

F.1.3.2 Measurement of Demod Performance requirements 1284

F.1.3.3 Measurement of Channel State Information reporting 1292

F.2 Measurement uncertainties and test tolerances for FR2 1297

F.2.1 Acceptable uncertainty of test system (normative) 1297

F.2.1.1 Measurement of test environments 1297

F.2.1.2 Measurement of Demod Performance requirements 1297

F.2.1.3 Measurement of Channel State Information reporting 1303

F.2.2 Interpretation of measurement results (normative) 1305

F.2.3 Test Tolerance and Derivation of Test Requirements (informative) 1306

F.2.3.1 Measurement of test environments 1306

F.2.3.2 Measurement of Demod Performance requirements 1306

F.2.3.3 Measurement of Channel State Information reporting 1308

Annex G (normative): Statistical Testing 1310

G.1 Statistical testing of Performance Requirements with throughput 1310

G.1.1 General 1310

G.1.2 Mapping throughput to error ratio 1310

G.1.3 Design of the test 1311

G.1.4 Pass Fail limit 1311

G.1.5 Minimum Test time 1312

G.1.5.0\_1 Minimum Test Time procedure for PDSCH scenarios with 30% or 70% Throughput requirement 1312

G.1.5.0\_2 Minimum Test Time procedure for PDSCH and PDCCH scenarios with 1% BLER requirement 1312

G.2 Theory to derive the numbers for statistical testing (informative) 1317

G.2.1 Error Ratio (ER) 1317

G.2.2 Test Design 1317

G.2.3 Confidence level 1318

G.2.4 Introduction: Supplier Risk versus Customer Risk 1318

G.2.5 Supplier Risk versus Customer Risk 1318

G.2.6 Introduction: Standard test versus early decision concept 1319

G.2.7 Standard test versus early decision concept 1319

G.2.8 Selectivity 1319

G.2.9 Design of the test 1320

G.2.10 Simulation to derive the pass fail limits 1321

G.3 Measuring throughput ratio 1322

G.3.1 General 1322

G.3.2 Establishing SNR 1322

G.3.3 Measuring T-put 1322

G.3.4 Number of samples for throughput ratios 1323

G.4 Statistical testing of Performance Requirements with BLER limit 1323

G.4.1 General 1323

G.4.2 Design of the test 1323

G.4.3 Numerical definition of the pass fail limits for 0.001% BLER 1323

G.4.3a Pass fail decision rules 1329

G.4.4 Simulation to derive the pass-fail limits for 0.001% BLER 1329

G.5 Statistical Testing of NR sidelink Performance Requirements – Non concurrent 1330

G.5.1 General 1330

G.5.2 Test method for PSCCH/PSSCH performance using sidelink HARQ feedback 1330

G.5.3 Test method for PSFCH performance 1332

G.5.4 Test time for PSSCH performance requirements with throughput 1334

G.5.5 Test time for PSCCH performance requirements with miss-detection probability 1335

G.5.6 Test time for PSFCH performance requirements with miss-detection probability 1335

Annex H: Approach for finding UE direction for FR2 Demod and CSI Testing 1337

H.0 Normative criteria for determining UE direction for Demod and CSI 1337

H.1 Procedure for finding UE direction 1337

H.1.1 Using Rx beam peak direction search 1337

H.1.2 RSRPB based scan with fallback option to Rx beam peak direction search 1337

H.1.3 Isolation based scan with fallback option to Rx beam peak direction search 1338

H.2 Wireless cable mode isolation procedure 1339

Annex I (informative): Change history 1340